(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "RFFC2071TR13" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 36.83 22.86 0))
    (property "Value" "RFFC2071TR13" (at 36.83 20.32 0))
    (property "Footprint" "DKMD2081" (at 36.83 -79.68 0))
    (property "Datasheet" "https://www.qorvo.com/products/d/da000696" (at 36.83 -179.68 0))
    (property "ki_description" "85 - 2700 MHz RF Synthesizer / VCO with Integrated RF Mixer" (at 36.83 -279.68 0))
    (property "Height" "0.9" (at 36.83 -379.68 0))
    (property "Mouser Part Number" "772-RFFC2071" (at 36.83 -479.68 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Qorvo/RFFC2071TR13?qs=tkvX2tz6JTEyTj7lyvTFWA%3D%3D" (at 36.83 -579.68 0))
    (property "Manufacturer_Name" "Qorvo" (at 36.83 -679.68 0))
    (property "Manufacturer_Part_Number" "RFFC2071TR13" (at 36.83 -779.68 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "ENBL/GPO5")
      (number "1")
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "EXT_LO")
      (number "2")
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "EXT_LO_DEC")
      (number "3")
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "REXT")
      (number "4")
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "ANA_VDD1")
      (number "5")
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "LFILT1")
      (number "6")
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "LFILT2")
      (number "7")
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "LFILT3")
      (number "8")
    )
    (pin passive line (at 10.16 -40.64 90) (length 5.08)
      (name "MODE/GPO6")
      (number "9")
    )
    (pin passive line (at 12.7 -40.64 90) (length 5.08)
      (name "REF_IN")
      (number "10")
    )
    (pin passive line (at 15.24 -40.64 90) (length 5.08)
      (name "NC_1")
      (number "11")
    )
    (pin passive line (at 17.78 -40.64 90) (length 5.08)
      (name "TM")
      (number "12")
    )
    (pin passive line (at 20.32 -40.64 90) (length 5.08)
      (name "MIX1_IPN")
      (number "13")
    )
    (pin passive line (at 22.86 -40.64 90) (length 5.08)
      (name "MIX1_IPP")
      (number "14")
    )
    (pin passive line (at 25.4 -40.64 90) (length 5.08)
      (name "GPO1/ADD1")
      (number "15")
    )
    (pin passive line (at 27.94 -40.64 90) (length 5.08)
      (name "GPO2/ADD2")
      (number "16")
    )
    (pin passive line (at 40.64 -17.78 180) (length 5.08)
      (name "MIX1_OPN")
      (number "17")
    )
    (pin passive line (at 40.64 -15.24 180) (length 5.08)
      (name "MIX1_OPP")
      (number "18")
    )
    (pin passive line (at 40.64 -12.7 180) (length 5.08)
      (name "DIG_VDD")
      (number "19")
    )
    (pin passive line (at 40.64 -10.16 180) (length 5.08)
      (name "NC_2")
      (number "20")
    )
    (pin passive line (at 40.64 -7.62 180) (length 5.08)
      (name "NC_3")
      (number "21")
    )
    (pin passive line (at 40.64 -5.08 180) (length 5.08)
      (name "ANA_VDD2")
      (number "22")
    )
    (pin passive line (at 40.64 -2.54 180) (length 5.08)
      (name "MIX2_IPP")
      (number "23")
    )
    (pin passive line (at 40.64 0 180) (length 5.08)
      (name "MIX2_IPN")
      (number "24")
    )
    (pin passive line (at 30.48 22.86 270) (length 5.08)
      (name "GPO3/FM")
      (number "25")
    )
    (pin passive line (at 27.94 22.86 270) (length 5.08)
      (name "GPO4/LD/DO")
      (number "26")
    )
    (pin passive line (at 25.4 22.86 270) (length 5.08)
      (name "MIX2_OPN")
      (number "27")
    )
    (pin passive line (at 22.86 22.86 270) (length 5.08)
      (name "MIX2_OPP")
      (number "28")
    )
    (pin passive line (at 20.32 22.86 270) (length 5.08)
      (name "RESETX")
      (number "29")
    )
    (pin passive line (at 17.78 22.86 270) (length 5.08)
      (name "ENX")
      (number "30")
    )
    (pin passive line (at 15.24 22.86 270) (length 5.08)
      (name "SCLK")
      (number "31")
    )
    (pin passive line (at 12.7 22.86 270) (length 5.08)
      (name "SDATA")
      (number "32")
    )
    (pin passive line (at 10.16 22.86 270) (length 5.08)
      (name "EP")
      (number "33")
    )
  )
)
