(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "HFCV-145+" (in_bom yes) (on_board yes)
    (property "Reference" "FL" (at 31.75 17.78 0))
    (property "Value" "HFCV-145+" (at 31.75 15.24 0))
    (property "Footprint" "HFCV145" (at 31.75 -84.76 0))
    (property "Datasheet" "https://www.minicircuits.com/WebStore/dashboardPdf?model=HFCV-145%2B" (at 31.75 -184.76 0))
    (property "ki_description" "Signal Conditioning HIGH PASS FLTR / SURF MT /RoHS" (at 31.75 -284.76 0))
    (property "Height" "1.6002" (at 31.75 -384.76 0))
    (property "Mouser Part Number" "139-HFCV-145" (at 31.75 -484.76 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/HFCV-145%2b?qs=xZ%2FP%252Ba9zWqbbbslkLTSMOA%3D%3D" (at 31.75 -584.76 0))
    (property "Manufacturer_Name" "Mini-Circuits" (at 31.75 -684.76 0))
    (property "Manufacturer_Part_Number" "HFCV-145+" (at 31.75 -784.76 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "INPUT")
      (number "1")
    )
    (pin passive line (at 17.78 -17.78 90) (length 5.08)
      (name "GND_1")
      (number "2")
    )
    (pin passive line (at 35.56 0 180) (length 5.08)
      (name "OUTPUT")
      (number "3")
    )
    (pin passive line (at 17.78 17.78 270) (length 5.08)
      (name "GND_2")
      (number "4")
    )
  )
)
