(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "HMC624ALP4ETR" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 31.75 12.7 0))
    (property "Value" "HMC624ALP4ETR" (at 31.75 10.16 0))
    (property "Footprint" "QFN50P400X400X90-25N-D" (at 31.75 -89.84 0))
    (property "Datasheet" "https://www.analog.com/HMC624A/datasheet" (at 31.75 -189.84 0))
    (property "ki_description" "0.1 GHz to 6.0 GHz, 0.5 dB LSB, 6-Bit, GaAs Digital Attenuator" (at 31.75 -289.84 0))
    (property "Height" "0.9" (at 31.75 -389.84 0))
    (property "Mouser Part Number" "584-HMC624ALP4ETR" (at 31.75 -489.84 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/HMC624ALP4ETR?qs=3izLlwrMQ7kIEdV2gXboXA%3D%3D" (at 31.75 -589.84 0))
    (property "Manufacturer_Name" "Analog Devices" (at 31.75 -689.84 0))
    (property "Manufacturer_Part_Number" "HMC624ALP4ETR" (at 31.75 -789.84 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "P/S")
      (number "1")
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "CLK")
      (number "2")
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "SERIN")
      (number "3")
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "LE")
      (number "4")
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "GND_1")
      (number "5")
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "ATTIN")
      (number "6")
    )
    (pin passive line (at 10.16 -27.94 90) (length 5.08)
      (name "ACG1")
      (number "7")
    )
    (pin passive line (at 12.7 -27.94 90) (length 5.08)
      (name "ACG2")
      (number "8")
    )
    (pin passive line (at 15.24 -27.94 90) (length 5.08)
      (name "ACG3")
      (number "9")
    )
    (pin passive line (at 17.78 -27.94 90) (length 5.08)
      (name "ACG4")
      (number "10")
    )
    (pin passive line (at 20.32 -27.94 90) (length 5.08)
      (name "ACG5")
      (number "11")
    )
    (pin passive line (at 22.86 -27.94 90) (length 5.08)
      (name "ACG6")
      (number "12")
    )
    (pin passive line (at 35.56 0 180) (length 5.08)
      (name "VDD")
      (number "18")
    )
    (pin passive line (at 35.56 -2.54 180) (length 5.08)
      (name "PUP1")
      (number "17")
    )
    (pin passive line (at 35.56 -5.08 180) (length 5.08)
      (name "PUP2")
      (number "16")
    )
    (pin passive line (at 35.56 -7.62 180) (length 5.08)
      (name "SEROUT")
      (number "15")
    )
    (pin passive line (at 35.56 -10.16 180) (length 5.08)
      (name "GND_2")
      (number "14")
    )
    (pin passive line (at 35.56 -12.7 180) (length 5.08)
      (name "ATTOUT")
      (number "13")
    )
    (pin passive line (at 10.16 12.7 270) (length 5.08)
      (name "EP")
      (number "25")
    )
    (pin passive line (at 12.7 12.7 270) (length 5.08)
      (name "D0")
      (number "24")
    )
    (pin passive line (at 15.24 12.7 270) (length 5.08)
      (name "D1")
      (number "23")
    )
    (pin passive line (at 17.78 12.7 270) (length 5.08)
      (name "D2")
      (number "22")
    )
    (pin passive line (at 20.32 12.7 270) (length 5.08)
      (name "D3")
      (number "21")
    )
    (pin passive line (at 22.86 12.7 270) (length 5.08)
      (name "D4")
      (number "20")
    )
    (pin passive line (at 25.4 12.7 270) (length 5.08)
      (name "D5")
      (number "19")
    )
  )
)
