(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "NCS4-232+" (in_bom yes) (on_board yes)
    (property "Reference" "T" (at 80.01 7.62 0))
    (property "Value" "NCS4-232+" (at 80.01 5.08 0))
    (property "Footprint" "NCS4232" (at 80.01 -94.92 0))
    (property "Datasheet" "" (at 80.01 -194.92 0))
    (property "ki_description" "Ceramic Balun RF Transformer.  50 1600 to 2300 MHz 1:4 Ratio." (at 80.01 -294.92 0))
    (property "Height" "0.84" (at 80.01 -394.92 0))
    (property "Mouser Part Number" "139-NCS4-232" (at 80.01 -494.92 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/NCS4-232%2b?qs=xZ%2FP%252Ba9zWqYBp16Imqylgw%3D%3D" (at 80.01 -594.92 0))
    (property "Manufacturer_Name" "Mini-Circuits" (at 80.01 -694.92 0))
    (property "Manufacturer_Part_Number" "NCS4-232+" (at 80.01 -794.92 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "PRIMARY_DOT(UNBALANCED_PORT)")
      (number "1")
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "PRIMARY(GND)")
      (number "2")
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "SECONDARY(BALANCED)")
      (number "3")
    )
    (pin passive line (at 83.82 -5.08 180) (length 5.08)
      (name "SECONDARY_DOT(BALANCED)")
      (number "4")
    )
    (pin passive line (at 83.82 -2.54 180) (length 5.08)
      (name "NOT_USED(GND_EXTERNALLY)")
      (number "5")
    )
    (pin no_connect line (at 83.82 0 180) (length 5.08)
      (name "NC")
      (number "6")
    )
  )
)
