(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "TCM1-382WX+" (in_bom yes) (on_board yes)
    (property "Reference" "T" (at 44.45 7.62 0))
    (property "Value" "TCM1-382WX+" (at 44.45 5.08 0))
    (property "Footprint" "TCM1382WX" (at 44.45 -94.92 0))
    (property "Datasheet" "https://www.mouser.kr/datasheet/2/1030/TCM1_382WX_2b-3105014.pdf" (at 44.45 -194.92 0))
    (property "ki_description" "Audio Transformers / Signal Transformers 1:1 CORE & WIRE Transformer, 0.5 - 3800 MHz, 50?" (at 44.45 -294.92 0))
    (property "Height" "4.06" (at 44.45 -394.92 0))
    (property "Mouser Part Number" "139-TCM1-382WX" (at 44.45 -494.92 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/TCM1-382WX%2b?qs=amGC7iS6iy9TpOSpP5xMJQ%3D%3D" (at 44.45 -594.92 0))
    (property "Manufacturer_Name" "Mini-Circuits" (at 44.45 -694.92 0))
    (property "Manufacturer_Part_Number" "TCM1-382WX+" (at 44.45 -794.92 0))
    (pin passive line (at 48.26 0 180) (length 5.08)
      (name "GND_1")
      (number "1")
    )
    (pin passive line (at 48.26 -2.54 180) (length 5.08)
      (name "GND_2")
      (number "2")
    )
    (pin passive line (at 48.26 -5.08 180) (length 5.08)
      (name "PRIMARY_DOT")
      (number "3")
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "SECONDARY")
      (number "4")
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "SECONDARY_DOT")
      (number "5")
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "NOT_USED")
      (number "6")
    )
  )
)
