(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(LED1-K_1)")
	(net 2 "Net-(LED1-A_1)")
	(net 3 "Net-(LED2-K_1)")
	(net 4 "GND")
	(net 5 "Net-(LED4-K_1)")
	(net 6 "Net-(LED4-A_1)")
	(net 7 "Net-(LED5-K_1)")
	(net 8 "Net-(LED7-A_1)")
	(net 9 "Net-(LED7-K_1)")
	(net 10 "Net-(LED8-K_1)")
	(net 11 "Net-(LED10-A_1)")
	(net 12 "Net-(LED10-K_1)")
	(net 13 "Net-(LED11-K_1)")
	(net 14 "Net-(LED13-K_1)")
	(net 15 "Net-(LED13-A_1)")
	(net 16 "Net-(LED14-K_1)")
	(net 17 "Net-(LED16-K_1)")
	(net 18 "Net-(LED16-A_1)")
	(net 19 "Net-(LED17-K_1)")
	(net 20 "Net-(LED19-A_1)")
	(net 21 "Net-(LED19-K_1)")
	(net 22 "Net-(LED20-K_1)")
	(net 23 "Net-(LED22-A_1)")
	(net 24 "Net-(LED22-K_1)")
	(net 25 "Net-(LED23-K_1)")
	(net 26 "Net-(LED25-K_1)")
	(net 27 "Net-(LED25-A_1)")
	(net 28 "Net-(LED26-K_1)")
	(net 29 "Net-(LED28-K_1)")
	(net 30 "Net-(LED28-A_1)")
	(net 31 "Net-(LED29-K_1)")
	(net 32 "VCC")
	(net 33 "Net-(LED31-A_1)")
	(net 34 "Net-(LED31-K_1)")
	(net 35 "Net-(LED32-K_1)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 161.035 123.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 15 "Net-(LED13-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 156.17 100)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED7"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(LED7-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(LED7-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(LED7-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(LED7-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 144.17 75)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED3"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(LED2-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(LED2-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 166.17 106)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED28"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(LED28-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(LED28-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(LED28-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(LED28-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 126.5 100)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED20"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(LED20-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(LED19-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(LED20-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(LED19-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 144.185 95)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED6"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(LED5-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(LED5-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 172.705 95)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED16"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(LED16-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(LED16-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(LED16-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(LED16-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 161 75 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(LED1-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 126.5 105)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED21"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(LED20-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(LED20-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 162.17 89.5)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED26"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(LED26-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(LED25-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(LED26-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(LED25-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 139.17 89)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED23"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(LED23-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(LED22-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(LED23-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(LED22-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 150.17 105)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED11"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(LED11-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(LED10-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(LED11-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(LED10-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 162.17 111)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED29"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(LED29-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(LED28-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(LED29-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(LED28-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 143.185 116)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(LED32-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(LED32-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 156.185 105)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED10"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(LED10-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(LED10-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(LED10-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(LED10-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 143.5 84)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED22"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(LED22-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(LED22-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(LED22-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(LED22-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 147 110.5 -90)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.77 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 5.31 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 166.5 98.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(LED25-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 156.185 75)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED1"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(LED1-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(LED1-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(LED1-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(LED1-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 126.515 95)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED19"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(LED19-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(LED19-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(LED19-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(LED19-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 150.205 123.5)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED14"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(LED14-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(LED13-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(LED14-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(LED13-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 139.17 111)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED32"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(LED32-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(LED31-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(LED32-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(LED31-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 150.17 95)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED5"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(LED5-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(LED4-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(LED5-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(LED4-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 172.705 100)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED17"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(LED17-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(LED16-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(LED17-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(LED16-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 156.205 123.5)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED13"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(LED13-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(LED13-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(LED13-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(LED13-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 144.185 105)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED12"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(LED11-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(LED11-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 144.205 123.5)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED15"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(LED14-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(LED14-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 150.17 100)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED8"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(LED8-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(LED7-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(LED8-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(LED7-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.9625 112.99)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 157.67 84.5)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED27"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(LED26-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(LED26-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 156.2 95)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED4"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(LED4-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(LED4-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(LED4-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(LED4-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 150.205 75)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED2"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(LED2-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(LED1-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(LED2-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(LED1-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 135.5 102)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(LED31-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 148.5 84 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(LED22-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 144.17 100)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED9"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(LED8-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(LED8-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 161 100 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(LED7-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 172.535 91)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(LED16-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 129 91.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(LED19-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 166.5 102)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(LED28-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 158.17 116)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED30"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(LED29-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(LED29-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 161 95 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(LED4-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 135.17 94)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED24"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(LED23-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(LED23-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.9625 116)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 172.705 105)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED18"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(LED17-K_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(LED17-K_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 135.17 106)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED31"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(LED31-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(LED31-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(LED31-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(LED31-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 161 105 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "390"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 11 "Net-(LED10-A_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B_HandSolder"
		(layer "F.Cu")
		(at 151.8725 109.5)
		(descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC-7352 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C3"
			(at 0 -2.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22u"
			(at 0 2.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6275 0)
			(size 1.515 2.39)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.165017)
			(net 32 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.6275 0)
			(size 1.515 2.39)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.165017)
			(net 4 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:GWJTLMS3CMG6G9XX5101"
		(layer "F.Cu")
		(at 166.17 94.5)
		(descr "GW JTLMS3.CM-G6G9-XX510-1")
		(tags "LED")
		(property "Reference" "LED25"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GW_JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at -0.005 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mid-Power LEDs - White"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "GW JTLMS3.CM-G8GW-XX53-1-60-R33"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "monster-lithophane-light-v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.705 0 90)
			(size 2.1 2.12)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(LED25-K_1)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.315 0)
			(size 0.92 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(LED25-A_1)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.83 0)
			(size 0.13 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(LED25-K_1)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.83 0)
			(size 0.11 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(LED25-A_1)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "GW_JTLMS3.CM-G8GW-XX53-1-60-R33.stp"
			(offset
				(xyz 0 0 0.07999999701)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(gr_circle
		(center 132.5 82.5)
		(end 134.5 82.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 132.5 117.5)
		(end 134.5 117.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 150 100)
		(end 182.5 100)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 167.5 82.5)
		(end 169.5 82.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 167.5 117.5)
		(end 169.5 117.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Litho Monster light"
		(at 143.5 128 0)
		(layer "F.SilkS")
	)
	(gr_text "Design by Maresz"
		(at 144 129.5 0)
		(layer "F.SilkS")
	)
	(gr_text "V1.0"
		(at 148.5 131 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 142 112 0)
		(layer "B.SilkS")
	)
	(gr_text "VCC 8-13V"
		(at 166.5 112 0)
		(layer "B.SilkS")
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 118 100)
					(mid 182 100)
					(end 118 100)
				)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 118 100)
					(mid 182 100)
					(end 118 100)
				)
			)
		)
	)
	(embedded_fonts no)
)
