(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1_rf1-In)")
	(net 2 "Net-(J2_rfdc1-In)")
	(net 3 "GND")
	(net 4 "Net-(L1-Pad1)")
	(net 5 "Net-(J1-Pin_2)")
	(net 6 "Net-(D1-A)")
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 174.21 102.8 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 1.0125 1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "L"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-Pin_2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(L1-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 173.43 105.2 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at -0.8125 1.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "L"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(clearance 0.15)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(L1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J2_rfdc1-In)")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
		(layer "F.Cu")
		(at 194.65 106 -90)
		(descr " Amphenol RF 901-143 https://www.amphenolrf.com/library/download/link/link_id/585682")
		(tags "SMA THT Female Jack Horizontal")
		(property "Reference" "J1_rf1"
			(at -5.2 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 4.3 -4.5)
			(end -4.3 -4.5)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.3 2.3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "Net-(J1_rf1-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 1)
				(max_length 3)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole roundrect
			(at -2.54 -2.54 270)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -2.54 2.54 270)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 -2.54 270)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 2.54 270)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-143_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 179.95 102.8 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -0.0875 -1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
		(layer "F.Cu")
		(at 164.65 106 90)
		(descr " Amphenol RF 901-143 https://www.amphenolrf.com/library/download/link/link_id/585682")
		(tags "SMA THT Female Jack Horizontal")
		(property "Reference" "J2_rfdc1"
			(at -5.2 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 5 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 4.3 -4.5)
			(end -4.3 -4.5)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2.3 2.3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "Net-(J2_rfdc1-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 1)
				(max_length 3)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole roundrect
			(at -2.54 -2.54 90)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -2.54 2.54 90)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 -2.54 90)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 2.54 90)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.1)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-143_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 176.42 99 90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 6.285 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 186.125 102.75 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "LED"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 177.725 106 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "biastee1.kicad_sch")
		(clearance 0.15)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1_rf1-In)")
			(pintype "passive")
			(clearance 0.2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J2_rfdc1-In)")
			(pintype "passive")
			(clearance 0.2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 160 97.5)
		(end 160.15 101.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.15 101.7)
		(end 199 97.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.15 110.3)
		(end 160.5 110.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.5 110.5)
		(end 199 110.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199 110.5)
		(end 199.15 110.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199 97.5)
		(end 160 97.5)
		(layer "Edge.Cuts")
	)
	(gr_text "RF"
		(at 196.05 100.95 0)
		(layer "B.SilkS")
	)
	(gr_text "RF+DC\n"
		(at 169 100.75 0)
		(layer "B.SilkS")
	)
	(gr_text "Bias-Tee by Maresz"
		(at 189.4 103.45 0)
		(layer "B.SilkS")
	)
	(gr_text "RF+DC\n"
		(at 161.05 101.05 0)
		(layer "F.SilkS")
	)
	(gr_text "RF"
		(at 192.95 101.3 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "Net-(J1_rf1-In)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.2 105.5) (xy 191.2 106.5) (xy 194.086185 107) (xy 194.651 106) (xy 194.086185 105)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(J2_rfdc1-In)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.1 106.5) (xy 168.1 105.5) (xy 165.213815 105) (xy 164.649 106) (xy 165.213815 107)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.15 107.7) (xy 193.75 107.2) (xy 191.15 106.65) (xy 190.1 106.65) (xy 168.15 106.65) (xy 164.65 107.45)
				(xy 163.1 107.45) (xy 163.1 104.5) (xy 164.95 104.5) (xy 165.6 104.75) (xy 168.15 105.3) (xy 169.2 105.3)
				(xy 169 101.6) (xy 161 101.6) (xy 161 110) (xy 168.7 110.05) (xy 198.7 110.05) (xy 198.65 101.95)
				(xy 196.15 101.9) (xy 196.2 104.7) (xy 196.2 105) (xy 196.2 103.7)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198 98) (xy 198 101.6) (xy 190.4 101.6) (xy 190.15 105.35) (xy 169 105.4) (xy 169 101.6) (xy 161 101.6)
				(xy 161 98)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198 101.6) (xy 198 104.6) (xy 198 104.4) (xy 194.15 104.65) (xy 191.2 105.3) (xy 190.15 105.35)
				(xy 190.2 101.4)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1.5)
		)
		(polygon
			(pts
				(xy 198 98) (xy 161 98) (xy 161 110) (xy 198.2 110.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1.5)
		)
		(polygon
			(pts
				(xy 194.6 104.6) (xy 165.95 104.55) (xy 165.95 107.4) (xy 194.8 107.4)
			)
		)
	)
)
