(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:Crystal_GND24"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Y"
				(at 3.175 5.08 0)
			)
			(property "Value" "Crystal_GND24"
				(at 3.175 3.175 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Four pin crystal, GND on pins 2 and 4"
				(at 0 0 0)
			)
			(property private "KLC_S3.3" "The rectangle is not a symbol body but a graphical element"
				(at 0 -12.7 0)
				(show_name)
			)
			(property private "KLC_S4.1" "Some pins are on 50mil grid to make the symbol small"
				(at 0 -15.24 0)
				(show_name)
			)
			(property "ki_keywords" "quartz ceramic resonator oscillator"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Crystal*"
				(at 0 0 0)
			)
			(symbol "Crystal_GND24_0_1"
				(polyline
					(pts
						(xy -2.54 2.286) (xy -2.54 3.556) (xy 2.54 3.556) (xy 2.54 2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 0) (xy -2.032 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -2.286) (xy -2.54 -3.556) (xy 2.54 -3.556) (xy 2.54 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -1.27) (xy -2.032 1.27)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.143 2.54)
					(end 1.143 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.81) (xy 0 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.032 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.032 -1.27) (xy 2.032 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Crystal_GND24_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 1.27)
					(name "G")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 1.27)
					(hide yes)
					(name "G")
					(number "4")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:LED"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MCU_ST_STM32C0:STM32C071CBTx"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 46.99 0)
			)
			(property "Value" "STM32C071CBTx"
				(at 2.54 46.99 0)
			)
			(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
				(at -10.16 -45.72 0)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071cb.pdf"
				(at 0 0 0)
			)
			(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 45 GPIO, LQFP48_GP"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
				(at 0 0 0)
			)
			(symbol "STM32C071CBTx_0_1"
				(rectangle
					(start -10.16 -45.72)
					(end 10.16 45.72)
					(fill
						(type background)
					)
				)
			)
			(symbol "STM32C071CBTx_1_1"
				(pin input line
					(at -12.7 40.64 0)
					(length 2.54)
					(name "VREF+")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 35.56 0)
					(length 2.54)
					(name "PF0")
					(number "8")
					(alternate "CRS_SYNC" bidirectional line)
					(alternate "RCC_OSC_IN" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 33.02 0)
					(length 2.54)
					(name "PF1")
					(number "9")
					(alternate "RCC_OSC_EN" bidirectional line)
					(alternate "RCC_OSC_OUT" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 30.48 0)
					(length 2.54)
					(name "PF2")
					(number "10")
					(alternate "RCC_MCO" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 27.94 0)
					(length 2.54)
					(name "PF3")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 22.86 0)
					(length 2.54)
					(name "PD0")
					(number "38")
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 20.32 0)
					(length 2.54)
					(name "PD1")
					(number "39")
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 17.78 0)
					(length 2.54)
					(name "PD2")
					(number "40")
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 15.24 0)
					(length 2.54)
					(name "PD3")
					(number "41")
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "PC6")
					(number "30")
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "PC7")
					(number "31")
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "PC13")
					(number "1")
					(alternate "PWR_WKUP2" bidirectional line)
					(alternate "RTC_OUT1" bidirectional line)
					(alternate "RTC_TS" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "PC14")
					(number "2")
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "RCC_OSCX_IN" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_BKIN2" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "PC15")
					(number "3")
					(alternate "RCC_OSC32_EN" bidirectional line)
					(alternate "RCC_OSCX_OUT" bidirectional line)
					(alternate "RCC_OSC_EN" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin power_in line
					(at 0 48.26 270)
					(length 2.54)
					(name "VDD")
					(number "6")
				)
				(pin power_in line
					(at 0 -48.26 90)
					(length 2.54)
					(name "VSS")
					(number "7")
				)
				(pin bidirectional line
					(at 12.7 40.64 180)
					(length 2.54)
					(name "PA0")
					(number "11")
					(alternate "ADC1_IN0" bidirectional line)
					(alternate "PWR_WKUP1" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 38.1 180)
					(length 2.54)
					(name "PA1")
					(number "12")
					(alternate "ADC1_IN1" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 35.56 180)
					(length 2.54)
					(name "PA2")
					(number "13")
					(alternate "ADC1_IN2" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "PWR_WKUP4" bidirectional line)
					(alternate "RCC_LSCO" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM16_CH1N" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 33.02 180)
					(length 2.54)
					(name "PA3")
					(number "14")
					(alternate "ADC1_IN3" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 30.48 180)
					(length 2.54)
					(name "PA4")
					(number "15")
					(alternate "ADC1_IN4" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RTC_OUT2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 27.94 180)
					(length 2.54)
					(name "PA5")
					(number "16")
					(alternate "ADC1_IN5" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 25.4 180)
					(length 2.54)
					(name "PA6")
					(number "17")
					(alternate "ADC1_IN6" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 22.86 180)
					(length 2.54)
					(name "PA7")
					(number "18")
					(alternate "ADC1_IN7" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 20.32 180)
					(length 2.54)
					(name "PA8")
					(number "28")
					(alternate "ADC1_IN8" bidirectional line)
					(alternate "CRS_SYNC" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RCC_MCO" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 17.78 180)
					(length 2.54)
					(name "PA9")
					(number "29")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "RCC_MCO" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "PA10")
					(number "32")
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 12.7 180)
					(length 2.54)
					(name "PA11")
					(number "33")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM1_BKIN2" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
					(alternate "USB_DM" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 10.16 180)
					(length 2.54)
					(name "PA12")
					(number "34")
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "I2S_CKIN" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USB_DP" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 7.62 180)
					(length 2.54)
					(name "PA13")
					(number "35")
					(alternate "ADC1_IN13" bidirectional line)
					(alternate "DEBUG_SWDIO" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "PA14")
					(number "36")
					(alternate "ADC1_IN14" bidirectional line)
					(alternate "DEBUG_SWCLK" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "PA15")
					(number "37")
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "PB0")
					(number "19")
					(alternate "ADC1_IN17" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "PB1")
					(number "20")
					(alternate "ADC1_IN18" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "PB2")
					(number "21")
					(alternate "ADC1_IN19" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "PB3")
					(number "42")
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "PB4")
					(number "43")
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "PB5")
					(number "44")
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "PWR_WKUP6" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM16_BKIN" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "PB6")
					(number "45")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "PWR_WKUP3" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM16_BKIN" bidirectional line)
					(alternate "TIM16_CH1N" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "PB7")
					(number "46")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -22.86 180)
					(length 2.54)
					(name "PB8")
					(number "47")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -25.4 180)
					(length 2.54)
					(name "PB9")
					(number "48")
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -27.94 180)
					(length 2.54)
					(name "PB10")
					(number "22")
					(alternate "ADC1_IN20" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -30.48 180)
					(length 2.54)
					(name "PB11")
					(number "23")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC1_IN21" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -33.02 180)
					(length 2.54)
					(name "PB12")
					(number "24")
					(alternate "ADC1_IN22" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM1_BKIN2" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -35.56 180)
					(length 2.54)
					(name "PB13")
					(number "25")
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -38.1 180)
					(length 2.54)
					(name "PB14")
					(number "26")
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -40.64 180)
					(length 2.54)
					(name "PB15")
					(number "27")
					(alternate "RTC_REFIN" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 63.5 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 36.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 53.34 63.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 36.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 57.15 44.45) (xy 63.5 44.45)
		)
	)
	(wire
		(pts
			(xy 107.95 116.84) (xy 107.95 120.65)
		)
	)
	(wire
		(pts
			(xy 53.34 63.5) (xy 53.34 96.52)
		)
	)
	(wire
		(pts
			(xy 186.69 116.84) (xy 186.69 127)
		)
	)
	(wire
		(pts
			(xy 46.99 66.04) (xy 35.56 66.04)
		)
	)
	(wire
		(pts
			(xy 80.01 36.83) (xy 80.01 53.34)
		)
	)
	(wire
		(pts
			(xy 67.31 71.12) (xy 45.72 71.12)
		)
	)
	(wire
		(pts
			(xy 92.71 81.28) (xy 96.52 81.28)
		)
	)
	(wire
		(pts
			(xy 161.29 147.32) (xy 161.29 146.05)
		)
	)
	(wire
		(pts
			(xy 173.99 134.62) (xy 173.99 138.43)
		)
	)
	(wire
		(pts
			(xy 92.71 99.06) (xy 115.57 99.06)
		)
	)
	(wire
		(pts
			(xy 186.69 147.32) (xy 186.69 146.05)
		)
	)
	(wire
		(pts
			(xy 92.71 114.3) (xy 110.49 114.3)
		)
	)
	(wire
		(pts
			(xy 110.49 116.84) (xy 186.69 116.84)
		)
	)
	(wire
		(pts
			(xy 92.71 71.12) (xy 96.52 71.12)
		)
	)
	(wire
		(pts
			(xy 41.91 76.2) (xy 41.91 78.74)
		)
	)
	(wire
		(pts
			(xy 161.29 134.62) (xy 161.29 138.43)
		)
	)
	(wire
		(pts
			(xy 92.71 119.38) (xy 105.41 119.38)
		)
	)
	(wire
		(pts
			(xy 53.34 63.5) (xy 53.34 53.34)
		)
	)
	(wire
		(pts
			(xy 35.56 66.04) (xy 35.56 71.12)
		)
	)
	(wire
		(pts
			(xy 92.71 91.44) (xy 96.52 91.44)
		)
	)
	(wire
		(pts
			(xy 80.01 152.4) (xy 80.01 154.94)
		)
	)
	(wire
		(pts
			(xy 173.99 120.65) (xy 173.99 127)
		)
	)
	(wire
		(pts
			(xy 58.42 87.63) (xy 63.5 87.63)
		)
	)
	(wire
		(pts
			(xy 161.29 147.32) (xy 173.99 147.32)
		)
	)
	(wire
		(pts
			(xy 53.34 53.34) (xy 80.01 53.34)
		)
	)
	(wire
		(pts
			(xy 71.12 36.83) (xy 80.01 36.83)
		)
	)
	(wire
		(pts
			(xy 63.5 93.98) (xy 67.31 93.98)
		)
	)
	(wire
		(pts
			(xy 173.99 147.32) (xy 173.99 146.05)
		)
	)
	(wire
		(pts
			(xy 92.71 78.74) (xy 96.52 78.74)
		)
	)
	(wire
		(pts
			(xy 57.15 36.83) (xy 71.12 36.83)
		)
	)
	(wire
		(pts
			(xy 105.41 123.19) (xy 161.29 123.19)
		)
	)
	(wire
		(pts
			(xy 63.5 44.45) (xy 63.5 46.99)
		)
	)
	(wire
		(pts
			(xy 107.95 120.65) (xy 173.99 120.65)
		)
	)
	(wire
		(pts
			(xy 50.8 36.83) (xy 57.15 36.83)
		)
	)
	(wire
		(pts
			(xy 57.15 63.5) (xy 53.34 63.5)
		)
	)
	(wire
		(pts
			(xy 53.34 96.52) (xy 67.31 96.52)
		)
	)
	(wire
		(pts
			(xy 35.56 71.12) (xy 38.1 71.12)
		)
	)
	(wire
		(pts
			(xy 92.71 93.98) (xy 96.52 93.98)
		)
	)
	(wire
		(pts
			(xy 92.71 73.66) (xy 96.52 73.66)
		)
	)
	(wire
		(pts
			(xy 115.57 99.06) (xy 127 99.06)
		)
	)
	(wire
		(pts
			(xy 173.99 147.32) (xy 186.69 147.32)
		)
	)
	(wire
		(pts
			(xy 46.99 68.58) (xy 46.99 66.04)
		)
	)
	(wire
		(pts
			(xy 63.5 87.63) (xy 63.5 93.98)
		)
	)
	(wire
		(pts
			(xy 92.71 76.2) (xy 96.52 76.2)
		)
	)
	(wire
		(pts
			(xy 92.71 68.58) (xy 96.52 68.58)
		)
	)
	(wire
		(pts
			(xy 186.69 134.62) (xy 186.69 138.43)
		)
	)
	(wire
		(pts
			(xy 92.71 66.04) (xy 96.52 66.04)
		)
	)
	(wire
		(pts
			(xy 92.71 96.52) (xy 96.52 96.52)
		)
	)
	(wire
		(pts
			(xy 105.41 119.38) (xy 105.41 123.19)
		)
	)
	(wire
		(pts
			(xy 92.71 116.84) (xy 107.95 116.84)
		)
	)
	(wire
		(pts
			(xy 64.77 63.5) (xy 67.31 63.5)
		)
	)
	(wire
		(pts
			(xy 161.29 123.19) (xy 161.29 127)
		)
	)
	(wire
		(pts
			(xy 67.31 68.58) (xy 46.99 68.58)
		)
	)
	(wire
		(pts
			(xy 92.71 106.68) (xy 96.52 106.68)
		)
	)
	(wire
		(pts
			(xy 173.99 147.32) (xy 173.99 149.86)
		)
	)
	(wire
		(pts
			(xy 80.01 53.34) (xy 80.01 55.88)
		)
	)
	(wire
		(pts
			(xy 63.5 44.45) (xy 71.12 44.45)
		)
	)
	(wire
		(pts
			(xy 115.57 106.68) (xy 115.57 109.22)
		)
	)
	(wire
		(pts
			(xy 110.49 114.3) (xy 110.49 116.84)
		)
	)
	(hierarchical_label "USB_DM"
		(shape input)
		(at 96.52 91.44 0)
	)
	(hierarchical_label "TRCTL"
		(shape input)
		(at 96.52 106.68 0)
	)
	(hierarchical_label "UART_RX"
		(shape input)
		(at 96.52 71.12 0)
	)
	(hierarchical_label "sw_ctrl"
		(shape input)
		(at 96.52 76.2 0)
	)
	(hierarchical_label "SYNT_MUX"
		(shape input)
		(at 96.52 78.74 0)
	)
	(hierarchical_label "SWCLK"
		(shape input)
		(at 127 99.06 0)
	)
	(hierarchical_label "SWDIO"
		(shape input)
		(at 96.52 96.52 0)
	)
	(hierarchical_label "DATA"
		(shape input)
		(at 96.52 81.28 0)
	)
	(hierarchical_label "USB_DP"
		(shape input)
		(at 96.52 93.98 0)
	)
	(hierarchical_label "LE"
		(shape input)
		(at 96.52 73.66 0)
	)
	(hierarchical_label "3V3"
		(shape input)
		(at 50.8 36.83 180)
	)
	(hierarchical_label "CLK"
		(shape input)
		(at 96.52 66.04 0)
	)
	(hierarchical_label "UART_TX"
		(shape input)
		(at 96.52 68.58 0)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 154.94 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR027"
			(at 80.01 161.29 0)
		)
		(property "Value" "GND"
			(at 80.01 159.258 0)
		)
		(property "Footprint" ""
			(at 80.01 154.94 0)
		)
		(property "Datasheet" ""
			(at 80.01 154.94 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 80.01 154.94 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 57.15 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C18"
			(at 60.96 39.3699 0)
		)
		(property "Value" "10n"
			(at 60.96 41.9099 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 58.1152 44.45 0)
		)
		(property "Datasheet" "~"
			(at 57.15 40.64 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 57.15 40.64 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 41.91 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR074"
			(at 41.91 85.09 0)
		)
		(property "Value" "GND"
			(at 41.91 83.058 0)
		)
		(property "Footprint" ""
			(at 41.91 78.74 0)
		)
		(property "Datasheet" ""
			(at 41.91 78.74 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 41.91 78.74 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR074")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 161.29 142.24 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 165.1 142.5574 90)
		)
		(property "Value" "LED"
			(at 165.1 145.0974 90)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 161.29 142.24 0)
		)
		(property "Datasheet" "~"
			(at 161.29 142.24 0)
		)
		(property "Description" "Light emitting diode"
			(at 161.29 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 161.29 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 173.99 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR07"
			(at 173.99 156.21 0)
		)
		(property "Value" "GND"
			(at 173.99 154.178 0)
		)
		(property "Footprint" ""
			(at 173.99 149.86 0)
		)
		(property "Datasheet" ""
			(at 173.99 149.86 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 173.99 149.86 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 186.69 142.24 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D3"
			(at 190.5 142.5574 90)
		)
		(property "Value" "LED"
			(at 190.5 145.0974 90)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 186.69 142.24 0)
		)
		(property "Datasheet" "~"
			(at 186.69 142.24 0)
		)
		(property "Description" "Light emitting diode"
			(at 186.69 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 186.69 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 115.57 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C58"
			(at 119.38 101.5999 0)
		)
		(property "Value" "C"
			(at 119.38 104.1399 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 116.5352 106.68 0)
		)
		(property "Datasheet" "~"
			(at 115.57 102.87 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 115.57 102.87 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C58")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 60.96 63.5 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R51"
			(at 60.96 57.15 90)
		)
		(property "Value" "R"
			(at 60.96 59.69 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 60.96 65.278 90)
		)
		(property "Datasheet" "~"
			(at 60.96 63.5 0)
		)
		(property "Description" "Resistor"
			(at 60.96 63.5 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R51")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 115.57 109.22 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR072"
			(at 115.57 115.57 0)
		)
		(property "Value" "GND"
			(at 115.57 113.538 0)
		)
		(property "Footprint" ""
			(at 115.57 109.22 0)
		)
		(property "Datasheet" ""
			(at 115.57 109.22 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 115.57 109.22 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR072")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 173.99 142.24 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 177.8 142.5574 90)
		)
		(property "Value" "LED"
			(at 177.8 145.0974 90)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 173.99 142.24 0)
		)
		(property "Datasheet" "~"
			(at 173.99 142.24 0)
		)
		(property "Description" "Light emitting diode"
			(at 173.99 142.24 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 173.99 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_ST_STM32C0:STM32C071CBTx")
		(at 80.01 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 82.1533 53.34 0)
		)
		(property "Value" "STM32C071CBTx"
			(at 82.1533 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 69.85 149.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071cb.pdf"
			(at 80.01 104.14 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 45 GPIO, LQFP48_GP"
			(at 80.01 104.14 0)
		)
		(pin "15")
		(pin "1")
		(pin "3")
		(pin "47")
		(pin "20")
		(pin "30")
		(pin "19")
		(pin "22")
		(pin "36")
		(pin "9")
		(pin "28")
		(pin "23")
		(pin "24")
		(pin "43")
		(pin "32")
		(pin "39")
		(pin "16")
		(pin "7")
		(pin "17")
		(pin "10")
		(pin "48")
		(pin "14")
		(pin "12")
		(pin "46")
		(pin "37")
		(pin "27")
		(pin "18")
		(pin "45")
		(pin "38")
		(pin "25")
		(pin "34")
		(pin "8")
		(pin "13")
		(pin "6")
		(pin "21")
		(pin "29")
		(pin "5")
		(pin "31")
		(pin "35")
		(pin "41")
		(pin "11")
		(pin "2")
		(pin "33")
		(pin "44")
		(pin "26")
		(pin "42")
		(pin "4")
		(pin "40")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Crystal_GND24")
		(at 41.91 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Y1"
			(at 41.91 62.23 0)
		)
		(property "Value" "Crystal_GND24"
			(at 41.91 64.77 0)
		)
		(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm_HandSoldering"
			(at 41.91 71.12 0)
		)
		(property "Datasheet" "~"
			(at 41.91 71.12 0)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 41.91 71.12 0)
		)
		(property private "KLC_S3.3" "The rectangle is not a symbol body but a graphical element"
			(at 41.91 83.82 0)
			(show_name yes)
		)
		(property private "KLC_S4.1" "Some pins are on 50mil grid to make the symbol small"
			(at 41.91 86.36 0)
			(show_name yes)
		)
		(pin "3")
		(pin "2")
		(pin "4")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "Y1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 63.5 46.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR026"
			(at 63.5 53.34 0)
		)
		(property "Value" "GND"
			(at 63.5 51.308 0)
		)
		(property "Footprint" ""
			(at 63.5 46.99 0)
		)
		(property "Datasheet" ""
			(at 63.5 46.99 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 63.5 46.99 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 161.29 130.81 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R57"
			(at 163.83 129.5399 0)
		)
		(property "Value" "1k"
			(at 163.83 132.0799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 163.068 130.81 90)
		)
		(property "Datasheet" "~"
			(at 161.29 130.81 0)
		)
		(property "Description" "Resistor"
			(at 161.29 130.81 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R57")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 173.99 130.81 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R58"
			(at 176.53 129.5399 0)
		)
		(property "Value" "1k"
			(at 176.53 132.0799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 175.768 130.81 90)
		)
		(property "Datasheet" "~"
			(at 173.99 130.81 0)
		)
		(property "Description" "Resistor"
			(at 173.99 130.81 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R58")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 58.42 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR071"
			(at 58.42 93.98 0)
		)
		(property "Value" "GND"
			(at 58.42 91.948 0)
		)
		(property "Footprint" ""
			(at 58.42 87.63 0)
		)
		(property "Datasheet" ""
			(at 58.42 87.63 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 58.42 87.63 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR071")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 71.12 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C17"
			(at 74.93 39.3699 0)
		)
		(property "Value" "100p"
			(at 74.93 41.9099 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 72.0852 44.45 0)
		)
		(property "Datasheet" "~"
			(at 71.12 40.64 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 71.12 40.64 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 186.69 130.81 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R59"
			(at 189.23 129.5399 0)
		)
		(property "Value" "1k"
			(at 189.23 132.0799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 188.468 130.81 90)
		)
		(property "Datasheet" "~"
			(at 186.69 130.81 0)
		)
		(property "Description" "Resistor"
			(at 186.69 130.81 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R59")
					(unit 1)
				)
			)
		)
	)
)
