(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(IC1-ANA_VDD1-Pad5)")
	(net 2 "unconnected-(IC1-ENBL{slash}GPO5-Pad1)")
	(net 3 "unconnected-(IC1-MODE{slash}GPO6-Pad9)")
	(net 4 "unconnected-(IC1-REXT-Pad4)")
	(net 5 "unconnected-(IC1-MIX2_OPN-Pad27)")
	(net 6 "unconnected-(IC1-LFILT3-Pad8)")
	(net 7 "unconnected-(IC1-LFILT2-Pad7)")
	(net 8 "unconnected-(IC1-EXT_LO_DEC-Pad3)")
	(net 9 "unconnected-(IC1-LFILT1-Pad6)")
	(net 10 "unconnected-(IC1-TM-Pad12)")
	(net 11 "unconnected-(IC1-RESETX-Pad29)")
	(net 12 "unconnected-(IC1-GPO4{slash}LD{slash}DO-Pad26)")
	(net 13 "unconnected-(IC1-MIX1_OPP-Pad18)")
	(net 14 "unconnected-(IC1-EXT_LO-Pad2)")
	(net 15 "unconnected-(IC1-NC_3-Pad21)")
	(net 16 "unconnected-(IC1-MIX2_IPN-Pad24)")
	(net 17 "unconnected-(IC1-REF_IN-Pad10)")
	(net 18 "unconnected-(IC1-MIX2_OPP-Pad28)")
	(net 19 "unconnected-(IC1-MIX1_IPP-Pad14)")
	(net 20 "unconnected-(IC1-DIG_VDD-Pad19)")
	(net 21 "unconnected-(IC1-NC_2-Pad20)")
	(net 22 "unconnected-(IC1-NC_1-Pad11)")
	(net 23 "unconnected-(IC1-ANA_VDD2-Pad22)")
	(net 24 "unconnected-(IC1-GPO2{slash}ADD2-Pad16)")
	(net 25 "unconnected-(IC1-EP-Pad33)")
	(net 26 "unconnected-(IC1-MIX1_OPN-Pad17)")
	(net 27 "unconnected-(IC1-GPO1{slash}ADD1-Pad15)")
	(net 28 "unconnected-(IC1-MIX2_IPP-Pad23)")
	(net 29 "unconnected-(IC1-GPO3{slash}FM-Pad25)")
	(net 30 "unconnected-(IC1-ENX-Pad30)")
	(net 31 "unconnected-(IC1-SCLK-Pad31)")
	(net 32 "unconnected-(IC1-SDATA-Pad32)")
	(net 33 "unconnected-(IC1-MIX1_IPN-Pad13)")
	(footprint "KiCad:DKMD2081"
		(layer "F.Cu")
		(at 103.7 100.05)
		(descr "QFN, 32-Pin, 5mm x 5mm")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "RFFC2071TR13"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.qorvo.com/products/d/da000696"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "85 - 2700 MHz RF Synthesizer / VCO with Integrated RF Mixer"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.9"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "772-RFFC2071"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Qorvo/RFFC2071TR13?qs=tkvX2tz6JTEyTj7lyvTFWA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Qorvo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "RFFC2071TR13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "lskonv1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.3 -1.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "unconnected-(IC1-ENBL{slash}GPO5-Pad1)")
			(pinfunction "ENBL/GPO5")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.3 -1.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(IC1-EXT_LO-Pad2)")
			(pinfunction "EXT_LO")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.3 -0.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(IC1-EXT_LO_DEC-Pad3)")
			(pinfunction "EXT_LO_DEC")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.3 -0.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(IC1-REXT-Pad4)")
			(pinfunction "REXT")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.3 0.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "unconnected-(IC1-ANA_VDD1-Pad5)")
			(pinfunction "ANA_VDD1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.3 0.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(IC1-LFILT1-Pad6)")
			(pinfunction "LFILT1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -2.3 1.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(IC1-LFILT2-Pad7)")
			(pinfunction "LFILT2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -2.3 1.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(IC1-LFILT3-Pad8)")
			(pinfunction "LFILT3")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.75 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "unconnected-(IC1-MODE{slash}GPO6-Pad9)")
			(pinfunction "MODE/GPO6")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -1.25 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(IC1-REF_IN-Pad10)")
			(pinfunction "REF_IN")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -0.75 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(IC1-NC_1-Pad11)")
			(pinfunction "NC_1")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -0.25 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(IC1-TM-Pad12)")
			(pinfunction "TM")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.25 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(IC1-MIX1_IPN-Pad13)")
			(pinfunction "MIX1_IPN")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.75 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(IC1-MIX1_IPP-Pad14)")
			(pinfunction "MIX1_IPP")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.25 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(IC1-GPO1{slash}ADD1-Pad15)")
			(pinfunction "GPO1/ADD1")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 1.75 2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(IC1-GPO2{slash}ADD2-Pad16)")
			(pinfunction "GPO2/ADD2")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.3 1.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(IC1-MIX1_OPN-Pad17)")
			(pinfunction "MIX1_OPN")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 2.3 1.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(IC1-MIX1_OPP-Pad18)")
			(pinfunction "MIX1_OPP")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 2.3 0.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(IC1-DIG_VDD-Pad19)")
			(pinfunction "DIG_VDD")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 2.3 0.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(IC1-NC_2-Pad20)")
			(pinfunction "NC_2")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 2.3 -0.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(IC1-NC_3-Pad21)")
			(pinfunction "NC_3")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 2.3 -0.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(IC1-ANA_VDD2-Pad22)")
			(pinfunction "ANA_VDD2")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 2.3 -1.25 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(IC1-MIX2_IPP-Pad23)")
			(pinfunction "MIX2_IPP")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 2.3 -1.75 90)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(IC1-MIX2_IPN-Pad24)")
			(pinfunction "MIX2_IPN")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 1.75 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(IC1-GPO3{slash}FM-Pad25)")
			(pinfunction "GPO3/FM")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 1.25 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(IC1-GPO4{slash}LD{slash}DO-Pad26)")
			(pinfunction "GPO4/LD/DO")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 0.75 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(IC1-MIX2_OPN-Pad27)")
			(pinfunction "MIX2_OPN")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 0.25 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(IC1-MIX2_OPP-Pad28)")
			(pinfunction "MIX2_OPP")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -0.25 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(IC1-RESETX-Pad29)")
			(pinfunction "RESETX")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -0.75 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(IC1-ENX-Pad30)")
			(pinfunction "ENX")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -1.25 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(IC1-SCLK-Pad31)")
			(pinfunction "SCLK")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at -1.75 -2.3)
			(size 0.23 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(IC1-SDATA-Pad32)")
			(pinfunction "SDATA")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 0 0)
			(size 3.7 3.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(IC1-EP-Pad33)")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "RFFC2071TR13.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(embedded_fonts no)
)
