(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:USB_C_Receptacle_USB2.0_16P"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 22.225 0)
			)
			(property "Value" "USB_C_Receptacle_USB2.0_16P"
				(at 0 19.685 0)
			)
			(property "Footprint" ""
				(at 3.81 0 0)
			)
			(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
				(at 3.81 0 0)
			)
			(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
				(at 0 0 0)
			)
			(property "ki_keywords" "usb universal serial bus type-C USB2.0"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "USB*C*Receptacle*"
				(at 0 0 0)
			)
			(symbol "USB_C_Receptacle_USB2.0_16P_0_0"
				(rectangle
					(start -0.254 -17.78)
					(end 0.254 -16.764)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 15.494)
					(end 9.144 14.986)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 10.414)
					(end 9.144 9.906)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 7.874)
					(end 9.144 7.366)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 2.794)
					(end 9.144 2.286)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 0.254)
					(end 9.144 -0.254)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 -2.286)
					(end 9.144 -2.794)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 -4.826)
					(end 9.144 -5.334)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 -12.446)
					(end 9.144 -12.954)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.16 -14.986)
					(end 9.144 -15.494)
					(fill
						(type none)
					)
				)
			)
			(symbol "USB_C_Receptacle_USB2.0_16P_0_1"
				(rectangle
					(start -10.16 17.78)
					(end 10.16 -17.78)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -8.89 -3.81) (xy -8.89 3.81)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -7.62 -3.81)
					(end -6.35 3.81)
					(fill
						(type outline)
					)
				)
				(arc
					(start -7.62 3.81)
					(mid -6.985 4.4423)
					(end -6.35 3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -7.62 3.81)
					(mid -6.985 4.4423)
					(end -6.35 3.81)
					(fill
						(type outline)
					)
				)
				(arc
					(start -8.89 3.81)
					(mid -6.985 5.7067)
					(end -5.08 3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -5.08 -3.81)
					(mid -6.985 -5.7067)
					(end -8.89 -3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -6.35 -3.81)
					(mid -6.985 -4.4423)
					(end -7.62 -3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start -6.35 -3.81)
					(mid -6.985 -4.4423)
					(end -7.62 -3.81)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -5.08 3.81) (xy -5.08 -3.81)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center -2.54 1.143)
					(radius 0.635)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.27 4.318) (xy 0 6.858) (xy 1.27 4.318) (xy -1.27 4.318)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 -2.032) (xy 2.54 0.508) (xy 2.54 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.302) (xy -2.54 -0.762) (xy -2.54 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.842) (xy 0 4.318)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 -5.842)
					(radius 1.27)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 1.905 1.778)
					(end 3.175 3.048)
					(fill
						(type outline)
					)
				)
			)
			(symbol "USB_C_Receptacle_USB2.0_16P_1_1"
				(pin passive line
					(at -7.62 -22.86 90)
					(length 5.08)
					(name "SHIELD")
					(number "S1")
				)
				(pin passive line
					(at 0 -22.86 90)
					(length 5.08)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 0 -22.86 90)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 0 -22.86 90)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B1")
				)
				(pin passive line
					(at 0 -22.86 90)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B12")
				)
				(pin passive line
					(at 15.24 15.24 180)
					(length 5.08)
					(name "VBUS")
					(number "A4")
				)
				(pin passive line
					(at 15.24 15.24 180)
					(length 5.08)
					(hide yes)
					(name "VBUS")
					(number "A9")
				)
				(pin passive line
					(at 15.24 15.24 180)
					(length 5.08)
					(hide yes)
					(name "VBUS")
					(number "B4")
				)
				(pin passive line
					(at 15.24 15.24 180)
					(length 5.08)
					(hide yes)
					(name "VBUS")
					(number "B9")
				)
				(pin bidirectional line
					(at 15.24 10.16 180)
					(length 5.08)
					(name "CC1")
					(number "A5")
				)
				(pin bidirectional line
					(at 15.24 7.62 180)
					(length 5.08)
					(name "CC2")
					(number "B5")
				)
				(pin bidirectional line
					(at 15.24 2.54 180)
					(length 5.08)
					(name "D-")
					(number "A7")
				)
				(pin bidirectional line
					(at 15.24 0 180)
					(length 5.08)
					(name "D-")
					(number "B7")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 5.08)
					(name "D+")
					(number "A6")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "D+")
					(number "B6")
				)
				(pin bidirectional line
					(at 15.24 -12.7 180)
					(length 5.08)
					(name "SBU1")
					(number "A8")
				)
				(pin bidirectional line
					(at 15.24 -15.24 180)
					(length 5.08)
					(name "SBU2")
					(number "B8")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 165.1 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 99.06 113.03) (xy 99.06 45.72)
		)
	)
	(wire
		(pts
			(xy 205.74 115.57) (xy 208.28 115.57)
		)
	)
	(wire
		(pts
			(xy 205.74 74.93) (xy 222.25 74.93)
		)
	)
	(wire
		(pts
			(xy 62.23 77.47) (xy 66.04 77.47)
		)
	)
	(wire
		(pts
			(xy 109.22 80.01) (xy 107.95 80.01)
		)
	)
	(wire
		(pts
			(xy 105.41 101.6) (xy 105.41 147.32)
		)
	)
	(wire
		(pts
			(xy 165.1 64.77) (xy 165.1 46.99)
		)
	)
	(wire
		(pts
			(xy 109.22 101.6) (xy 105.41 101.6)
		)
	)
	(wire
		(pts
			(xy 205.74 95.25) (xy 238.76 95.25)
		)
	)
	(wire
		(pts
			(xy 157.48 77.47) (xy 173.99 77.47)
		)
	)
	(wire
		(pts
			(xy 205.74 109.22) (xy 209.55 109.22)
		)
	)
	(wire
		(pts
			(xy 109.22 104.14) (xy 106.68 104.14)
		)
	)
	(wire
		(pts
			(xy 158.75 46.99) (xy 165.1 46.99)
		)
	)
	(wire
		(pts
			(xy 104.14 149.86) (xy 214.63 149.86)
		)
	)
	(wire
		(pts
			(xy 167.64 111.76) (xy 167.64 109.22)
		)
	)
	(wire
		(pts
			(xy 127 111.76) (xy 167.64 111.76)
		)
	)
	(wire
		(pts
			(xy 157.48 82.55) (xy 173.99 82.55)
		)
	)
	(wire
		(pts
			(xy 96.52 43.18) (xy 125.73 43.18)
		)
	)
	(wire
		(pts
			(xy 232.41 46.99) (xy 232.41 77.47)
		)
	)
	(wire
		(pts
			(xy 157.48 74.93) (xy 173.99 74.93)
		)
	)
	(wire
		(pts
			(xy 81.28 39.37) (xy 125.73 39.37)
		)
	)
	(wire
		(pts
			(xy 209.55 133.35) (xy 214.63 133.35)
		)
	)
	(wire
		(pts
			(xy 209.55 109.22) (xy 209.55 133.35)
		)
	)
	(wire
		(pts
			(xy 208.28 137.16) (xy 214.63 137.16)
		)
	)
	(wire
		(pts
			(xy 107.95 80.01) (xy 107.95 53.34)
		)
	)
	(wire
		(pts
			(xy 232.41 77.47) (xy 205.74 77.47)
		)
	)
	(wire
		(pts
			(xy 165.1 46.99) (xy 232.41 46.99)
		)
	)
	(wire
		(pts
			(xy 102.87 96.52) (xy 109.22 96.52)
		)
	)
	(wire
		(pts
			(xy 106.68 50.8) (xy 125.73 50.8)
		)
	)
	(wire
		(pts
			(xy 62.23 77.47) (xy 62.23 80.01)
		)
	)
	(wire
		(pts
			(xy 96.52 110.49) (xy 96.52 43.18)
		)
	)
	(wire
		(pts
			(xy 73.66 119.38) (xy 127 119.38)
		)
	)
	(wire
		(pts
			(xy 109.22 99.06) (xy 104.14 99.06)
		)
	)
	(wire
		(pts
			(xy 104.14 99.06) (xy 104.14 149.86)
		)
	)
	(wire
		(pts
			(xy 106.68 144.78) (xy 214.63 144.78)
		)
	)
	(wire
		(pts
			(xy 105.41 147.32) (xy 214.63 147.32)
		)
	)
	(wire
		(pts
			(xy 157.48 85.09) (xy 173.99 85.09)
		)
	)
	(wire
		(pts
			(xy 127 119.38) (xy 127 111.76)
		)
	)
	(wire
		(pts
			(xy 106.68 104.14) (xy 106.68 144.78)
		)
	)
	(wire
		(pts
			(xy 73.66 127) (xy 138.43 127)
		)
	)
	(wire
		(pts
			(xy 138.43 127) (xy 138.43 115.57)
		)
	)
	(wire
		(pts
			(xy 102.87 152.4) (xy 102.87 96.52)
		)
	)
	(wire
		(pts
			(xy 138.43 115.57) (xy 173.99 115.57)
		)
	)
	(wire
		(pts
			(xy 208.28 115.57) (xy 208.28 137.16)
		)
	)
	(wire
		(pts
			(xy 157.48 69.85) (xy 173.99 69.85)
		)
	)
	(wire
		(pts
			(xy 167.64 109.22) (xy 173.99 109.22)
		)
	)
	(wire
		(pts
			(xy 157.48 80.01) (xy 173.99 80.01)
		)
	)
	(wire
		(pts
			(xy 158.75 52.07) (xy 222.25 52.07)
		)
	)
	(wire
		(pts
			(xy 58.42 77.47) (xy 62.23 77.47)
		)
	)
	(wire
		(pts
			(xy 157.48 64.77) (xy 165.1 64.77)
		)
	)
	(wire
		(pts
			(xy 107.95 53.34) (xy 125.73 53.34)
		)
	)
	(wire
		(pts
			(xy 73.66 110.49) (xy 96.52 110.49)
		)
	)
	(wire
		(pts
			(xy 106.68 82.55) (xy 106.68 50.8)
		)
	)
	(wire
		(pts
			(xy 109.22 82.55) (xy 106.68 82.55)
		)
	)
	(wire
		(pts
			(xy 99.06 45.72) (xy 125.73 45.72)
		)
	)
	(wire
		(pts
			(xy 222.25 52.07) (xy 222.25 74.93)
		)
	)
	(wire
		(pts
			(xy 214.63 152.4) (xy 102.87 152.4)
		)
	)
	(wire
		(pts
			(xy 157.48 87.63) (xy 173.99 87.63)
		)
	)
	(wire
		(pts
			(xy 73.66 113.03) (xy 99.06 113.03)
		)
	)
	(symbol
		(lib_id "Connector:USB_C_Receptacle_USB2.0_16P")
		(at 66.04 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 66.04 31.75 0)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_16P"
			(at 66.04 34.29 0)
		)
		(property "Footprint" "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
			(at 69.85 54.61 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 69.85 54.61 0)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 66.04 54.61 0)
		)
		(pin "A4")
		(pin "A9")
		(pin "B7")
		(pin "B12")
		(pin "A12")
		(pin "B9")
		(pin "B1")
		(pin "A5")
		(pin "B8")
		(pin "B6")
		(pin "A6")
		(pin "B5")
		(pin "A8")
		(pin "S1")
		(pin "A1")
		(pin "B4")
		(pin "A7")
		(instances
			(project ""
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 62.23 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR030"
			(at 62.23 86.36 0)
		)
		(property "Value" "GND"
			(at 62.23 85.09 0)
		)
		(property "Footprint" ""
			(at 62.23 80.01 0)
		)
		(property "Datasheet" ""
			(at 62.23 80.01 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 62.23 80.01 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR030")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 173.99 60.96)
		(size 31.75 59.69)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "Mixer"
			(at 173.99 60.2484 0)
		)
		(property "Sheetfile" "mixer.kicad_sch"
			(at 173.99 121.2346 0)
		)
		(pin "3V_DIGIT" input
			(at 205.74 77.47 0)
		)
		(pin "3V_MIXER" input
			(at 205.74 74.93 0)
		)
		(pin "?" input
			(at 205.74 82.55 0)
		)
		(pin "ENBL_MIXER" input
			(at 173.99 85.09 180)
		)
		(pin "ENX_MIXER" input
			(at 173.99 82.55 180)
		)
		(pin "FREQ_REF" input
			(at 205.74 95.25 0)
		)
		(pin "LO_EXT" input
			(at 205.74 88.9 0)
		)
		(pin "MODE_MIXER" input
			(at 173.99 87.63 180)
		)
		(pin "PLL_Lock" input
			(at 173.99 69.85 180)
		)
		(pin "RESETX_MIXER" input
			(at 173.99 80.01 180)
		)
		(pin "RF_MIX_IN1" input
			(at 173.99 109.22 180)
		)
		(pin "RF_MIX_IN2" input
			(at 173.99 115.57 180)
		)
		(pin "RF_MIX_OUT1" input
			(at 205.74 109.22 0)
		)
		(pin "RF_MIX_OUT2" input
			(at 205.74 115.57 0)
		)
		(pin "SCLK_MIXER" input
			(at 173.99 77.47 180)
		)
		(pin "SDATA_MIXER" input
			(at 173.99 74.93 180)
		)
		(instances
			(project "lskonv1"
				(path
					(page "2")
				)
			)
		)
	)
	(sheet
		(at 238.76 91.44)
		(size 27.94 25.4)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "REF"
			(at 238.76 90.7284 0)
		)
		(property "Sheetfile" "reference.kicad_sch"
			(at 238.76 117.4246 0)
		)
		(pin "FREQ_REF" input
			(at 238.76 95.25 180)
		)
		(instances
			(project "lskonv1"
				(path
					(page "5")
				)
			)
		)
	)
	(sheet
		(at 214.63 129.54)
		(size 43.18 26.67)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "OUT_DATT"
			(at 214.63 128.8284 0)
		)
		(property "Sheetfile" "out_datt.kicad_sch"
			(at 214.63 156.7946 0)
		)
		(pin "3V_IN" input
			(at 257.81 132.08 0)
		)
		(pin "RF_IN_1" input
			(at 214.63 133.35 180)
		)
		(pin "RF_IN_2" input
			(at 214.63 137.16 180)
		)
		(pin "RF_OUT_1" input
			(at 257.81 135.89 0)
		)
		(pin "RF_OUT_2" input
			(at 257.81 139.7 0)
		)
		(pin "SERIAL_CLK" input
			(at 214.63 144.78 180)
		)
		(pin "SERIAL_DATA" input
			(at 214.63 147.32 180)
		)
		(pin "SERIAL_LE1" input
			(at 214.63 149.86 180)
		)
		(pin "SERIAL_LE2" input
			(at 214.63 152.4 180)
		)
		(instances
			(project "lskonv1"
				(path
					(page "7")
				)
			)
		)
	)
	(sheet
		(at 44.45 106.68)
		(size 29.21 26.67)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "RF_Frontend"
			(at 44.45 105.9684 0)
		)
		(property "Sheetfile" "rf_frontend.kicad_sch"
			(at 44.45 133.9346 0)
		)
		(pin "5V_LNA_CH1" input
			(at 73.66 110.49 0)
		)
		(pin "5V_LNA_CH2" input
			(at 73.66 113.03 0)
		)
		(pin "RF1_IN" input
			(at 44.45 119.38 180)
		)
		(pin "RF1_OUT" input
			(at 73.66 119.38 0)
		)
		(pin "RF2_IN" input
			(at 44.45 127 180)
		)
		(pin "RF2_OUT" input
			(at 73.66 127 0)
		)
		(instances
			(project "lskonv1"
				(path
					(page "6")
				)
			)
		)
	)
	(sheet
		(at 125.73 35.56)
		(size 33.02 20.32)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "PSU"
			(at 125.73 34.8484 0)
		)
		(property "Sheetfile" "psu.kicad_sch"
			(at 125.73 56.4646 0)
		)
		(pin "3V_DIGIT" input
			(at 158.75 46.99 0)
		)
		(pin "3V_MIXER" input
			(at 158.75 52.07 0)
		)
		(pin "5V_VIN" input
			(at 125.73 39.37 180)
		)
		(pin "LNA1_PSU" input
			(at 125.73 43.18 180)
		)
		(pin "LNA2_PSU" input
			(at 125.73 45.72 180)
		)
		(pin "LNA_CH1_EN" input
			(at 125.73 53.34 180)
		)
		(pin "LNA_CH2_EN" input
			(at 125.73 50.8 180)
		)
		(instances
			(project "lskonv1"
				(path
					(page "4")
				)
			)
		)
	)
	(sheet
		(at 109.22 62.23)
		(size 48.26 45.72)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "MCU"
			(at 109.22 61.5184 0)
		)
		(property "Sheetfile" "mcu.kicad_sch"
			(at 109.22 108.5346 0)
		)
		(pin "3V_DIGIT" input
			(at 157.48 64.77 0)
		)
		(pin "DATT_LE1" input
			(at 109.22 99.06 180)
		)
		(pin "DATT_LE2" input
			(at 109.22 96.52 180)
		)
		(pin "DATT_SCK" input
			(at 109.22 104.14 180)
		)
		(pin "DATT_SDA" input
			(at 109.22 101.6 180)
		)
		(pin "ENBL_MIXER" input
			(at 157.48 85.09 0)
		)
		(pin "ENX_MIXER" input
			(at 157.48 82.55 0)
		)
		(pin "LNA_CH1_EN" input
			(at 109.22 80.01 180)
		)
		(pin "LNA_CH2_EN" input
			(at 109.22 82.55 180)
		)
		(pin "MCU_RST" input
			(at 109.22 88.9 180)
		)
		(pin "MODE_MIXER" input
			(at 157.48 87.63 0)
		)
		(pin "PLL_LOCK_MIXER" input
			(at 157.48 69.85 0)
		)
		(pin "RESETX_MIXER" input
			(at 157.48 80.01 0)
		)
		(pin "SCLK_MIXER" input
			(at 157.48 77.47 0)
		)
		(pin "SDATA_MIXER" input
			(at 157.48 74.93 0)
		)
		(instances
			(project "lskonv1"
				(path
					(page "3")
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
