(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MCU_ST_STM32F0:STM32F042G6Ux"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -17.78 21.59 0)
			)
			(property "Value" "STM32F042G6Ux"
				(at 5.08 21.59 0)
			)
			(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
				(at -17.78 -20.32 0)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042g6.pdf"
				(at 0 0 0)
			)
			(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
				(at 0 0 0)
			)
			(symbol "STM32F042G6Ux_0_1"
				(rectangle
					(start -17.78 -20.32)
					(end 17.78 20.32)
					(fill
						(type background)
					)
				)
			)
			(symbol "STM32F042G6Ux_1_1"
				(pin input line
					(at -20.32 15.24 0)
					(length 2.54)
					(name "NRST")
					(number "4")
				)
				(pin bidirectional line
					(at -20.32 10.16 0)
					(length 2.54)
					(name "PF0")
					(number "2")
					(alternate "CRS_SYNC" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "RCC_OSC_IN" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 7.62 0)
					(length 2.54)
					(name "PF1")
					(number "3")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "RCC_OSC_OUT" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 2.54 0)
					(length 2.54)
					(name "PB0")
					(number "14")
					(alternate "ADC_IN8" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "TSC_G3_IO2" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 0 0)
					(length 2.54)
					(name "PB1")
					(number "15")
					(alternate "ADC_IN9" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "TSC_G3_IO3" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 -2.54 0)
					(length 2.54)
					(name "PB3")
					(number "24")
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "TSC_G5_IO1" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 -5.08 0)
					(length 2.54)
					(name "PB4")
					(number "25")
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TSC_G5_IO2" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 -7.62 0)
					(length 2.54)
					(name "PB5")
					(number "26")
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "SYS_WKUP6" bidirectional line)
					(alternate "TIM16_BKIN" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 -10.16 0)
					(length 2.54)
					(name "PB6")
					(number "27")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "TIM16_CH1N" bidirectional line)
					(alternate "TSC_G5_IO3" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 -12.7 0)
					(length 2.54)
					(name "PB7")
					(number "28")
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "TSC_G5_IO4" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at -20.32 -15.24 0)
					(length 2.54)
					(name "PB8")
					(number "1")
					(alternate "CAN_RX" bidirectional line)
					(alternate "CEC" bidirectional line)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TSC_SYNC" bidirectional line)
				)
				(pin power_in line
					(at -2.54 22.86 270)
					(length 2.54)
					(name "VDD")
					(number "17")
				)
				(pin power_in line
					(at 0 22.86 270)
					(length 2.54)
					(name "VDDA")
					(number "5")
				)
				(pin power_in line
					(at 0 -22.86 90)
					(length 2.54)
					(name "VSSA")
					(number "16")
				)
				(pin power_in line
					(at 2.54 22.86 270)
					(length 2.54)
					(name "VDDIO2")
					(number "18")
				)
				(pin bidirectional line
					(at 20.32 15.24 180)
					(length 2.54)
					(name "PA0")
					(number "6")
					(alternate "ADC_IN0" bidirectional line)
					(alternate "RTC_TAMP2" bidirectional line)
					(alternate "SYS_WKUP1" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "TSC_G1_IO1" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 12.7 180)
					(length 2.54)
					(name "PA1")
					(number "7")
					(alternate "ADC_IN1" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "TSC_G1_IO2" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 10.16 180)
					(length 2.54)
					(name "PA2")
					(number "8")
					(alternate "ADC_IN2" bidirectional line)
					(alternate "SYS_WKUP4" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TSC_G1_IO3" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 7.62 180)
					(length 2.54)
					(name "PA3")
					(number "9")
					(alternate "ADC_IN3" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "TSC_G1_IO4" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 5.08 180)
					(length 2.54)
					(name "PA4")
					(number "10")
					(alternate "ADC_IN4" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TSC_G2_IO1" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 2.54 180)
					(length 2.54)
					(name "PA5")
					(number "11")
					(alternate "ADC_IN5" bidirectional line)
					(alternate "CEC" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "TSC_G2_IO2" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 0 180)
					(length 2.54)
					(name "PA6")
					(number "12")
					(alternate "ADC_IN6" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TSC_G2_IO3" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "PA7")
					(number "13")
					(alternate "ADC_IN7" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TSC_G2_IO4" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "PA9/PA11")
					(number "19")
					(alternate "CAN_RX (PA11)" bidirectional line)
					(alternate "I2C1_SCL (PA11)" bidirectional line)
					(alternate "I2C1_SCL (PA9)" bidirectional line)
					(alternate "PA11" bidirectional line)
					(alternate "PA9" bidirectional line)
					(alternate "TIM1_CH2 (PA9)" bidirectional line)
					(alternate "TIM1_CH4 (PA11)" bidirectional line)
					(alternate "TSC_G4_IO1 (PA9)" bidirectional line)
					(alternate "TSC_G4_IO3 (PA11)" bidirectional line)
					(alternate "USART1_CTS (PA11)" bidirectional line)
					(alternate "USART1_TX (PA9)" bidirectional line)
					(alternate "USB_DM (PA11)" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "PA10/PA12")
					(number "20")
					(alternate "CAN_TX (PA12)" bidirectional line)
					(alternate "I2C1_SDA (PA10)" bidirectional line)
					(alternate "PA10" bidirectional line)
					(alternate "PA12" bidirectional line)
					(alternate "TIM17_BKIN (PA10)" bidirectional line)
					(alternate "TIM1_CH3 (PA10)" bidirectional line)
					(alternate "TIM1_ETR (PA12)" bidirectional line)
					(alternate "TSC_G4_IO2 (PA10)" bidirectional line)
					(alternate "TSC_G4_IO4 (PA12)" bidirectional line)
					(alternate "USART1_DE (PA12)" bidirectional line)
					(alternate "USART1_RTS (PA12)" bidirectional line)
					(alternate "USART1_RX (PA10)" bidirectional line)
					(alternate "USB_DP (PA12)" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "PA13")
					(number "21")
					(alternate "IR_OUT" bidirectional line)
					(alternate "SYS_SWDIO" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "PA14")
					(number "22")
					(alternate "SYS_SWCLK" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "PA15")
					(number "23")
					(alternate "I2S1_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 135.89 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 138.43 90.17) (xy 135.89 90.17)
		)
	)
	(wire
		(pts
			(xy 135.89 93.98) (xy 135.89 90.17)
		)
	)
	(wire
		(pts
			(xy 138.43 93.98) (xy 138.43 90.17)
		)
	)
	(wire
		(pts
			(xy 133.35 90.17) (xy 133.35 93.98)
		)
	)
	(wire
		(pts
			(xy 111.76 76.2) (xy 109.22 76.2)
		)
	)
	(wire
		(pts
			(xy 133.35 73.66) (xy 133.35 90.17)
		)
	)
	(wire
		(pts
			(xy 109.22 87.63) (xy 109.22 90.17)
		)
	)
	(wire
		(pts
			(xy 135.89 90.17) (xy 133.35 90.17)
		)
	)
	(wire
		(pts
			(xy 109.22 90.17) (xy 115.57 90.17)
		)
	)
	(wire
		(pts
			(xy 135.89 139.7) (xy 135.89 142.24)
		)
	)
	(wire
		(pts
			(xy 115.57 90.17) (xy 115.57 101.6)
		)
	)
	(wire
		(pts
			(xy 109.22 76.2) (xy 109.22 80.01)
		)
	)
	(wire
		(pts
			(xy 109.22 97.79) (xy 109.22 99.06)
		)
	)
	(hierarchical_label "DATT_LE2"
		(shape input)
		(at 214.63 104.14 0)
	)
	(hierarchical_label "RESETX_MIXER"
		(shape input)
		(at 184.15 80.01 0)
	)
	(hierarchical_label "ENX_MIXER"
		(shape input)
		(at 180.2013 75.7342 0)
	)
	(hierarchical_label "PLL_LOCK_MIXER"
		(shape input)
		(at 184.15 100.33 0)
	)
	(hierarchical_label "SDATA_MIXER"
		(shape input)
		(at 189.23 95.25 0)
	)
	(hierarchical_label "SCLK_MIXER"
		(shape input)
		(at 185.42 88.9 0)
	)
	(hierarchical_label "MODE_MIXER"
		(shape input)
		(at 175.26 66.04 0)
	)
	(hierarchical_label "ENBL_MIXER"
		(shape input)
		(at 177.8 69.85 0)
	)
	(hierarchical_label "DATT_SCK"
		(shape input)
		(at 214.63 76.2 0)
	)
	(hierarchical_label "LNA_CH1_EN"
		(shape input)
		(at 43.18 104.14 0)
	)
	(hierarchical_label "3V_DIGIT"
		(shape input)
		(at 133.35 73.66 0)
	)
	(hierarchical_label "DATT_LE1"
		(shape input)
		(at 215.9 95.25 0)
	)
	(hierarchical_label "MCU_RST"
		(shape input)
		(at 115.57 90.17 0)
	)
	(hierarchical_label "DATT_SDA"
		(shape input)
		(at 214.63 83.82 0)
	)
	(hierarchical_label "LNA_CH2_EN"
		(shape input)
		(at 43.18 106.68 0)
	)
	(hierarchical_label "3V_DIGIT"
		(shape input)
		(at 111.76 76.2 0)
	)
	(symbol
		(lib_id "Device:R")
		(at 109.22 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R24"
			(at 111.76 82.5499 0)
		)
		(property "Value" "100k"
			(at 111.76 85.0899 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 107.442 83.82 90)
		)
		(property "Datasheet" "~"
			(at 109.22 83.82 0)
		)
		(property "Description" "Resistor"
			(at 109.22 83.82 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_ST_STM32F0:STM32F042G6Ux")
		(at 135.89 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 138.0333 139.7 0)
		)
		(property "Value" "STM32F042G6Ux"
			(at 138.0333 142.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at 118.11 137.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042g6.pdf"
			(at 135.89 116.84 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 135.89 116.84 0)
		)
		(pin "6")
		(pin "2")
		(pin "12")
		(pin "10")
		(pin "1")
		(pin "7")
		(pin "8")
		(pin "14")
		(pin "26")
		(pin "24")
		(pin "25")
		(pin "21")
		(pin "19")
		(pin "15")
		(pin "18")
		(pin "16")
		(pin "20")
		(pin "17")
		(pin "23")
		(pin "5")
		(pin "11")
		(pin "28")
		(pin "9")
		(pin "27")
		(pin "22")
		(pin "4")
		(pin "3")
		(pin "13")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 109.22 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C33"
			(at 102.616 92.202 0)
		)
		(property "Value" "1n"
			(at 102.616 94.742 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 110.1852 97.79 0)
		)
		(property "Datasheet" "~"
			(at 109.22 93.98 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 109.22 93.98 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "C33")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 109.22 99.06 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR041"
			(at 109.22 105.41 0)
		)
		(property "Value" "GND"
			(at 109.22 103.378 0)
		)
		(property "Footprint" ""
			(at 109.22 99.06 0)
		)
		(property "Datasheet" ""
			(at 109.22 99.06 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 109.22 99.06 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR041")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 135.89 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR042"
			(at 135.89 148.59 0)
		)
		(property "Value" "GND"
			(at 135.89 146.558 0)
		)
		(property "Footprint" ""
			(at 135.89 142.24 0)
		)
		(property "Datasheet" ""
			(at 135.89 142.24 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 135.89 142.24 0)
		)
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "#PWR042")
					(unit 1)
				)
			)
		)
	)
)
