(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(IC1-PC)")
	(net 2 "Net-(J1-In)")
	(net 3 "Net-(IC1-P1)")
	(net 4 "Net-(J2-In)")
	(net 5 "Net-(IC1-P2)")
	(net 6 "Net-(J3-In)")
	(net 7 "Net-(IC1-P3)")
	(net 8 "Net-(J4-In)")
	(net 9 "Net-(IC1-P4)")
	(net 10 "Net-(J5-In)")
	(net 11 "Net-(D1-K)")
	(net 12 "Net-(D1-A)")
	(net 13 "Net-(D2-K)")
	(net 14 "Net-(D3-K)")
	(net 15 "GND")
	(net 16 "Net-(IC1-VCTL1)")
	(net 17 "Net-(IC1-VCTL2)")
	(net 18 "VCC")
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 126.25 92 45)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D3"
			(at 0 -1.65 45)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.65 45)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.024999 0 45)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 14 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.024999 0 45)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 13 "Net-(D2-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 128.5 88.025 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 13 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 11 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 123 105.225 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0.025 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J1-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(IC1-PC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 131.4 104.6 135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.989949 2.404163 135)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 135)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 135)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J2-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 135)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(IC1-P1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 120.25 83.25)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 10 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(IC1-VCTL2)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(IC1-VCTL1)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 124.75 83.25)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 7.46 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D3-K)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:QFN40P180X180X43-13N-D"
		(layer "F.Cu")
		(at 123 98.05 180)
		(descr "EQFN12-E2")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "NJG1684ME2-TE1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.nisshinbo-microdevices.co.jp/en/pdf/datasheet/NJG1684ME2_E.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Switch IC CDMA, GSM, LTE, UMTS SP4T 50Ohm 12-EQFN (1.8x1.8)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.427"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Nisshinbo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "NJG1684ME2-TE1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "513-NJG1684ME2-TE1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nisshinbo/NJG1684ME2-TE1?qs=chTDxNqvsymdJZJqSy5VSg%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1.75 4.05 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.95 -0.4 270)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(IC1-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC1-P2)")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.95 0.4 270)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.4 0.95 180)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(D3-K)")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 0.95 180)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(IC1-VCTL2)")
			(pinfunction "VCTL2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.4 0.95 180)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(IC1-VCTL1)")
			(pinfunction "VCTL1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.95 0.4 270)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.95 0 270)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(IC1-P4)")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.95 -0.4 270)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(IC1-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.4 -0.95 180)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "GND_3")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0 -0.95 180)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(IC1-PC)")
			(pinfunction "PC")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -0.4 -0.95 180)
			(size 0.2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0 0 180)
			(size 0.84 0.84)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "GND_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "NJG1684ME2-TE1.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 131.401992 91.898008 -135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0.922056 -2.616295 45)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 45)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 225)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J3-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 225)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(IC1-P2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114.601992 91.901992 135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -0.633579 -2.616295 135)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 135)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 135)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(IC1-P4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 135)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J5-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114.601992 104.598008 -135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -0.70429 2.404163 45)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 45)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 225)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(IC1-P3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 225)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J4-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Maresz_custom:SMA_Straight_PCB_Edge_6mm"
		(layer "F.Cu")
		(at 135.25 91.25 -90)
		(property "Reference" "J3"
			(at -4.25 -2 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.75)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J3-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.75 -2)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2 270)
			(size 7 4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.SilkS")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135 87.5) (xy 135 95) (xy 139.5 95) (xy 139.5 87.5)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Maresz_custom:SMA_Straight_PCB_Edge_6mm"
		(layer "F.Cu")
		(at 110.75 105.25 90)
		(property "Reference" "J4"
			(at -4.25 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.75 180)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(J4-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.75 -2 180)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2 90)
			(size 7 4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2 180)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.SilkS")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 111 109) (xy 111 101.5) (xy 106.5 101.5) (xy 106.5 109)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Maresz_custom:SMA_Straight_PCB_Edge_6mm"
		(layer "F.Cu")
		(at 110.75 91.25 90)
		(property "Reference" "J5"
			(at -4.25 -2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.75 180)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J5-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.75 -2 180)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2 90)
			(size 7 4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2 180)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.SilkS")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 111 95) (xy 111 87.5) (xy 106.5 87.5) (xy 106.5 95)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Maresz_custom:SMA_Straight_PCB_Edge_6mm"
		(layer "F.Cu")
		(at 135.25 105.25 -90)
		(property "Reference" "J2"
			(at -4.25 -2 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.75)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J2-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.75 -2)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2 270)
			(size 7 4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.SilkS")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135 101.5) (xy 135 109) (xy 139.5 109) (xy 139.5 101.5)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Maresz_custom:SMA_Straight_PCB_Edge_6mm"
		(layer "F.Cu")
		(at 123 110 180)
		(property "Reference" "J1"
			(at -4.25 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.75 270)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(J1-In)")
			(pinfunction "In")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -2.75 -2 270)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2 180)
			(size 7 4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2 270)
			(size 4 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.SilkS")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 126.75 109.75) (xy 119.25 109.75) (xy 119.25 114.25) (xy 126.75 114.25)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 128.5 84.25 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "sp4t-njg1684-v01.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 11 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 12 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 106.25 79.25)
		(end 139.75 114.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 115.25 84 0)
		(layer "F.SilkS")
	)
	(gr_text "VCC"
		(at 115.5 86.5 0)
		(layer "F.SilkS")
	)
	(gr_text "C1"
		(at 116.5 89 0)
		(layer "F.SilkS")
	)
	(gr_text "C2"
		(at 116.5 91.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Design by Maresz\nv1.0"
		(at 129.6 109.2 0)
		(layer "B.SilkS")
	)
	(gr_text "NJG1684ME2\n3GHz SP4T eval"
		(at 133.2 100.5 0)
		(layer "B.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.625 90.775) (xy 129.975 92.425) (xy 129.725 92.175) (xy 131.375 90.525)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.01)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.35 97.75) (xy 123 98.05) (xy 123.65 97.75) (xy 124.15 97.55) (xy 124.15 96.9) (xy 123.5 97.55)
				(xy 122.5 97.55) (xy 121.85 96.9) (xy 121.85 97.55)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(IC1-P1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.6 98.35) (xy 125.85 98.35) (xy 126.05 98.55) (xy 125.35 99.25) (xy 124.6 98.55)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125 99.6) (xy 126.2 98.3) (xy 124.85 97.05) (xy 124.1 97.2) (xy 124.103368 95.6) (xy 131.4 87.7)
				(xy 139.2 87.7) (xy 139.2 109) (xy 134.2 114) (xy 125.001772 114) (xy 125 101.15)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.55 98.7) (xy 122.7 98.7) (xy 122.7 99.3) (xy 122.698228 99.6) (xy 121.998228 100.2) (xy 121.998228 114)
				(xy 120.998228 114) (xy 121 101.15) (xy 121 99.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.575 102.875) (xy 132.225 104.525) (xy 132.475 104.275) (xy 130.825 102.625)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121 99.6) (xy 119.8 98.3) (xy 121.15 97.05) (xy 121.9 97.2) (xy 121.896632 95.6) (xy 114.6 87.7)
				(xy 106.8 87.7) (xy 106.8 109) (xy 111.8 114) (xy 120.998228 114) (xy 121 101.15)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(IC1-P2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.6 97.95) (xy 125.35 97.25) (xy 126.05 97.95) (xy 125.85 98.15) (xy 124.6 98.15)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(IC1-P3)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.4 98.35) (xy 120.15 98.35) (xy 119.95 98.55) (xy 120.65 99.25) (xy 121.4 98.55)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.775 104.375) (xy 131.425 106.025) (xy 131.675 105.775) (xy 130.025 104.125)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.45 102.85) (xy 113.8 104.5) (xy 113.55 104.25) (xy 115.2 102.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.425 92.275) (xy 130.775 93.925) (xy 130.525 93.675) (xy 132.175 92.025)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.525 92.225) (xy 115.175 93.875) (xy 115.425 93.625) (xy 113.775 91.975)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.4 96.8) (xy 122.35 97.55) (xy 122.35 97.75) (xy 121.5 97.75) (xy 121.1 96.95)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.446256 98.7) (xy 123.296256 98.7) (xy 123.296256 99.3) (xy 123.298028 99.6) (xy 123.998028 100.2)
				(xy 123.998028 114) (xy 124.998028 114) (xy 124.996256 101.15) (xy 124.996256 99.6)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.6 96.8) (xy 123.65 97.55) (xy 123.65 97.75) (xy 124.5 97.75) (xy 124.9 96.95)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.3 90.7) (xy 115.95 92.35) (xy 116.2 92.1) (xy 114.55 90.45)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Net-(IC1-PC)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.5 100.2) (xy 122.9 99.6) (xy 122.9 99.4) (xy 123.1 99.4) (xy 123.1 99.6) (xy 123.5 100.2)
				(xy 123.5 100.6) (xy 122.5 100.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.2 104.4) (xy 114.55 106.05) (xy 114.3 105.8) (xy 115.95 104.15)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(IC1-P4)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.4 97.95) (xy 120.65 97.25) (xy 119.95 97.95) (xy 120.15 98.15) (xy 121.4 98.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.75 107.25) (xy 115 107.25) (xy 121 100.75) (xy 121 99.3) (xy 122.75 99.3) (xy 122.75 97.75)
				(xy 114.5 89.25) (xy 106.75 89.25) (xy 106.75 93.25) (xy 113.25 93.25) (xy 118.25 98.25) (xy 113.5 103.25)
				(xy 106.75 103.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125 114) (xy 125 99.3) (xy 121 99.3) (xy 121 114)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.001)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.25 107.25) (xy 131 107.25) (xy 125 100.75) (xy 125 99.3) (xy 123.25 99.3) (xy 123.25 97.75)
				(xy 131.5 89.25) (xy 139.25 89.25) (xy 139.25 93.25) (xy 132.75 93.25) (xy 127.75 98.25) (xy 132.5 103.25)
				(xy 139.25 103.25)
			)
		)
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.75 109) (xy 111.75 114) (xy 134.25 114) (xy 139.25 109) (xy 139.25 84.75) (xy 134.25 79.75)
				(xy 111.75 79.75) (xy 106.75 84.75)
			)
		)
	)
	(embedded_fonts no)
)
