(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "TCCH-80+" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 39.37 7.62 0))
    (property "Value" "TCCH-80+" (at 39.37 5.08 0))
    (property "Footprint" "TCCH80" (at 39.37 -94.92 0))
    (property "Datasheet" "https://www.minicircuits.com/pdfs/TCCH-80+.pdf" (at 39.37 -194.92 0))
    (property "ki_description" "RF Choke" (at 39.37 -294.92 0))
    (property "Height" "3.81" (at 39.37 -394.92 0))
    (property "Mouser Part Number" "139-TCCH-80" (at 39.37 -494.92 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/TCCH-80%2b?qs=xZ%2FP%252Ba9zWqbIZgt27nGgHg%3D%3D" (at 39.37 -594.92 0))
    (property "Manufacturer_Name" "Mini-Circuits" (at 39.37 -694.92 0))
    (property "Manufacturer_Part_Number" "TCCH-80+" (at 39.37 -794.92 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "RF-IN_&_DC")
      (number "1")
    )
    (pin passive line (at 43.18 0 180) (length 5.08)
      (name "NOT_USED_1")
      (number "2")
    )
    (pin passive line (at 43.18 -2.54 180) (length 5.08)
      (name "DC")
      (number "3")
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "NOT_USED_2")
      (number "4")
    )
  )
)
