(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:Conn_01x03_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x03_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x03, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x03_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0.8636 2.54)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 2.667)
					(end 0 2.413)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
			)
		)
		(symbol "Connector:Conn_Coaxial_Small"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0.254 3.048 0)
			)
			(property "Value" "Conn_Coaxial_Small"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" " ~"
				(at 0 0 0)
			)
			(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
				(at 0 0 0)
			)
			(property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*"
				(at 0 0 0)
			)
			(symbol "Conn_Coaxial_Small_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy -0.508 0)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
			)
			(symbol "Conn_Coaxial_Small_1_1"
				(arc
					(start -1.1916 -0.6311)
					(mid 0.327 -1.3081)
					(end 1.3484 0.0039)
					(fill
						(type none)
					)
				)
				(arc
					(start 1.3484 -0.0039)
					(mid 0.327 1.3081)
					(end -1.1916 0.6311)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -2.54 0 0)
					(length 1.27)
					(name "In")
					(number "1")
				)
				(pin passive line
					(at 2.54 0 180)
					(length 1.27)
					(name "Ext")
					(number "2")
				)
			)
		)
		(symbol "Device:C"
			(pin_numbers hide)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:L"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -1.27 0 90)
			)
			(property "Value" "L"
				(at 1.905 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_0_1"
				(arc
					(start 0 -2.54)
					(mid 0.6323 -1.905)
					(end 0 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.27)
					(mid 0.6323 -0.635)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.6323 0.635)
					(end 0 1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.27)
					(mid 0.6323 1.905)
					(end 0 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 111.76 64.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 59.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 64.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 77.47 82.55) (xy 91.44 82.55)
		)
	)
	(wire
		(pts
			(xy 72.39 64.77) (xy 72.39 82.55)
		)
	)
	(wire
		(pts
			(xy 158.75 82.55) (xy 158.75 93.98)
		)
	)
	(wire
		(pts
			(xy 109.22 59.69) (xy 72.39 59.69)
		)
	)
	(wire
		(pts
			(xy 72.39 93.98) (xy 114.3 93.98)
		)
	)
	(wire
		(pts
			(xy 72.39 59.69) (xy 72.39 64.77)
		)
	)
	(wire
		(pts
			(xy 72.39 64.77) (xy 81.28 64.77)
		)
	)
	(wire
		(pts
			(xy 109.22 59.69) (xy 109.22 57.15)
		)
	)
	(wire
		(pts
			(xy 101.6 64.77) (xy 111.76 64.77)
		)
	)
	(wire
		(pts
			(xy 88.9 64.77) (xy 93.98 64.77)
		)
	)
	(wire
		(pts
			(xy 114.3 93.98) (xy 114.3 97.79)
		)
	)
	(wire
		(pts
			(xy 114.3 59.69) (xy 109.22 59.69)
		)
	)
	(wire
		(pts
			(xy 114.3 57.15) (xy 114.3 59.69)
		)
	)
	(wire
		(pts
			(xy 111.76 82.55) (xy 153.67 82.55)
		)
	)
	(wire
		(pts
			(xy 111.76 72.39) (xy 111.76 74.93)
		)
	)
	(wire
		(pts
			(xy 111.76 57.15) (xy 111.76 64.77)
		)
	)
	(wire
		(pts
			(xy 72.39 82.55) (xy 72.39 93.98)
		)
	)
	(wire
		(pts
			(xy 114.3 93.98) (xy 158.75 93.98)
		)
	)
	(wire
		(pts
			(xy 99.06 82.55) (xy 111.76 82.55)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 114.3 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 114.3 104.14 0)
		)
		(property "Value" "GND"
			(at 114.3 102.87 0)
		)
		(property "Footprint" ""
			(at 114.3 97.79 0)
		)
		(property "Datasheet" ""
			(at 114.3 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 114.3 97.79 0)
		)
		(pin "1")
		(instances
			(project "biastee1"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_Coaxial_Small")
		(at 74.93 82.55 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1_rf1"
			(at 75.4495 76.2 0)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 75.4495 78.74 0)
		)
		(property "Footprint" "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
			(at 74.93 82.55 0)
		)
		(property "Datasheet" " ~"
			(at 74.93 82.55 0)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 74.93 82.55 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "biastee1"
				(path
					(reference "J1_rf1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 95.25 82.55 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 95.25 74.93 90)
		)
		(property "Value" "C"
			(at 95.25 77.47 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 99.06 81.5848 0)
		)
		(property "Datasheet" "~"
			(at 95.25 82.55 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 95.25 82.55 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "biastee1"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 85.09 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 83.5025 58.42 0)
		)
		(property "Value" "LED"
			(at 83.5025 60.96 0)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 85.09 64.77 0)
		)
		(property "Datasheet" "~"
			(at 85.09 64.77 0)
		)
		(property "Description" "Light emitting diode"
			(at 85.09 64.77 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "biastee1"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 111.76 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L2"
			(at 113.03 67.3099 0)
		)
		(property "Value" "L"
			(at 113.03 69.8499 0)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 111.76 68.58 0)
		)
		(property "Datasheet" "~"
			(at 111.76 68.58 0)
		)
		(property "Description" "Inductor"
			(at 111.76 68.58 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "biastee1"
				(path
					(reference "L2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_Coaxial_Small")
		(at 156.21 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2_rfdc1"
			(at 155.6904 76.2 0)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 155.6904 78.74 0)
		)
		(property "Footprint" "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
			(at 156.21 82.55 0)
		)
		(property "Datasheet" " ~"
			(at 156.21 82.55 0)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 156.21 82.55 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "biastee1"
				(path
					(reference "J2_rfdc1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 111.76 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L1"
			(at 113.03 77.4699 0)
		)
		(property "Value" "6.8uH"
			(at 113.03 80.0099 0)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 111.76 78.74 0)
		)
		(property "Datasheet" "~"
			(at 111.76 78.74 0)
		)
		(property "Description" "Inductor"
			(at 111.76 78.74 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "biastee1"
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 111.76 52.07 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 111.76 46.99 90)
		)
		(property "Value" "Conn_01x03_Pin"
			(at 111.76 49.53 90)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 111.76 52.07 0)
		)
		(property "Datasheet" "~"
			(at 111.76 52.07 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 111.76 52.07 0)
		)
		(pin "3")
		(pin "1")
		(pin "2")
		(instances
			(project "biastee1"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 97.79 64.77 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 97.79 58.42 90)
		)
		(property "Value" "1k"
			(at 97.79 60.96 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 97.79 66.548 90)
		)
		(property "Datasheet" "~"
			(at 97.79 64.77 0)
		)
		(property "Description" "Resistor"
			(at 97.79 64.77 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "biastee1"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
