(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "ADE-5+:ADE-5+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 34.29 7.62 0)
			)
			(property "Value" "ADE-5+"
				(at 34.29 5.08 0)
			)
			(property "Footprint" "ADE5"
				(at 34.29 -94.92 0)
			)
			(property "Datasheet" "https://www.minicircuits.com/pdfs/ADE-5+.pdf"
				(at 34.29 -194.92 0)
			)
			(property "Description" "RF Mixer DBL BAL MIX / SURF MT /   RoHS"
				(at 0 0 0)
			)
			(property "Height" "2.84"
				(at 34.29 -394.92 0)
			)
			(property "Mouser Part Number" "139-ADE-5"
				(at 34.29 -494.92 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ADE-5%2b?qs=xZ%2FP%252Ba9zWqYmwk%2F%2Fds48gw%3D%3D"
				(at 34.29 -594.92 0)
			)
			(property "Manufacturer_Name" "Mini-Circuits"
				(at 34.29 -694.92 0)
			)
			(property "Manufacturer_Part_Number" "ADE-5+"
				(at 34.29 -794.92 0)
			)
			(symbol "ADE-5+_1_1"
				(rectangle
					(start 5.08 2.54)
					(end 33.02 -7.62)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "GROUND_1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "IF")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RF")
					(number "3")
				)
				(pin passive line
					(at 38.1 0 180)
					(length 5.08)
					(name "LO")
					(number "6")
				)
				(pin passive line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "GROUND_3")
					(number "5")
				)
				(pin passive line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "GROUND_2")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:L"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -1.27 0 90)
			)
			(property "Value" "L"
				(at 1.905 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_0_1"
				(arc
					(start 0 2.54)
					(mid 0.6323 1.905)
					(end 0 1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.27)
					(mid 0.6323 0.635)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.6323 -0.635)
					(end 0 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.27)
					(mid 0.6323 -1.905)
					(end 0 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "ERA-1SM+:ERA-1SM+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.366 13.97 0)
			)
			(property "Value" "ERA-1SM+"
				(at 7.366 11.43 0)
			)
			(property "Footprint" "ERA1SM"
				(at 26.67 -66.98 0)
			)
			(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
				(at 26.67 -166.98 0)
			)
			(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
				(at 0 0 0)
			)
			(property "Height" "1.52"
				(at 26.67 -366.98 0)
			)
			(property "Mouser Part Number" "139-ERA-1SM"
				(at 26.67 -466.98 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
				(at 26.67 -566.98 0)
			)
			(property "Manufacturer_Name" "Mini-Circuits"
				(at 26.67 -666.98 0)
			)
			(property "Manufacturer_Part_Number" "ERA-1SM+"
				(at 26.67 -766.98 0)
			)
			(symbol "ERA-1SM+_1_1"
				(rectangle
					(start -6.35 20.32)
					(end 3.81 -11.43)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 25.4 270)
					(length 5.08)
					(name "RF_-_OUT_AND_DC_-_IN")
					(number "3")
				)
				(pin passive line
					(at -3.81 -16.51 90)
					(length 5.08)
					(name "RF_IN")
					(number "1")
				)
				(pin passive line
					(at 1.27 25.4 270)
					(length 5.08)
					(name "GND_1")
					(number "2")
				)
				(pin passive line
					(at 1.27 -16.51 90)
					(length 5.08)
					(name "GND_2")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 190.5 59.69)
		(end 223.52 85.09)
		(fill
			(type none)
		)
	)
	(text "75MHz LPF"
		(exclude_from_sim no)
		(at 204.47 83.312 0)
	)
	(text "-3dB\n"
		(exclude_from_sim no)
		(at 106.426 81.28 0)
	)
	(text "-3dB\n"
		(exclude_from_sim no)
		(at 199.136 95.25 0)
	)
	(text "-1dB\n"
		(exclude_from_sim no)
		(at 84.582 58.42 0)
	)
	(text "-1dB\n"
		(exclude_from_sim no)
		(at 176.022 64.77 0)
	)
	(junction
		(at 187.96 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 214.63 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 200.66 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 171.45 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 67.31 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 194.31 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 105.41 83.82) (xy 107.95 83.82)
		)
	)
	(wire
		(pts
			(xy 125.73 97.79) (xy 127 97.79)
		)
	)
	(wire
		(pts
			(xy 97.79 69.85) (xy 97.79 78.74)
		)
	)
	(wire
		(pts
			(xy 146.05 67.31) (xy 158.75 67.31)
		)
	)
	(wire
		(pts
			(xy 146.05 54.61) (xy 88.9 54.61)
		)
	)
	(wire
		(pts
			(xy 163.83 78.74) (xy 158.75 78.74)
		)
	)
	(wire
		(pts
			(xy 198.12 97.79) (xy 200.66 97.79)
		)
	)
	(wire
		(pts
			(xy 107.95 83.82) (xy 107.95 86.36)
		)
	)
	(wire
		(pts
			(xy 67.31 60.96) (xy 69.85 60.96)
		)
	)
	(wire
		(pts
			(xy 181.61 97.79) (xy 187.96 97.79)
		)
	)
	(wire
		(pts
			(xy 149.86 72.39) (xy 149.86 69.85)
		)
	)
	(wire
		(pts
			(xy 187.96 107.95) (xy 187.96 110.49)
		)
	)
	(wire
		(pts
			(xy 80.01 71.12) (xy 80.01 73.66)
		)
	)
	(wire
		(pts
			(xy 129.54 125.73) (xy 125.73 125.73)
		)
	)
	(wire
		(pts
			(xy 187.96 97.79) (xy 190.5 97.79)
		)
	)
	(wire
		(pts
			(xy 168.91 86.36) (xy 163.83 86.36)
		)
	)
	(wire
		(pts
			(xy 146.05 64.77) (xy 146.05 54.61)
		)
	)
	(wire
		(pts
			(xy 200.66 97.79) (xy 215.9 97.79)
		)
	)
	(wire
		(pts
			(xy 67.31 63.5) (xy 67.31 60.96)
		)
	)
	(wire
		(pts
			(xy 209.55 67.31) (xy 214.63 67.31)
		)
	)
	(wire
		(pts
			(xy 125.73 109.22) (xy 125.73 115.57)
		)
	)
	(wire
		(pts
			(xy 158.75 69.85) (xy 158.75 67.31)
		)
	)
	(wire
		(pts
			(xy 95.25 78.74) (xy 95.25 83.82)
		)
	)
	(wire
		(pts
			(xy 95.25 93.98) (xy 95.25 96.52)
		)
	)
	(wire
		(pts
			(xy 171.45 67.31) (xy 194.31 67.31)
		)
	)
	(wire
		(pts
			(xy 200.66 107.95) (xy 200.66 110.49)
		)
	)
	(wire
		(pts
			(xy 95.25 83.82) (xy 97.79 83.82)
		)
	)
	(wire
		(pts
			(xy 107.95 64.77) (xy 107.95 67.31)
		)
	)
	(wire
		(pts
			(xy 168.91 67.31) (xy 171.45 67.31)
		)
	)
	(wire
		(pts
			(xy 125.73 97.79) (xy 125.73 101.6)
		)
	)
	(wire
		(pts
			(xy 125.73 109.22) (xy 137.16 109.22)
		)
	)
	(wire
		(pts
			(xy 116.84 97.79) (xy 116.84 83.82)
		)
	)
	(wire
		(pts
			(xy 171.45 77.47) (xy 171.45 80.01)
		)
	)
	(wire
		(pts
			(xy 200.66 97.79) (xy 200.66 100.33)
		)
	)
	(wire
		(pts
			(xy 194.31 67.31) (xy 201.93 67.31)
		)
	)
	(wire
		(pts
			(xy 187.96 100.33) (xy 187.96 97.79)
		)
	)
	(wire
		(pts
			(xy 116.84 83.82) (xy 107.95 83.82)
		)
	)
	(wire
		(pts
			(xy 77.47 60.96) (xy 80.01 60.96)
		)
	)
	(wire
		(pts
			(xy 95.25 86.36) (xy 95.25 83.82)
		)
	)
	(wire
		(pts
			(xy 107.95 93.98) (xy 107.95 96.52)
		)
	)
	(wire
		(pts
			(xy 88.9 60.96) (xy 80.01 60.96)
		)
	)
	(wire
		(pts
			(xy 168.91 92.71) (xy 168.91 86.36)
		)
	)
	(wire
		(pts
			(xy 171.45 67.31) (xy 171.45 69.85)
		)
	)
	(wire
		(pts
			(xy 214.63 67.31) (xy 238.76 67.31)
		)
	)
	(wire
		(pts
			(xy 149.86 69.85) (xy 146.05 69.85)
		)
	)
	(wire
		(pts
			(xy 67.31 71.12) (xy 67.31 73.66)
		)
	)
	(wire
		(pts
			(xy 163.83 86.36) (xy 163.83 78.74)
		)
	)
	(wire
		(pts
			(xy 88.9 54.61) (xy 88.9 60.96)
		)
	)
	(wire
		(pts
			(xy 80.01 60.96) (xy 80.01 63.5)
		)
	)
	(wire
		(pts
			(xy 214.63 74.93) (xy 214.63 77.47)
		)
	)
	(wire
		(pts
			(xy 93.98 67.31) (xy 107.95 67.31)
		)
	)
	(wire
		(pts
			(xy 137.16 116.84) (xy 137.16 119.38)
		)
	)
	(wire
		(pts
			(xy 158.75 67.31) (xy 161.29 67.31)
		)
	)
	(wire
		(pts
			(xy 124.46 97.79) (xy 125.73 97.79)
		)
	)
	(wire
		(pts
			(xy 127 83.82) (xy 130.81 83.82)
		)
	)
	(wire
		(pts
			(xy 168.91 97.79) (xy 173.99 97.79)
		)
	)
	(wire
		(pts
			(xy 194.31 74.93) (xy 194.31 77.47)
		)
	)
	(wire
		(pts
			(xy 125.73 125.73) (xy 125.73 123.19)
		)
	)
	(wire
		(pts
			(xy 158.75 78.74) (xy 158.75 80.01)
		)
	)
	(wire
		(pts
			(xy 59.69 60.96) (xy 67.31 60.96)
		)
	)
	(wire
		(pts
			(xy 158.75 77.47) (xy 158.75 78.74)
		)
	)
	(wire
		(pts
			(xy 107.95 69.85) (xy 97.79 69.85)
		)
	)
	(wire
		(pts
			(xy 97.79 78.74) (xy 95.25 78.74)
		)
	)
	(wire
		(pts
			(xy 127 92.71) (xy 127 83.82)
		)
	)
	(hierarchical_label "9V"
		(shape input)
		(at 129.54 125.73 0)
	)
	(hierarchical_label "mix_IF"
		(shape input)
		(at 238.76 67.31 0)
	)
	(hierarchical_label "mix_LO"
		(shape input)
		(at 215.9 97.79 0)
	)
	(hierarchical_label "mix_RF"
		(shape input)
		(at 59.69 60.96 180)
	)
	(symbol
		(lib_id "Device:R")
		(at 194.31 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R30"
			(at 194.31 91.44 90)
		)
		(property "Value" "18"
			(at 194.31 93.98 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 194.31 99.568 90)
		)
		(property "Datasheet" "~"
			(at 194.31 97.79 0)
		)
		(property "Description" "Resistor"
			(at 194.31 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R30")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 214.63 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C35"
			(at 218.44 69.8499 0)
		)
		(property "Value" "51p"
			(at 218.44 72.3899 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 215.5952 74.93 0)
		)
		(property "Datasheet" "~"
			(at 214.63 71.12 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 214.63 71.12 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C35")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 158.75 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R23"
			(at 161.29 72.3899 0)
		)
		(property "Value" "820"
			(at 161.29 74.9299 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 156.972 73.66 90)
		)
		(property "Datasheet" "~"
			(at 158.75 73.66 0)
		)
		(property "Description" "Resistor"
			(at 158.75 73.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R23")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 214.63 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR053"
			(at 214.63 83.82 0)
		)
		(property "Value" "GND"
			(at 214.63 81.788 0)
		)
		(property "Footprint" ""
			(at 214.63 77.47 0)
		)
		(property "Datasheet" ""
			(at 214.63 77.47 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 214.63 77.47 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR053")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 177.8 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C32"
			(at 177.8 90.17 90)
		)
		(property "Value" "10n"
			(at 177.8 92.71 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 181.61 96.8248 0)
		)
		(property "Datasheet" "~"
			(at 177.8 97.79 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 177.8 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C32")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 187.96 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R29"
			(at 190.5 102.8699 0)
		)
		(property "Value" "300"
			(at 190.5 105.4099 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 186.182 104.14 90)
		)
		(property "Datasheet" "~"
			(at 187.96 104.14 0)
		)
		(property "Description" "Resistor"
			(at 187.96 104.14 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R29")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 107.95 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R28"
			(at 110.49 88.8999 0)
		)
		(property "Value" "300"
			(at 110.49 91.4399 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 106.172 90.17 90)
		)
		(property "Datasheet" "~"
			(at 107.95 90.17 0)
		)
		(property "Description" "Resistor"
			(at 107.95 90.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R28")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 67.31 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R20"
			(at 69.85 66.0399 0)
		)
		(property "Value" "820"
			(at 69.85 68.5799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 65.532 67.31 90)
		)
		(property "Datasheet" "~"
			(at 67.31 67.31 0)
		)
		(property "Description" "Resistor"
			(at 67.31 67.31 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 194.31 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C34"
			(at 198.12 69.8499 0)
		)
		(property "Value" "51p"
			(at 198.12 72.3899 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 195.2752 74.93 0)
		)
		(property "Datasheet" "~"
			(at 194.31 71.12 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 194.31 71.12 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C34")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 95.25 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR047"
			(at 95.25 102.87 0)
		)
		(property "Value" "GND"
			(at 95.25 100.584 0)
		)
		(property "Footprint" ""
			(at 95.25 96.52 0)
		)
		(property "Datasheet" ""
			(at 95.25 96.52 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 95.25 96.52 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR047")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 205.74 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L12"
			(at 205.74 62.23 90)
		)
		(property "Value" "150nH"
			(at 205.74 64.77 90)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 205.74 67.31 0)
		)
		(property "Datasheet" "~"
			(at 205.74 67.31 0)
		)
		(property "Description" "Inductor"
			(at 205.74 67.31 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 93.98 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR046"
			(at 93.98 73.66 0)
		)
		(property "Value" "GND"
			(at 93.98 71.374 0)
		)
		(property "Footprint" ""
			(at 93.98 67.31 0)
		)
		(property "Datasheet" ""
			(at 93.98 67.31 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 93.98 67.31 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR046")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 95.25 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R26"
			(at 97.79 88.8999 0)
		)
		(property "Value" "300"
			(at 97.79 91.4399 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 93.472 90.17 90)
		)
		(property "Datasheet" "~"
			(at 95.25 90.17 0)
		)
		(property "Description" "Resistor"
			(at 95.25 90.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R26")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 67.31 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR041"
			(at 67.31 80.01 0)
		)
		(property "Value" "GND"
			(at 67.31 77.724 0)
		)
		(property "Footprint" ""
			(at 67.31 73.66 0)
		)
		(property "Datasheet" ""
			(at 67.31 73.66 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 67.31 73.66 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR041")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 130.81 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR049"
			(at 130.81 90.17 0)
		)
		(property "Value" "GND"
			(at 130.81 87.884 0)
		)
		(property "Footprint" ""
			(at 130.81 83.82 0)
		)
		(property "Datasheet" ""
			(at 130.81 83.82 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 130.81 83.82 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR049")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 101.6 83.82 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R27"
			(at 101.6 77.47 90)
		)
		(property "Value" "18"
			(at 101.6 80.01 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 101.6 85.598 90)
		)
		(property "Datasheet" "~"
			(at 101.6 83.82 0)
		)
		(property "Description" "Resistor"
			(at 101.6 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R27")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 165.1 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R24"
			(at 165.1 60.96 90)
		)
		(property "Value" "5,6"
			(at 165.1 63.5 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 165.1 69.088 90)
		)
		(property "Datasheet" "~"
			(at 165.1 67.31 0)
		)
		(property "Description" "Resistor"
			(at 165.1 67.31 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 171.45 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR044"
			(at 171.45 86.36 0)
		)
		(property "Value" "GND"
			(at 171.45 84.074 0)
		)
		(property "Footprint" ""
			(at 171.45 80.01 0)
		)
		(property "Datasheet" ""
			(at 171.45 80.01 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 171.45 80.01 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR044")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 120.65 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C31"
			(at 120.65 90.17 90)
		)
		(property "Value" "10n"
			(at 120.65 92.71 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 124.46 96.8248 0)
		)
		(property "Datasheet" "~"
			(at 120.65 97.79 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 120.65 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C31")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR042"
			(at 80.01 80.01 0)
		)
		(property "Value" "GND"
			(at 80.01 77.724 0)
		)
		(property "Footprint" ""
			(at 80.01 73.66 0)
		)
		(property "Datasheet" ""
			(at 80.01 73.66 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 80.01 73.66 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR042")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 200.66 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR051"
			(at 200.66 116.84 0)
		)
		(property "Value" "GND"
			(at 200.66 114.554 0)
		)
		(property "Footprint" ""
			(at 200.66 110.49 0)
		)
		(property "Datasheet" ""
			(at 200.66 110.49 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 200.66 110.49 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR051")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "ERA-1SM+:ERA-1SM+")
		(at 152.4 93.98 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC10"
			(at 147.955 85.09 90)
		)
		(property "Value" "ERA-1SM+"
			(at 147.955 87.63 90)
		)
		(property "Footprint" "ERA1SM"
			(at 219.38 67.31 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
			(at 319.38 67.31 0)
		)
		(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
			(at 152.4 93.98 0)
		)
		(property "Height" "1.52"
			(at 519.38 67.31 0)
		)
		(property "Mouser Part Number" "139-ERA-1SM"
			(at 619.38 67.31 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
			(at 719.38 67.31 0)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at 819.38 67.31 0)
		)
		(property "Manufacturer_Part_Number" "ERA-1SM+"
			(at 919.38 67.31 0)
		)
		(pin "4")
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR048"
			(at 107.95 102.87 0)
		)
		(property "Value" "GND"
			(at 107.95 100.584 0)
		)
		(property "Footprint" ""
			(at 107.95 96.52 0)
		)
		(property "Datasheet" ""
			(at 107.95 96.52 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 107.95 96.52 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR048")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 137.16 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR055"
			(at 137.16 125.73 0)
		)
		(property "Value" "GND"
			(at 137.16 123.444 0)
		)
		(property "Footprint" ""
			(at 137.16 119.38 0)
		)
		(property "Datasheet" ""
			(at 137.16 119.38 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 137.16 119.38 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR055")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 194.31 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR052"
			(at 194.31 83.82 0)
		)
		(property "Value" "GND"
			(at 194.31 81.788 0)
		)
		(property "Footprint" ""
			(at 194.31 77.47 0)
		)
		(property "Datasheet" ""
			(at 194.31 77.47 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 194.31 77.47 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR052")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 200.66 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R31"
			(at 203.2 102.8699 0)
		)
		(property "Value" "300"
			(at 203.2 105.4099 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 198.882 104.14 90)
		)
		(property "Datasheet" "~"
			(at 200.66 104.14 0)
		)
		(property "Description" "Resistor"
			(at 200.66 104.14 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R31")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 137.16 113.03 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C33"
			(at 140.97 111.7599 0)
		)
		(property "Value" "10n"
			(at 140.97 114.2999 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 136.1948 109.22 0)
		)
		(property "Datasheet" "~"
			(at 137.16 113.03 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 137.16 113.03 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C33")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 125.73 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L11"
			(at 127 104.1399 0)
		)
		(property "Value" "470N"
			(at 127 106.6799 0)
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder"
			(at 125.73 105.41 0)
		)
		(property "Datasheet" "~"
			(at 125.73 105.41 0)
		)
		(property "Description" "Inductor"
			(at 125.73 105.41 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 171.45 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R25"
			(at 173.99 72.3899 0)
		)
		(property "Value" "820"
			(at 173.99 74.9299 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 169.672 73.66 90)
		)
		(property "Datasheet" "~"
			(at 171.45 73.66 0)
		)
		(property "Description" "Resistor"
			(at 171.45 73.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R25")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "ADE-5+:ADE-5+")
		(at 146.05 69.85 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC9"
			(at 127 57.15 0)
		)
		(property "Value" "ADE-5+"
			(at 127 59.69 0)
		)
		(property "Footprint" "ADE5"
			(at 111.76 -25.07 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/ADE-5+.pdf"
			(at 111.76 -125.07 0)
		)
		(property "Description" "RF Mixer DBL BAL MIX / SURF MT /   RoHS"
			(at 146.05 69.85 0)
		)
		(property "Height" "2.84"
			(at 111.76 -325.07 0)
		)
		(property "Mouser Part Number" "139-ADE-5"
			(at 111.76 -425.07 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ADE-5%2b?qs=xZ%2FP%252Ba9zWqYmwk%2F%2Fds48gw%3D%3D"
			(at 111.76 -525.07 0)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at 111.76 -625.07 0)
		)
		(property "Manufacturer_Part_Number" "ADE-5+"
			(at 111.76 -725.07 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "6")
		(pin "3")
		(pin "5")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 149.86 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR045"
			(at 149.86 78.74 0)
		)
		(property "Value" "GND"
			(at 149.86 76.454 0)
		)
		(property "Footprint" ""
			(at 149.86 72.39 0)
		)
		(property "Datasheet" ""
			(at 149.86 72.39 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 149.86 72.39 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR045")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 73.66 60.96 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R21"
			(at 73.66 54.61 90)
		)
		(property "Value" "5,6"
			(at 73.66 57.15 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 73.66 62.738 90)
		)
		(property "Datasheet" "~"
			(at 73.66 60.96 0)
		)
		(property "Description" "Resistor"
			(at 73.66 60.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 125.73 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R32"
			(at 128.27 118.1099 0)
		)
		(property "Value" "R"
			(at 128.27 120.6499 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 123.952 119.38 90)
		)
		(property "Datasheet" "~"
			(at 125.73 119.38 0)
		)
		(property "Description" "Resistor"
			(at 125.73 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R32")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 80.01 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R22"
			(at 82.55 66.0399 0)
		)
		(property "Value" "820"
			(at 82.55 68.5799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 78.232 67.31 90)
		)
		(property "Datasheet" "~"
			(at 80.01 67.31 0)
		)
		(property "Description" "Resistor"
			(at 80.01 67.31 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 187.96 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR050"
			(at 187.96 116.84 0)
		)
		(property "Value" "GND"
			(at 187.96 114.554 0)
		)
		(property "Footprint" ""
			(at 187.96 110.49 0)
		)
		(property "Datasheet" ""
			(at 187.96 110.49 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 187.96 110.49 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR050")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 158.75 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR043"
			(at 158.75 86.36 0)
		)
		(property "Value" "GND"
			(at 158.75 84.074 0)
		)
		(property "Footprint" ""
			(at 158.75 80.01 0)
		)
		(property "Datasheet" ""
			(at 158.75 80.01 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 158.75 80.01 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR043")
					(unit 1)
				)
			)
		)
	)
)
