(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "4259-63:4259-63"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 34.29 7.62 0)
			)
			(property "Value" "4259-63"
				(at 34.29 5.08 0)
			)
			(property "Footprint" "SOT65P210X110-6N"
				(at 34.29 -94.92 0)
			)
			(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe4259ds.pdf"
				(at 34.29 -194.92 0)
			)
			(property "Description" "RF switch IC"
				(at 0 0 0)
			)
			(property "Height" "1.1"
				(at 34.29 -394.92 0)
			)
			(property "Mouser Part Number" "81-4259-63"
				(at 34.29 -494.92 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/pSemi/4259-63?qs=iw0hurA%2FaD37qvQcKdATTw%3D%3D"
				(at 34.29 -594.92 0)
			)
			(property "Manufacturer_Name" "Peregrine Semiconductor"
				(at 34.29 -694.92 0)
			)
			(property "Manufacturer_Part_Number" "4259-63"
				(at 34.29 -794.92 0)
			)
			(symbol "4259-63_1_1"
				(rectangle
					(start 5.08 2.54)
					(end 33.02 -7.62)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RF1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RF2")
					(number "3")
				)
				(pin passive line
					(at 38.1 0 180)
					(length 5.08)
					(name "~{CTRL_OR_VDD}")
					(number "6")
				)
				(pin passive line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "RFC")
					(number "5")
				)
				(pin passive line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "CTRL")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "74xGxx:74LVC1GU04DRL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 10.16 0)
			)
			(property "Value" "74LVC1GU04DRL"
				(at 17.78 10.16 0)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
				(at 0 -12.7 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1gu04.pdf"
				(at -3.81 0 0)
			)
			(property "Description" "Single Inverter Gate, SOT-553"
				(at 0 0 0)
			)
			(property "ki_keywords" "inverter cmos"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOT*553*"
				(at 0 0 0)
			)
			(symbol "74LVC1GU04DRL_0_1"
				(rectangle
					(start -5.08 7.62)
					(end -5.08 -7.62)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -5.08 -7.62) (xy 10.16 0) (xy -5.08 7.62)
					)
					(fill
						(type background)
					)
				)
				(circle
					(center 11.43 0)
					(radius 1.27)
					(fill
						(type none)
					)
				)
			)
			(symbol "74LVC1GU04DRL_1_1"
				(pin input line
					(at -10.16 0 0)
					(length 5.08)
					(name "~")
					(number "2")
				)
				(pin power_in line
					(at 0 10.16 270)
					(length 5.08)
					(name "VCC")
					(number "5")
				)
				(pin power_in line
					(at 0 -10.16 90)
					(length 5.08)
					(name "GND")
					(number "3")
				)
				(pin no_connect line
					(at 10.16 0 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin output line
					(at 17.78 0 180)
					(length 5.08)
					(name "~")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:L"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -1.27 0 90)
			)
			(property "Value" "L"
				(at 1.905 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_0_1"
				(arc
					(start 0 2.54)
					(mid 0.6323 1.905)
					(end 0 1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.27)
					(mid 0.6323 0.635)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.6323 -0.635)
					(end 0 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.27)
					(mid 0.6323 -1.905)
					(end 0 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "ERA-1SM+:ERA-1SM+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.366 13.97 0)
			)
			(property "Value" "ERA-1SM+"
				(at 7.366 11.43 0)
			)
			(property "Footprint" "ERA1SM"
				(at 26.67 -66.98 0)
			)
			(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
				(at 26.67 -166.98 0)
			)
			(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
				(at 0 0 0)
			)
			(property "Height" "1.52"
				(at 26.67 -366.98 0)
			)
			(property "Mouser Part Number" "139-ERA-1SM"
				(at 26.67 -466.98 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
				(at 26.67 -566.98 0)
			)
			(property "Manufacturer_Name" "Mini-Circuits"
				(at 26.67 -666.98 0)
			)
			(property "Manufacturer_Part_Number" "ERA-1SM+"
				(at 26.67 -766.98 0)
			)
			(symbol "ERA-1SM+_1_1"
				(rectangle
					(start -6.35 20.32)
					(end 3.81 -11.43)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 25.4 270)
					(length 5.08)
					(name "RF_-_OUT_AND_DC_-_IN")
					(number "3")
				)
				(pin passive line
					(at -3.81 -16.51 90)
					(length 5.08)
					(name "RF_IN")
					(number "1")
				)
				(pin passive line
					(at 1.27 25.4 270)
					(length 5.08)
					(name "GND_1")
					(number "2")
				)
				(pin passive line
					(at 1.27 -16.51 90)
					(length 5.08)
					(name "GND_2")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "PHA-101+:PHA-101+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 39.37 7.62 0)
			)
			(property "Value" "PHA-101+"
				(at 39.37 5.08 0)
			)
			(property "Footprint" "GALI19"
				(at 39.37 -94.92 0)
			)
			(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/PHA-101+.pdf"
				(at 39.37 -194.92 0)
			)
			(property "Description" "RF Amplifier MMIC AMPLIFIER"
				(at 0 0 0)
			)
			(property "Height" "1.6"
				(at 39.37 -394.92 0)
			)
			(property "Mouser Part Number" "139-PHA-101"
				(at 39.37 -494.92 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/PHA-101%2b?qs=xZ%2FP%252Ba9zWqbA11kwlpohzA%3D%3D"
				(at 39.37 -594.92 0)
			)
			(property "Manufacturer_Name" "Mini-Circuits"
				(at 39.37 -694.92 0)
			)
			(property "Manufacturer_Part_Number" "PHA-101+"
				(at 39.37 -794.92 0)
			)
			(symbol "PHA-101+_1_1"
				(rectangle
					(start 5.08 2.54)
					(end 38.1 -5.08)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RF-IN")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GND_1")
					(number "2")
				)
				(pin passive line
					(at 43.18 0 180)
					(length 5.08)
					(name "RF-OUT_&_DC-IN")
					(number "3")
				)
				(pin passive line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "GND_2")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "RF_Amplifier:PGA-103"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -1.27 7.62 0)
			)
			(property "Value" "PGA-103"
				(at 2.54 5.08 0)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
				(at 1.27 10.16 0)
			)
			(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-103+.pdf"
				(at 0 0 0)
			)
			(property "Description" "50-4000MHz +11dB Low Noise Amplifier, SOT-89"
				(at 0 0 0)
			)
			(property "ki_keywords" "RF amplifier"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOT?89*"
				(at 0 0 0)
			)
			(symbol "PGA-103_0_1"
				(polyline
					(pts
						(xy 5.08 0) (xy -5.08 5.08) (xy -5.08 -5.08) (xy 5.08 0)
					)
					(fill
						(type background)
					)
				)
			)
			(symbol "PGA-103_1_1"
				(pin input line
					(at -7.62 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin power_in line
					(at -2.54 -7.62 90)
					(length 3.81)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "~")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 50.8 27.94)
		(end 82.55 55.88)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 217.17 133.35)
		(end 247.65 156.21)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 129.54 71.12)
		(end 162.56 96.52)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 165.1 27.94)
		(end 196.85 55.88)
		(fill
			(type none)
		)
	)
	(text "75MHz LPF"
		(exclude_from_sim no)
		(at 231.648 154.686 0)
	)
	(text "75MHz LPF"
		(exclude_from_sim no)
		(at 152.4 94.742 0)
	)
	(text "-3dB"
		(exclude_from_sim no)
		(at 66.294 23.876 0)
	)
	(junction
		(at 173.99 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 241.3 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 265.43 20.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 203.2 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 153.67 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 26.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 276.86 27.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 220.98 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 20.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 267.97 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 17.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 135.89 78.74) (xy 142.24 78.74)
		)
	)
	(wire
		(pts
			(xy 91.44 138.43) (xy 111.76 138.43)
		)
	)
	(wire
		(pts
			(xy 276.86 27.94) (xy 276.86 31.75)
		)
	)
	(wire
		(pts
			(xy 231.14 17.78) (xy 252.73 17.78)
		)
	)
	(wire
		(pts
			(xy 148.59 35.56) (xy 154.94 35.56)
		)
	)
	(wire
		(pts
			(xy 73.66 45.72) (xy 73.66 48.26)
		)
	)
	(wire
		(pts
			(xy 226.06 78.74) (xy 228.6 78.74)
		)
	)
	(wire
		(pts
			(xy 170.18 45.72) (xy 170.18 48.26)
		)
	)
	(wire
		(pts
			(xy 149.86 78.74) (xy 153.67 78.74)
		)
	)
	(wire
		(pts
			(xy 162.56 35.56) (xy 170.18 35.56)
		)
	)
	(wire
		(pts
			(xy 63.5 78.74) (xy 63.5 120.65)
		)
	)
	(wire
		(pts
			(xy 33.02 35.56) (xy 33.02 125.73)
		)
	)
	(wire
		(pts
			(xy 86.36 138.43) (xy 91.44 138.43)
		)
	)
	(wire
		(pts
			(xy 256.54 119.38) (xy 248.92 119.38)
		)
	)
	(wire
		(pts
			(xy 167.64 78.74) (xy 173.99 78.74)
		)
	)
	(wire
		(pts
			(xy 265.43 27.94) (xy 276.86 27.94)
		)
	)
	(wire
		(pts
			(xy 252.73 20.32) (xy 265.43 20.32)
		)
	)
	(wire
		(pts
			(xy 170.18 38.1) (xy 170.18 35.56)
		)
	)
	(wire
		(pts
			(xy 125.73 17.78) (xy 135.89 17.78)
		)
	)
	(wire
		(pts
			(xy 274.32 124.46) (xy 274.32 127)
		)
	)
	(wire
		(pts
			(xy 156.21 60.96) (xy 158.75 60.96)
		)
	)
	(wire
		(pts
			(xy 207.01 116.84) (xy 210.82 116.84)
		)
	)
	(wire
		(pts
			(xy 187.96 35.56) (xy 182.88 35.56)
		)
	)
	(wire
		(pts
			(xy 49.53 142.24) (xy 49.53 143.51)
		)
	)
	(wire
		(pts
			(xy 73.66 38.1) (xy 73.66 35.56)
		)
	)
	(wire
		(pts
			(xy 153.67 86.36) (xy 153.67 88.9)
		)
	)
	(wire
		(pts
			(xy 252.73 17.78) (xy 252.73 20.32)
		)
	)
	(wire
		(pts
			(xy 210.82 121.92) (xy 203.2 121.92)
		)
	)
	(wire
		(pts
			(xy 59.69 119.38) (xy 59.69 123.19)
		)
	)
	(wire
		(pts
			(xy 220.98 147.32) (xy 220.98 149.86)
		)
	)
	(wire
		(pts
			(xy 252.73 35.56) (xy 255.27 35.56)
		)
	)
	(wire
		(pts
			(xy 236.22 139.7) (xy 241.3 139.7)
		)
	)
	(wire
		(pts
			(xy 167.64 20.32) (xy 167.64 17.78)
		)
	)
	(wire
		(pts
			(xy 173.99 74.93) (xy 173.99 78.74)
		)
	)
	(wire
		(pts
			(xy 220.98 139.7) (xy 220.98 128.27)
		)
	)
	(wire
		(pts
			(xy 248.92 121.92) (xy 267.97 121.92)
		)
	)
	(wire
		(pts
			(xy 207.01 102.87) (xy 207.01 116.84)
		)
	)
	(wire
		(pts
			(xy 205.74 35.56) (xy 208.28 35.56)
		)
	)
	(wire
		(pts
			(xy 144.78 60.96) (xy 148.59 60.96)
		)
	)
	(wire
		(pts
			(xy 45.72 142.24) (xy 49.53 142.24)
		)
	)
	(wire
		(pts
			(xy 254 38.1) (xy 251.46 38.1)
		)
	)
	(wire
		(pts
			(xy 67.31 151.13) (xy 78.74 151.13)
		)
	)
	(wire
		(pts
			(xy 254 40.64) (xy 254 38.1)
		)
	)
	(wire
		(pts
			(xy 214.63 78.74) (xy 218.44 78.74)
		)
	)
	(wire
		(pts
			(xy 33.02 125.73) (xy 73.66 125.73)
		)
	)
	(wire
		(pts
			(xy 241.3 81.28) (xy 241.3 78.74)
		)
	)
	(wire
		(pts
			(xy 256.54 139.7) (xy 261.62 139.7)
		)
	)
	(wire
		(pts
			(xy 200.66 78.74) (xy 203.2 78.74)
		)
	)
	(wire
		(pts
			(xy 252.73 24.13) (xy 252.73 20.32)
		)
	)
	(wire
		(pts
			(xy 241.3 147.32) (xy 241.3 149.86)
		)
	)
	(wire
		(pts
			(xy 111.76 120.65) (xy 115.57 120.65)
		)
	)
	(wire
		(pts
			(xy 252.73 31.75) (xy 252.73 35.56)
		)
	)
	(wire
		(pts
			(xy 167.64 17.78) (xy 162.56 17.78)
		)
	)
	(wire
		(pts
			(xy 55.88 45.72) (xy 55.88 48.26)
		)
	)
	(wire
		(pts
			(xy 170.18 35.56) (xy 175.26 35.56)
		)
	)
	(wire
		(pts
			(xy 187.96 45.72) (xy 187.96 48.26)
		)
	)
	(wire
		(pts
			(xy 139.7 40.64) (xy 139.7 43.18)
		)
	)
	(wire
		(pts
			(xy 135.89 17.78) (xy 148.59 17.78)
		)
	)
	(wire
		(pts
			(xy 267.97 121.92) (xy 267.97 116.84)
		)
	)
	(wire
		(pts
			(xy 73.66 35.56) (xy 68.58 35.56)
		)
	)
	(wire
		(pts
			(xy 153.67 78.74) (xy 160.02 78.74)
		)
	)
	(wire
		(pts
			(xy 203.2 78.74) (xy 207.01 78.74)
		)
	)
	(wire
		(pts
			(xy 220.98 139.7) (xy 228.6 139.7)
		)
	)
	(wire
		(pts
			(xy 148.59 26.67) (xy 154.94 26.67)
		)
	)
	(wire
		(pts
			(xy 187.96 38.1) (xy 187.96 35.56)
		)
	)
	(wire
		(pts
			(xy 173.99 78.74) (xy 175.26 78.74)
		)
	)
	(wire
		(pts
			(xy 267.97 116.84) (xy 274.32 116.84)
		)
	)
	(wire
		(pts
			(xy 154.94 17.78) (xy 154.94 26.67)
		)
	)
	(wire
		(pts
			(xy 185.42 66.04) (xy 185.42 71.12)
		)
	)
	(wire
		(pts
			(xy 198.12 119.38) (xy 210.82 119.38)
		)
	)
	(wire
		(pts
			(xy 241.3 78.74) (xy 236.22 78.74)
		)
	)
	(wire
		(pts
			(xy 267.97 109.22) (xy 274.32 109.22)
		)
	)
	(wire
		(pts
			(xy 67.31 153.67) (xy 67.31 151.13)
		)
	)
	(wire
		(pts
			(xy 55.88 35.56) (xy 60.96 35.56)
		)
	)
	(wire
		(pts
			(xy 91.44 146.05) (xy 91.44 148.59)
		)
	)
	(wire
		(pts
			(xy 73.66 35.56) (xy 83.82 35.56)
		)
	)
	(wire
		(pts
			(xy 208.28 38.1) (xy 208.28 41.91)
		)
	)
	(wire
		(pts
			(xy 33.02 35.56) (xy 55.88 35.56)
		)
	)
	(wire
		(pts
			(xy 91.44 35.56) (xy 97.79 35.56)
		)
	)
	(wire
		(pts
			(xy 190.5 78.74) (xy 193.04 78.74)
		)
	)
	(wire
		(pts
			(xy 252.73 35.56) (xy 251.46 35.56)
		)
	)
	(wire
		(pts
			(xy 173.99 67.31) (xy 173.99 60.96)
		)
	)
	(wire
		(pts
			(xy 86.36 151.13) (xy 86.36 138.43)
		)
	)
	(wire
		(pts
			(xy 59.69 123.19) (xy 73.66 123.19)
		)
	)
	(wire
		(pts
			(xy 262.89 35.56) (xy 262.89 102.87)
		)
	)
	(wire
		(pts
			(xy 63.5 78.74) (xy 135.89 78.74)
		)
	)
	(wire
		(pts
			(xy 190.5 66.04) (xy 185.42 66.04)
		)
	)
	(wire
		(pts
			(xy 248.92 116.84) (xy 252.73 116.84)
		)
	)
	(wire
		(pts
			(xy 203.2 121.92) (xy 203.2 78.74)
		)
	)
	(wire
		(pts
			(xy 220.98 128.27) (xy 256.54 128.27)
		)
	)
	(wire
		(pts
			(xy 134.62 68.58) (xy 158.75 68.58)
		)
	)
	(wire
		(pts
			(xy 135.89 86.36) (xy 135.89 88.9)
		)
	)
	(wire
		(pts
			(xy 241.3 139.7) (xy 248.92 139.7)
		)
	)
	(wire
		(pts
			(xy 256.54 128.27) (xy 256.54 119.38)
		)
	)
	(wire
		(pts
			(xy 111.76 138.43) (xy 111.76 125.73)
		)
	)
	(wire
		(pts
			(xy 111.76 123.19) (xy 115.57 123.19)
		)
	)
	(wire
		(pts
			(xy 135.89 25.4) (xy 135.89 26.67)
		)
	)
	(wire
		(pts
			(xy 265.43 20.32) (xy 276.86 20.32)
		)
	)
	(wire
		(pts
			(xy 97.79 40.64) (xy 97.79 43.18)
		)
	)
	(wire
		(pts
			(xy 148.59 26.67) (xy 148.59 27.94)
		)
	)
	(wire
		(pts
			(xy 187.96 35.56) (xy 198.12 35.56)
		)
	)
	(wire
		(pts
			(xy 262.89 102.87) (xy 207.01 102.87)
		)
	)
	(wire
		(pts
			(xy 35.56 153.67) (xy 39.37 153.67)
		)
	)
	(wire
		(pts
			(xy 139.7 35.56) (xy 148.59 35.56)
		)
	)
	(wire
		(pts
			(xy 148.59 25.4) (xy 148.59 26.67)
		)
	)
	(wire
		(pts
			(xy 55.88 119.38) (xy 59.69 119.38)
		)
	)
	(wire
		(pts
			(xy 49.53 163.83) (xy 49.53 166.37)
		)
	)
	(wire
		(pts
			(xy 63.5 120.65) (xy 73.66 120.65)
		)
	)
	(wire
		(pts
			(xy 173.99 60.96) (xy 158.75 60.96)
		)
	)
	(wire
		(pts
			(xy 55.88 38.1) (xy 55.88 35.56)
		)
	)
	(hierarchical_label "9V"
		(shape input)
		(at 125.73 17.78 180)
	)
	(hierarchical_label "ANT"
		(shape input)
		(at 261.62 139.7 0)
	)
	(hierarchical_label "sw_ctrl"
		(shape input)
		(at 35.56 153.67 180)
	)
	(hierarchical_label "9V"
		(shape input)
		(at 144.78 60.96 180)
	)
	(hierarchical_label "3V3"
		(shape input)
		(at 115.57 120.65 0)
	)
	(hierarchical_label "mix_IF"
		(shape input)
		(at 115.57 123.19 0)
	)
	(hierarchical_label "3V3"
		(shape input)
		(at 252.73 116.84 0)
	)
	(hierarchical_label "sw_ctrl"
		(shape input)
		(at 274.32 109.22 0)
	)
	(hierarchical_label "9V"
		(shape input)
		(at 231.14 17.78 180)
	)
	(hierarchical_label "3V3"
		(shape input)
		(at 45.72 142.24 180)
	)
	(symbol
		(lib_id "Device:C")
		(at 276.86 24.13 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C12"
			(at 280.67 22.8599 0)
		)
		(property "Value" "C"
			(at 280.67 25.3999 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 275.8948 20.32 0)
		)
		(property "Datasheet" "~"
			(at 276.86 24.13 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 276.86 24.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 163.83 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C36"
			(at 163.83 71.12 90)
		)
		(property "Value" "10n"
			(at 163.83 73.66 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 167.64 77.7748 0)
		)
		(property "Datasheet" "~"
			(at 163.83 78.74 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 163.83 78.74 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C36")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4259-63:4259-63")
		(at 73.66 120.65 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC3"
			(at 92.71 113.03 0)
		)
		(property "Value" "4259-63"
			(at 92.71 115.57 0)
		)
		(property "Footprint" "SOT65P210X110-6N"
			(at 107.95 215.57 0)
		)
		(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe4259ds.pdf"
			(at 107.95 315.57 0)
		)
		(property "Description" "RF switch IC"
			(at 73.66 120.65 0)
		)
		(property "Height" "1.1"
			(at 107.95 515.57 0)
		)
		(property "Mouser Part Number" "81-4259-63"
			(at 107.95 615.57 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/pSemi/4259-63?qs=iw0hurA%2FaD37qvQcKdATTw%3D%3D"
			(at 107.95 715.57 0)
		)
		(property "Manufacturer_Name" "Peregrine Semiconductor"
			(at 107.95 815.57 0)
		)
		(property "Manufacturer_Part_Number" "4259-63"
			(at 107.95 915.57 0)
		)
		(pin "2")
		(pin "1")
		(pin "5")
		(pin "6")
		(pin "3")
		(pin "4")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 267.97 113.03 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R11"
			(at 270.51 111.7599 0)
		)
		(property "Value" "100"
			(at 270.51 114.2999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 269.748 113.03 90)
		)
		(property "Datasheet" "~"
			(at 267.97 113.03 0)
		)
		(property "Description" "Resistor"
			(at 267.97 113.03 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 274.32 120.65 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C15"
			(at 278.13 119.3799 0)
		)
		(property "Value" "1n"
			(at 278.13 121.9199 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 273.3548 116.84 0)
		)
		(property "Datasheet" "~"
			(at 274.32 120.65 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 274.32 120.65 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 97.79 43.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR05"
			(at 97.79 49.53 0)
		)
		(property "Value" "GND"
			(at 97.79 47.498 0)
		)
		(property "Footprint" ""
			(at 97.79 43.18 0)
		)
		(property "Datasheet" ""
			(at 97.79 43.18 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 97.79 43.18 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4259-63:4259-63")
		(at 210.82 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC2"
			(at 229.87 109.22 0)
		)
		(property "Value" "4259-63"
			(at 229.87 111.76 0)
		)
		(property "Footprint" "SOT65P210X110-6N"
			(at 245.11 211.76 0)
		)
		(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe4259ds.pdf"
			(at 245.11 311.76 0)
		)
		(property "Description" "RF switch IC"
			(at 210.82 116.84 0)
		)
		(property "Height" "1.1"
			(at 245.11 511.76 0)
		)
		(property "Mouser Part Number" "81-4259-63"
			(at 245.11 611.76 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/pSemi/4259-63?qs=iw0hurA%2FaD37qvQcKdATTw%3D%3D"
			(at 245.11 711.76 0)
		)
		(property "Manufacturer_Name" "Peregrine Semiconductor"
			(at 245.11 811.76 0)
		)
		(property "Manufacturer_Part_Number" "4259-63"
			(at 245.11 911.76 0)
		)
		(pin "2")
		(pin "1")
		(pin "5")
		(pin "6")
		(pin "3")
		(pin "4")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PHA-101+:PHA-101+")
		(at 208.28 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC5"
			(at 229.87 27.94 0)
		)
		(property "Value" "PHA-101+"
			(at 229.87 30.48 0)
		)
		(property "Footprint" "GALI19"
			(at 247.65 130.48 0)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/PHA-101+.pdf"
			(at 247.65 230.48 0)
		)
		(property "Description" "RF Amplifier MMIC AMPLIFIER"
			(at 208.28 35.56 0)
		)
		(property "Height" "1.6"
			(at 247.65 430.48 0)
		)
		(property "Mouser Part Number" "139-PHA-101"
			(at 247.65 530.48 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/PHA-101%2b?qs=xZ%2FP%252Ba9zWqbA11kwlpohzA%3D%3D"
			(at 247.65 630.48 0)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at 247.65 730.48 0)
		)
		(property "Manufacturer_Part_Number" "PHA-101+"
			(at 247.65 830.48 0)
		)
		(pin "3")
		(pin "1")
		(pin "2")
		(pin "4")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 91.44 148.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR022"
			(at 91.44 154.94 0)
		)
		(property "Value" "GND"
			(at 91.44 152.908 0)
		)
		(property "Footprint" ""
			(at 91.44 148.59 0)
		)
		(property "Datasheet" ""
			(at 91.44 148.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 91.44 148.59 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR022")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 55.88 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 55.88 54.61 0)
		)
		(property "Value" "GND"
			(at 55.88 52.578 0)
		)
		(property "Footprint" ""
			(at 55.88 48.26 0)
		)
		(property "Datasheet" ""
			(at 55.88 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 55.88 48.26 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 220.98 143.51 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 224.79 142.2399 0)
		)
		(property "Value" "51p"
			(at 224.79 144.7799 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 221.9452 147.32 0)
		)
		(property "Datasheet" "~"
			(at 220.98 143.51 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 220.98 143.51 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 252.73 27.94 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L3"
			(at 254 26.6699 0)
		)
		(property "Value" "L"
			(at 254 29.2099 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 252.73 27.94 0)
		)
		(property "Datasheet" "~"
			(at 252.73 27.94 0)
		)
		(property "Description" "Inductor"
			(at 252.73 27.94 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 208.28 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR014"
			(at 208.28 48.26 0)
		)
		(property "Value" "GND"
			(at 208.28 46.228 0)
		)
		(property "Footprint" ""
			(at 208.28 41.91 0)
		)
		(property "Datasheet" ""
			(at 208.28 41.91 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 208.28 41.91 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 148.59 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L2"
			(at 149.86 30.4799 0)
		)
		(property "Value" "L"
			(at 149.86 33.0199 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 148.59 31.75 0)
		)
		(property "Datasheet" "~"
			(at 148.59 31.75 0)
		)
		(property "Description" "Inductor"
			(at 148.59 31.75 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 91.44 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C16"
			(at 95.25 140.9699 0)
		)
		(property "Value" "1n"
			(at 95.25 143.5099 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 92.4052 146.05 0)
		)
		(property "Datasheet" "~"
			(at 91.44 142.24 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 91.44 142.24 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 187.96 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR013"
			(at 187.96 54.61 0)
		)
		(property "Value" "GND"
			(at 187.96 52.578 0)
		)
		(property "Footprint" ""
			(at 187.96 48.26 0)
		)
		(property "Datasheet" ""
			(at 187.96 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 187.96 48.26 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 153.67 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR019"
			(at 153.67 95.25 0)
		)
		(property "Value" "GND"
			(at 153.67 93.218 0)
		)
		(property "Footprint" ""
			(at 153.67 88.9 0)
		)
		(property "Datasheet" ""
			(at 153.67 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 153.67 88.9 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR019")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 241.3 143.51 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C2"
			(at 245.11 142.2399 0)
		)
		(property "Value" "51p"
			(at 245.11 144.7799 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 242.2652 147.32 0)
		)
		(property "Datasheet" "~"
			(at 241.3 143.51 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 241.3 143.51 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 232.41 139.7 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L1"
			(at 232.41 134.62 90)
		)
		(property "Value" "150nH"
			(at 232.41 137.16 90)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 232.41 139.7 0)
		)
		(property "Datasheet" "~"
			(at 232.41 139.7 0)
		)
		(property "Description" "Inductor"
			(at 232.41 139.7 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 55.88 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR011"
			(at 55.88 125.73 0)
		)
		(property "Value" "GND"
			(at 55.88 123.698 0)
		)
		(property "Footprint" ""
			(at 55.88 119.38 0)
		)
		(property "Datasheet" ""
			(at 55.88 119.38 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 55.88 119.38 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 153.67 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C11"
			(at 157.48 81.2799 0)
		)
		(property "Value" "51p"
			(at 157.48 83.8199 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 154.6352 86.36 0)
		)
		(property "Datasheet" "~"
			(at 153.67 82.55 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 153.67 82.55 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 274.32 127 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR023"
			(at 274.32 133.35 0)
		)
		(property "Value" "GND"
			(at 274.32 131.318 0)
		)
		(property "Footprint" ""
			(at 274.32 127 0)
		)
		(property "Datasheet" ""
			(at 274.32 127 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 274.32 127 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 254 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR015"
			(at 254 46.99 0)
		)
		(property "Value" "GND"
			(at 254 44.958 0)
		)
		(property "Footprint" ""
			(at 254 40.64 0)
		)
		(property "Datasheet" ""
			(at 254 40.64 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 254 40.64 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 196.85 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C8"
			(at 196.85 71.12 90)
		)
		(property "Value" "10n"
			(at 196.85 73.66 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 200.66 77.7748 0)
		)
		(property "Datasheet" "~"
			(at 196.85 78.74 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 196.85 78.74 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 170.18 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 172.72 40.6399 0)
		)
		(property "Value" "R"
			(at 172.72 43.1799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 168.402 41.91 90)
		)
		(property "Datasheet" "~"
			(at 170.18 41.91 0)
		)
		(property "Description" "Resistor"
			(at 170.18 41.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 135.89 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C10"
			(at 139.7 81.2799 0)
		)
		(property "Value" "51p"
			(at 139.7 83.8199 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 136.8552 86.36 0)
		)
		(property "Datasheet" "~"
			(at 135.89 82.55 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 135.89 82.55 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 87.63 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C4"
			(at 87.63 27.94 90)
		)
		(property "Value" "10n"
			(at 87.63 30.48 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 91.44 34.5948 0)
		)
		(property "Datasheet" "~"
			(at 87.63 35.56 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 87.63 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 55.88 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 58.42 40.6399 0)
		)
		(property "Value" "300"
			(at 58.42 43.1799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 54.102 41.91 90)
		)
		(property "Datasheet" "~"
			(at 55.88 41.91 0)
		)
		(property "Description" "Resistor"
			(at 55.88 41.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "RF_Amplifier:PGA-103")
		(at 182.88 78.74 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 182.88 86.36 0)
		)
		(property "Value" "PGA-103"
			(at 182.88 88.9 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 181.61 88.9 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PGA-103+.pdf"
			(at 182.88 78.74 0)
		)
		(property "Description" "50-4000MHz +11dB Low Noise Amplifier, SOT-89"
			(at 182.88 78.74 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 232.41 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C9"
			(at 232.41 71.12 90)
		)
		(property "Value" "330p"
			(at 232.41 73.66 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 236.22 77.7748 0)
		)
		(property "Datasheet" "~"
			(at 232.41 78.74 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 232.41 78.74 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 49.53 166.37 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR066"
			(at 49.53 172.72 0)
		)
		(property "Value" "GND"
			(at 49.53 170.688 0)
		)
		(property "Footprint" ""
			(at 49.53 166.37 0)
		)
		(property "Datasheet" ""
			(at 49.53 166.37 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 49.53 166.37 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR066")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 158.75 17.78 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C37"
			(at 158.75 21.59 90)
		)
		(property "Value" "C"
			(at 158.75 24.13 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 162.56 16.8148 0)
		)
		(property "Datasheet" "~"
			(at 158.75 17.78 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 158.75 17.78 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C37")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 241.3 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR016"
			(at 241.3 87.63 0)
		)
		(property "Value" "GND"
			(at 241.3 85.598 0)
		)
		(property "Footprint" ""
			(at 241.3 81.28 0)
		)
		(property "Datasheet" ""
			(at 241.3 81.28 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 241.3 81.28 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 187.96 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 190.5 40.6399 0)
		)
		(property "Value" "R"
			(at 190.5 43.1799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 186.182 41.91 90)
		)
		(property "Datasheet" "~"
			(at 187.96 41.91 0)
		)
		(property "Description" "Resistor"
			(at 187.96 41.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 276.86 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR020"
			(at 276.86 38.1 0)
		)
		(property "Value" "GND"
			(at 276.86 36.068 0)
		)
		(property "Footprint" ""
			(at 276.86 31.75 0)
		)
		(property "Datasheet" ""
			(at 276.86 31.75 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 276.86 31.75 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR020")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 241.3 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR02"
			(at 241.3 156.21 0)
		)
		(property "Value" "GND"
			(at 241.3 154.178 0)
		)
		(property "Footprint" ""
			(at 241.3 149.86 0)
		)
		(property "Datasheet" ""
			(at 241.3 149.86 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 241.3 149.86 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 198.12 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR010"
			(at 198.12 125.73 0)
		)
		(property "Value" "GND"
			(at 198.12 123.698 0)
		)
		(property "Footprint" ""
			(at 198.12 119.38 0)
		)
		(property "Datasheet" ""
			(at 198.12 119.38 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 198.12 119.38 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 265.43 24.13 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C13"
			(at 269.24 22.8599 0)
		)
		(property "Value" "C"
			(at 269.24 25.3999 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 264.4648 20.32 0)
		)
		(property "Datasheet" "~"
			(at 265.43 24.13 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 265.43 24.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 167.64 20.32 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR054"
			(at 167.64 26.67 0)
		)
		(property "Value" "GND"
			(at 167.64 24.638 0)
		)
		(property "Footprint" ""
			(at 167.64 20.32 0)
		)
		(property "Datasheet" ""
			(at 167.64 20.32 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 167.64 20.32 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR054")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 220.98 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01"
			(at 220.98 156.21 0)
		)
		(property "Value" "GND"
			(at 220.98 154.178 0)
		)
		(property "Footprint" ""
			(at 220.98 149.86 0)
		)
		(property "Datasheet" ""
			(at 220.98 149.86 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 220.98 149.86 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 173.99 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L6"
			(at 175.26 69.8499 0)
		)
		(property "Value" "L"
			(at 175.26 72.3899 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 173.99 71.12 0)
		)
		(property "Datasheet" "~"
			(at 173.99 71.12 0)
		)
		(property "Description" "Inductor"
			(at 173.99 71.12 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 135.89 26.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR08"
			(at 135.89 33.02 0)
		)
		(property "Value" "GND"
			(at 135.89 30.988 0)
		)
		(property "Footprint" ""
			(at 135.89 26.67 0)
		)
		(property "Datasheet" ""
			(at 135.89 26.67 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 135.89 26.67 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 190.5 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR017"
			(at 190.5 72.39 0)
		)
		(property "Value" "GND"
			(at 190.5 70.358 0)
		)
		(property "Footprint" ""
			(at 190.5 66.04 0)
		)
		(property "Datasheet" ""
			(at 190.5 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 190.5 66.04 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 73.66 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 76.2 40.6399 0)
		)
		(property "Value" "300"
			(at 76.2 43.1799 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 71.882 41.91 90)
		)
		(property "Datasheet" "~"
			(at 73.66 41.91 0)
		)
		(property "Description" "Resistor"
			(at 73.66 41.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 252.73 139.7 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C19"
			(at 252.73 132.08 90)
		)
		(property "Value" "1n"
			(at 252.73 134.62 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 256.54 138.7348 0)
		)
		(property "Datasheet" "~"
			(at 252.73 139.7 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 252.73 139.7 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "ERA-1SM+:ERA-1SM+")
		(at 114.3 39.37 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC4"
			(at 119.126 28.448 90)
		)
		(property "Value" "ERA-1SM+"
			(at 119.126 30.988 90)
		)
		(property "Footprint" "ERA1SM"
			(at 47.32 66.04 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
			(at -52.68 66.04 0)
		)
		(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
			(at 114.3 39.37 0)
		)
		(property "Height" "1.52"
			(at -252.68 66.04 0)
		)
		(property "Mouser Part Number" "139-ERA-1SM"
			(at -352.68 66.04 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
			(at -452.68 66.04 0)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at -552.68 66.04 0)
		)
		(property "Manufacturer_Part_Number" "ERA-1SM+"
			(at -652.68 66.04 0)
		)
		(pin "3")
		(pin "4")
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 152.4 60.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R9"
			(at 152.4 54.61 90)
		)
		(property "Value" "R"
			(at 152.4 57.15 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 152.4 59.182 90)
		)
		(property "Datasheet" "~"
			(at 152.4 60.96 0)
		)
		(property "Description" "Resistor"
			(at 152.4 60.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 170.18 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR012"
			(at 170.18 54.61 0)
		)
		(property "Value" "GND"
			(at 170.18 52.578 0)
		)
		(property "Footprint" ""
			(at 170.18 48.26 0)
		)
		(property "Datasheet" ""
			(at 170.18 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 170.18 48.26 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 148.59 21.59 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 151.13 20.3199 0)
		)
		(property "Value" "R"
			(at 151.13 22.8599 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 150.368 21.59 90)
		)
		(property "Datasheet" "~"
			(at 148.59 21.59 0)
		)
		(property "Description" "Resistor"
			(at 148.59 21.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 210.82 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L4"
			(at 210.82 73.66 90)
		)
		(property "Value" "620nH"
			(at 210.82 76.2 90)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 210.82 78.74 0)
		)
		(property "Datasheet" "~"
			(at 210.82 78.74 0)
		)
		(property "Description" "Inductor"
			(at 210.82 78.74 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 158.75 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C5"
			(at 158.75 27.94 90)
		)
		(property "Value" "10n"
			(at 158.75 30.48 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 162.56 34.5948 0)
		)
		(property "Datasheet" "~"
			(at 158.75 35.56 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 158.75 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 135.89 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR018"
			(at 135.89 95.25 0)
		)
		(property "Value" "GND"
			(at 135.89 93.218 0)
		)
		(property "Footprint" ""
			(at 135.89 88.9 0)
		)
		(property "Datasheet" ""
			(at 135.89 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 135.89 88.9 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR018")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 146.05 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L5"
			(at 146.05 73.66 90)
		)
		(property "Value" "150nH"
			(at 146.05 76.2 90)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 146.05 78.74 0)
		)
		(property "Datasheet" "~"
			(at 146.05 78.74 0)
		)
		(property "Description" "Inductor"
			(at 146.05 78.74 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 179.07 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 179.07 29.21 90)
		)
		(property "Value" "0"
			(at 179.07 31.75 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 179.07 37.338 90)
		)
		(property "Datasheet" "~"
			(at 179.07 35.56 0)
		)
		(property "Description" "Resistor"
			(at 179.07 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 134.62 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR021"
			(at 134.62 74.93 0)
		)
		(property "Value" "GND"
			(at 134.62 72.898 0)
		)
		(property "Footprint" ""
			(at 134.62 68.58 0)
		)
		(property "Datasheet" ""
			(at 134.62 68.58 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 134.62 68.58 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR021")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 158.75 64.77 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C14"
			(at 162.56 63.4999 0)
		)
		(property "Value" "C"
			(at 162.56 66.0399 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 157.7848 60.96 0)
		)
		(property "Datasheet" "~"
			(at 158.75 64.77 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 158.75 64.77 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 135.89 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 139.7 20.3199 0)
		)
		(property "Value" "C"
			(at 139.7 22.8599 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 136.8552 25.4 0)
		)
		(property "Datasheet" "~"
			(at 135.89 21.59 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 135.89 21.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 73.66 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR04"
			(at 73.66 54.61 0)
		)
		(property "Value" "GND"
			(at 73.66 52.578 0)
		)
		(property "Footprint" ""
			(at 73.66 48.26 0)
		)
		(property "Datasheet" ""
			(at 73.66 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 73.66 48.26 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 82.55 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R10"
			(at 82.55 144.78 90)
		)
		(property "Value" "100"
			(at 82.55 147.32 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 82.55 152.908 90)
		)
		(property "Datasheet" "~"
			(at 82.55 151.13 0)
		)
		(property "Description" "Resistor"
			(at 82.55 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 222.25 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 222.25 72.39 90)
		)
		(property "Value" "150"
			(at 222.25 74.93 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 222.25 80.518 90)
		)
		(property "Datasheet" "~"
			(at 222.25 78.74 0)
		)
		(property "Description" "Resistor"
			(at 222.25 78.74 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xGxx:74LVC1GU04DRL")
		(at 49.53 153.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 71.12 147.2498 0)
		)
		(property "Value" "74LVC1GU04DRL"
			(at 71.12 149.7898 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-553"
			(at 49.53 166.37 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1gu04.pdf"
			(at 45.72 153.67 0)
		)
		(property "Description" "Single Inverter Gate, SOT-553"
			(at 49.53 153.67 0)
		)
		(pin "3")
		(pin "2")
		(pin "5")
		(pin "1")
		(pin "4")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 139.7 43.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR06"
			(at 139.7 49.53 0)
		)
		(property "Value" "GND"
			(at 139.7 47.498 0)
		)
		(property "Footprint" ""
			(at 139.7 43.18 0)
		)
		(property "Datasheet" ""
			(at 139.7 43.18 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 139.7 43.18 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 201.93 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C6"
			(at 201.93 27.94 90)
		)
		(property "Value" "10n"
			(at 201.93 30.48 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 205.74 34.5948 0)
		)
		(property "Datasheet" "~"
			(at 201.93 35.56 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 201.93 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 64.77 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 64.77 29.21 90)
		)
		(property "Value" "18"
			(at 64.77 31.75 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 64.77 37.338 90)
		)
		(property "Datasheet" "~"
			(at 64.77 35.56 0)
		)
		(property "Description" "Resistor"
			(at 64.77 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 259.08 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C7"
			(at 259.08 27.94 90)
		)
		(property "Value" "10n"
			(at 259.08 30.48 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 262.89 34.5948 0)
		)
		(property "Datasheet" "~"
			(at 259.08 35.56 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 259.08 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
)
