(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C_Polarized"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_Polarized"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Polarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "CP_*"
				(at 0 0 0)
			)
			(symbol "C_Polarized_0_1"
				(rectangle
					(start -2.286 0.508)
					(end 2.286 1.016)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 2.286) (xy -0.762 2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 2.794) (xy -1.27 1.778)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.508)
					(end -2.286 -1.016)
					(fill
						(type outline)
					)
				)
			)
			(symbol "C_Polarized_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:L"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -1.27 0 90)
			)
			(property "Value" "L"
				(at 1.905 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_0_1"
				(arc
					(start 0 2.54)
					(mid 0.6323 1.905)
					(end 0 1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.27)
					(mid 0.6323 0.635)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.6323 -0.635)
					(end 0 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.27)
					(mid 0.6323 -1.905)
					(end 0 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulator_Linear:LT1962-3.3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 8.89 0)
			)
			(property "Value" "LT1962-3.3"
				(at 1.27 -6.35 0)
			)
			(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
				(at 0 -8.89 0)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
				(at 0 -13.97 0)
			)
			(property "Description" "3.3V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "LDO 3.3V"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
				(at 0 0 0)
			)
			(symbol "LT1962-3.3_0_1"
				(rectangle
					(start -7.62 7.62)
					(end 7.62 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "LT1962-3.3_1_1"
				(pin power_in line
					(at -10.16 5.08 0)
					(length 2.54)
					(name "IN")
					(number "8")
				)
				(pin input line
					(at -10.16 -2.54 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "5")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 5.08 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 2.54 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_out line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin input line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "SENSE")
					(number "2")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "BYP")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 109.22 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 81.28 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 128.27 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 76.2 48.26) (xy 81.28 48.26)
		)
	)
	(wire
		(pts
			(xy 85.09 55.88) (xy 81.28 55.88)
		)
	)
	(wire
		(pts
			(xy 76.2 33.02) (xy 76.2 48.26)
		)
	)
	(wire
		(pts
			(xy 81.28 48.26) (xy 85.09 48.26)
		)
	)
	(wire
		(pts
			(xy 113.03 48.26) (xy 128.27 48.26)
		)
	)
	(wire
		(pts
			(xy 81.28 55.88) (xy 81.28 48.26)
		)
	)
	(wire
		(pts
			(xy 49.53 48.26) (xy 62.23 48.26)
		)
	)
	(wire
		(pts
			(xy 109.22 50.8) (xy 105.41 50.8)
		)
	)
	(wire
		(pts
			(xy 113.03 50.8) (xy 113.03 48.26)
		)
	)
	(wire
		(pts
			(xy 53.34 33.02) (xy 58.42 33.02)
		)
	)
	(wire
		(pts
			(xy 105.41 48.26) (xy 109.22 48.26)
		)
	)
	(wire
		(pts
			(xy 49.53 55.88) (xy 55.88 55.88)
		)
	)
	(wire
		(pts
			(xy 113.03 58.42) (xy 105.41 58.42)
		)
	)
	(wire
		(pts
			(xy 76.2 33.02) (xy 91.44 33.02)
		)
	)
	(wire
		(pts
			(xy 128.27 58.42) (xy 128.27 60.96)
		)
	)
	(wire
		(pts
			(xy 66.04 33.02) (xy 76.2 33.02)
		)
	)
	(wire
		(pts
			(xy 95.25 60.96) (xy 95.25 63.5)
		)
	)
	(wire
		(pts
			(xy 128.27 50.8) (xy 128.27 48.26)
		)
	)
	(wire
		(pts
			(xy 105.41 58.42) (xy 105.41 55.88)
		)
	)
	(wire
		(pts
			(xy 55.88 55.88) (xy 62.23 55.88)
		)
	)
	(wire
		(pts
			(xy 55.88 55.88) (xy 55.88 59.69)
		)
	)
	(wire
		(pts
			(xy 128.27 48.26) (xy 138.43 48.26)
		)
	)
	(wire
		(pts
			(xy 62.23 48.26) (xy 76.2 48.26)
		)
	)
	(wire
		(pts
			(xy 109.22 48.26) (xy 109.22 50.8)
		)
	)
	(wire
		(pts
			(xy 113.03 48.26) (xy 109.22 48.26)
		)
	)
	(hierarchical_label "9V-in"
		(shape input)
		(at 53.34 33.02 180)
	)
	(hierarchical_label "9V-1"
		(shape input)
		(at 91.44 33.02 0)
	)
	(hierarchical_label "3V3-1"
		(shape input)
		(at 138.43 48.26 0)
	)
	(symbol
		(lib_id "Device:C_Polarized")
		(at 128.27 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C62"
			(at 132.08 52.4509 0)
		)
		(property "Value" "10u"
			(at 132.08 54.9909 0)
		)
		(property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B_HandSolder"
			(at 129.2352 58.42 0)
		)
		(property "Datasheet" "~"
			(at 128.27 54.61 0)
		)
		(property "Description" "Polarized capacitor"
			(at 128.27 54.61 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C62")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 49.53 52.07 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C59"
			(at 53.34 50.7999 0)
		)
		(property "Value" "1n"
			(at 53.34 53.3399 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 48.5648 48.26 0)
		)
		(property "Datasheet" "~"
			(at 49.53 52.07 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 49.53 52.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C59")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 113.03 54.61 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C61"
			(at 116.84 53.3399 0)
		)
		(property "Value" "10n"
			(at 116.84 55.8799 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 112.0648 50.8 0)
		)
		(property "Datasheet" "~"
			(at 113.03 54.61 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 113.03 54.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C61")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 95.25 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR079"
			(at 95.25 69.85 0)
		)
		(property "Value" "GND"
			(at 95.25 67.564 0)
		)
		(property "Footprint" ""
			(at 95.25 63.5 0)
		)
		(property "Datasheet" ""
			(at 95.25 63.5 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 95.25 63.5 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR079")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 128.27 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR080"
			(at 128.27 67.31 0)
		)
		(property "Value" "GND"
			(at 128.27 65.024 0)
		)
		(property "Footprint" ""
			(at 128.27 60.96 0)
		)
		(property "Datasheet" ""
			(at 128.27 60.96 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 128.27 60.96 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR080")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 55.88 59.69 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR077"
			(at 55.88 66.04 0)
		)
		(property "Value" "GND"
			(at 55.88 63.754 0)
		)
		(property "Footprint" ""
			(at 55.88 59.69 0)
		)
		(property "Datasheet" ""
			(at 55.88 59.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 55.88 59.69 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR077")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 62.23 33.02 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L16"
			(at 62.23 27.94 90)
		)
		(property "Value" "1uH"
			(at 62.23 30.48 90)
		)
		(property "Footprint" "Inductor_SMD:L_1210_3225Metric_Pad1.42x2.65mm_HandSolder"
			(at 62.23 33.02 0)
		)
		(property "Datasheet" "~"
			(at 62.23 33.02 0)
		)
		(property "Description" "Inductor"
			(at 62.23 33.02 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulator_Linear:LT1962-3.3")
		(at 95.25 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U4"
			(at 95.25 40.64 0)
		)
		(property "Value" "LT1962-3.3"
			(at 95.25 43.18 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 95.25 62.23 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1962fb.pdf"
			(at 95.25 67.31 0)
		)
		(property "Description" "3.3V, 300mA, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 95.25 53.34 0)
		)
		(pin "6")
		(pin "3")
		(pin "2")
		(pin "7")
		(pin "1")
		(pin "4")
		(pin "5")
		(pin "8")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "U4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Polarized")
		(at 62.23 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C60"
			(at 66.04 49.9109 0)
		)
		(property "Value" "47u"
			(at 66.04 52.4509 0)
		)
		(property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_HandSolder"
			(at 63.1952 55.88 0)
		)
		(property "Datasheet" "~"
			(at 62.23 52.07 0)
		)
		(property "Description" "Polarized capacitor"
			(at 62.23 52.07 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C60")
					(unit 1)
				)
			)
		)
	)
)
