(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "4259-63:4259-63"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 34.29 7.62 0)
			)
			(property "Value" "4259-63"
				(at 34.29 5.08 0)
			)
			(property "Footprint" "SOT65P210X110-6N"
				(at 34.29 -94.92 0)
			)
			(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe4259ds.pdf"
				(at 34.29 -194.92 0)
			)
			(property "Description" "RF switch IC"
				(at 0 0 0)
			)
			(property "Height" "1.1"
				(at 34.29 -394.92 0)
			)
			(property "Mouser Part Number" "81-4259-63"
				(at 34.29 -494.92 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/pSemi/4259-63?qs=iw0hurA%2FaD37qvQcKdATTw%3D%3D"
				(at 34.29 -594.92 0)
			)
			(property "Manufacturer_Name" "Peregrine Semiconductor"
				(at 34.29 -694.92 0)
			)
			(property "Manufacturer_Part_Number" "4259-63"
				(at 34.29 -794.92 0)
			)
			(symbol "4259-63_1_1"
				(rectangle
					(start 5.08 2.54)
					(end 33.02 -7.62)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RF1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RF2")
					(number "3")
				)
				(pin passive line
					(at 38.1 0 180)
					(length 5.08)
					(name "~{CTRL_OR_VDD}")
					(number "6")
				)
				(pin passive line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "RFC")
					(number "5")
				)
				(pin passive line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "CTRL")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:L"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -1.27 0 90)
			)
			(property "Value" "L"
				(at 1.905 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_0_1"
				(arc
					(start 0 2.54)
					(mid 0.6323 1.905)
					(end 0 1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.27)
					(mid 0.6323 0.635)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.6323 -0.635)
					(end 0 -1.27)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.27)
					(mid 0.6323 -1.905)
					(end 0 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "ERA-1SM+:ERA-1SM+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.366 13.97 0)
			)
			(property "Value" "ERA-1SM+"
				(at 7.366 11.43 0)
			)
			(property "Footprint" "ERA1SM"
				(at 26.67 -66.98 0)
			)
			(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
				(at 26.67 -166.98 0)
			)
			(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
				(at 0 0 0)
			)
			(property "Height" "1.52"
				(at 26.67 -366.98 0)
			)
			(property "Mouser Part Number" "139-ERA-1SM"
				(at 26.67 -466.98 0)
			)
			(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
				(at 26.67 -566.98 0)
			)
			(property "Manufacturer_Name" "Mini-Circuits"
				(at 26.67 -666.98 0)
			)
			(property "Manufacturer_Part_Number" "ERA-1SM+"
				(at 26.67 -766.98 0)
			)
			(symbol "ERA-1SM+_1_1"
				(rectangle
					(start -6.35 20.32)
					(end 3.81 -11.43)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 25.4 270)
					(length 5.08)
					(name "RF_-_OUT_AND_DC_-_IN")
					(number "3")
				)
				(pin passive line
					(at -3.81 -16.51 90)
					(length 5.08)
					(name "RF_IN")
					(number "1")
				)
				(pin passive line
					(at 1.27 25.4 270)
					(length 5.08)
					(name "GND_1")
					(number "2")
				)
				(pin passive line
					(at 1.27 -16.51 90)
					(length 5.08)
					(name "GND_2")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 91.44 114.3)
		(end 123.19 140.97)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 146.05 73.66)
		(end 177.8 100.33)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 62.23 116.84)
		(end 83.82 127)
		(fill
			(type none)
		)
	)
	(text "910MHz BPF?"
		(exclude_from_sim no)
		(at 72.39 114.554 0)
	)
	(text "-3dB\n"
		(exclude_from_sim no)
		(at 212.852 119.38 0)
	)
	(text "1,1GHz LPF"
		(exclude_from_sim no)
		(at 97.79 117.348 0)
	)
	(text "1,1GHz LPF"
		(exclude_from_sim no)
		(at 152.4 76.708 0)
	)
	(junction
		(at 168.91 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 160.02 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 255.27 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 105.41 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 134.62 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 50.8 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 208.28 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 57.15)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 134.62 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 195.58 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 128.27 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 195.58 121.92) (xy 198.12 121.92)
		)
	)
	(wire
		(pts
			(xy 105.41 132.08) (xy 114.3 132.08)
		)
	)
	(wire
		(pts
			(xy 152.4 81.28) (xy 152.4 83.82)
		)
	)
	(wire
		(pts
			(xy 142.24 81.28) (xy 152.4 81.28)
		)
	)
	(wire
		(pts
			(xy 218.44 121.92) (xy 218.44 97.79)
		)
	)
	(wire
		(pts
			(xy 106.68 66.04) (xy 106.68 68.58)
		)
	)
	(wire
		(pts
			(xy 50.8 91.44) (xy 50.8 93.98)
		)
	)
	(wire
		(pts
			(xy 50.8 81.28) (xy 53.34 81.28)
		)
	)
	(wire
		(pts
			(xy 255.27 106.68) (xy 255.27 111.76)
		)
	)
	(wire
		(pts
			(xy 105.41 132.08) (xy 105.41 134.62)
		)
	)
	(wire
		(pts
			(xy 134.62 134.62) (xy 134.62 137.16)
		)
	)
	(wire
		(pts
			(xy 266.7 111.76) (xy 273.05 111.76)
		)
	)
	(wire
		(pts
			(xy 165.1 81.28) (xy 168.91 81.28)
		)
	)
	(wire
		(pts
			(xy 271.78 92.71) (xy 269.24 92.71)
		)
	)
	(wire
		(pts
			(xy 135.89 106.68) (xy 139.7 106.68)
		)
	)
	(wire
		(pts
			(xy 231.14 92.71) (xy 231.14 81.28)
		)
	)
	(wire
		(pts
			(xy 78.74 86.36) (xy 78.74 88.9)
		)
	)
	(wire
		(pts
			(xy 63.5 91.44) (xy 63.5 93.98)
		)
	)
	(wire
		(pts
			(xy 134.62 134.62) (xy 134.62 132.08)
		)
	)
	(wire
		(pts
			(xy 128.27 57.15) (xy 106.68 57.15)
		)
	)
	(wire
		(pts
			(xy 34.29 81.28) (xy 38.1 81.28)
		)
	)
	(wire
		(pts
			(xy 128.27 78.74) (xy 128.27 81.28)
		)
	)
	(wire
		(pts
			(xy 218.44 97.79) (xy 231.14 97.79)
		)
	)
	(wire
		(pts
			(xy 214.63 95.25) (xy 231.14 95.25)
		)
	)
	(wire
		(pts
			(xy 255.27 111.76) (xy 255.27 115.57)
		)
	)
	(wire
		(pts
			(xy 205.74 121.92) (xy 208.28 121.92)
		)
	)
	(wire
		(pts
			(xy 160.02 91.44) (xy 168.91 91.44)
		)
	)
	(wire
		(pts
			(xy 128.27 81.28) (xy 120.65 81.28)
		)
	)
	(wire
		(pts
			(xy 45.72 81.28) (xy 50.8 81.28)
		)
	)
	(wire
		(pts
			(xy 102.87 121.92) (xy 97.79 121.92)
		)
	)
	(wire
		(pts
			(xy 102.87 57.15) (xy 106.68 57.15)
		)
	)
	(wire
		(pts
			(xy 54.61 121.92) (xy 97.79 121.92)
		)
	)
	(wire
		(pts
			(xy 135.89 116.84) (xy 135.89 106.68)
		)
	)
	(wire
		(pts
			(xy 149.86 134.62) (xy 154.94 134.62)
		)
	)
	(wire
		(pts
			(xy 50.8 83.82) (xy 50.8 81.28)
		)
	)
	(wire
		(pts
			(xy 195.58 132.08) (xy 195.58 134.62)
		)
	)
	(wire
		(pts
			(xy 195.58 124.46) (xy 195.58 121.92)
		)
	)
	(wire
		(pts
			(xy 208.28 121.92) (xy 218.44 121.92)
		)
	)
	(wire
		(pts
			(xy 110.49 121.92) (xy 114.3 121.92)
		)
	)
	(wire
		(pts
			(xy 114.3 121.92) (xy 114.3 124.46)
		)
	)
	(wire
		(pts
			(xy 160.02 91.44) (xy 160.02 93.98)
		)
	)
	(wire
		(pts
			(xy 157.48 81.28) (xy 152.4 81.28)
		)
	)
	(wire
		(pts
			(xy 132.08 121.92) (xy 134.62 121.92)
		)
	)
	(wire
		(pts
			(xy 255.27 123.19) (xy 255.27 127)
		)
	)
	(wire
		(pts
			(xy 63.5 81.28) (xy 67.31 81.28)
		)
	)
	(wire
		(pts
			(xy 134.62 147.32) (xy 134.62 144.78)
		)
	)
	(wire
		(pts
			(xy 90.17 57.15) (xy 95.25 57.15)
		)
	)
	(wire
		(pts
			(xy 208.28 132.08) (xy 208.28 134.62)
		)
	)
	(wire
		(pts
			(xy 255.27 111.76) (xy 259.08 111.76)
		)
	)
	(wire
		(pts
			(xy 152.4 91.44) (xy 160.02 91.44)
		)
	)
	(wire
		(pts
			(xy 114.3 121.92) (xy 124.46 121.92)
		)
	)
	(wire
		(pts
			(xy 128.27 81.28) (xy 134.62 81.28)
		)
	)
	(wire
		(pts
			(xy 142.24 134.62) (xy 134.62 134.62)
		)
	)
	(wire
		(pts
			(xy 132.08 147.32) (xy 134.62 147.32)
		)
	)
	(wire
		(pts
			(xy 60.96 81.28) (xy 63.5 81.28)
		)
	)
	(wire
		(pts
			(xy 134.62 121.92) (xy 135.89 121.92)
		)
	)
	(wire
		(pts
			(xy 168.91 81.28) (xy 168.91 83.82)
		)
	)
	(wire
		(pts
			(xy 134.62 121.92) (xy 134.62 124.46)
		)
	)
	(wire
		(pts
			(xy 208.28 121.92) (xy 208.28 124.46)
		)
	)
	(wire
		(pts
			(xy 177.8 106.68) (xy 172.72 106.68)
		)
	)
	(wire
		(pts
			(xy 177.8 116.84) (xy 177.8 106.68)
		)
	)
	(wire
		(pts
			(xy 189.23 121.92) (xy 195.58 121.92)
		)
	)
	(wire
		(pts
			(xy 271.78 90.17) (xy 271.78 92.71)
		)
	)
	(wire
		(pts
			(xy 177.8 121.92) (xy 181.61 121.92)
		)
	)
	(wire
		(pts
			(xy 97.79 132.08) (xy 105.41 132.08)
		)
	)
	(wire
		(pts
			(xy 63.5 81.28) (xy 63.5 83.82)
		)
	)
	(wire
		(pts
			(xy 269.24 97.79) (xy 269.24 106.68)
		)
	)
	(wire
		(pts
			(xy 231.14 81.28) (xy 168.91 81.28)
		)
	)
	(wire
		(pts
			(xy 269.24 95.25) (xy 271.78 95.25)
		)
	)
	(wire
		(pts
			(xy 269.24 106.68) (xy 255.27 106.68)
		)
	)
	(wire
		(pts
			(xy 121.92 88.9) (xy 121.92 86.36)
		)
	)
	(wire
		(pts
			(xy 128.27 71.12) (xy 128.27 57.15)
		)
	)
	(wire
		(pts
			(xy 106.68 57.15) (xy 106.68 58.42)
		)
	)
	(wire
		(pts
			(xy 97.79 121.92) (xy 97.79 124.46)
		)
	)
	(wire
		(pts
			(xy 74.93 81.28) (xy 78.74 81.28)
		)
	)
	(wire
		(pts
			(xy 121.92 86.36) (xy 120.65 86.36)
		)
	)
	(hierarchical_label "9V"
		(shape input)
		(at 132.08 147.32 180)
	)
	(hierarchical_label "mix_RF"
		(shape input)
		(at 271.78 95.25 0)
	)
	(hierarchical_label "9V"
		(shape input)
		(at 90.17 57.15 180)
	)
	(hierarchical_label "soc_TX"
		(shape input)
		(at 34.29 81.28 180)
	)
	(hierarchical_label "3V3"
		(shape input)
		(at 271.78 90.17 0)
	)
	(hierarchical_label "sw_ctrl"
		(shape input)
		(at 273.05 111.76 0)
	)
	(hierarchical_label "soc_RX"
		(shape input)
		(at 54.61 121.92 180)
	)
	(symbol
		(lib_id "power:GND")
		(at 106.68 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR033"
			(at 106.68 74.93 0)
		)
		(property "Value" "GND"
			(at 106.68 72.644 0)
		)
		(property "Footprint" ""
			(at 106.68 68.58 0)
		)
		(property "Datasheet" ""
			(at 106.68 68.58 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 106.68 68.58 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR033")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 50.8 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR029"
			(at 50.8 100.33 0)
		)
		(property "Value" "GND"
			(at 50.8 98.044 0)
		)
		(property "Footprint" ""
			(at 50.8 93.98 0)
		)
		(property "Datasheet" ""
			(at 50.8 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 50.8 93.98 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR029")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 106.68 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L9"
			(at 106.68 116.84 90)
		)
		(property "Value" "8.2n"
			(at 106.68 119.38 90)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 106.68 121.92 0)
		)
		(property "Datasheet" "~"
			(at 106.68 121.92 0)
		)
		(property "Description" "Inductor"
			(at 106.68 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 255.27 119.38 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C38"
			(at 259.08 118.1099 0)
		)
		(property "Value" "100p"
			(at 259.08 120.6499 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 254.3048 115.57 0)
		)
		(property "Datasheet" "~"
			(at 255.27 119.38 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 255.27 119.38 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C38")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 255.27 127 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR056"
			(at 255.27 133.35 0)
		)
		(property "Value" "GND"
			(at 255.27 131.064 0)
		)
		(property "Footprint" ""
			(at 255.27 127 0)
		)
		(property "Datasheet" ""
			(at 255.27 127 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 255.27 127 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR056")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 105.41 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR035"
			(at 105.41 140.97 0)
		)
		(property "Value" "GND"
			(at 105.41 138.684 0)
		)
		(property "Footprint" ""
			(at 105.41 134.62 0)
		)
		(property "Datasheet" ""
			(at 105.41 134.62 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 105.41 134.62 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR035")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 63.5 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR030"
			(at 63.5 100.33 0)
		)
		(property "Value" "GND"
			(at 63.5 98.044 0)
		)
		(property "Footprint" ""
			(at 63.5 93.98 0)
		)
		(property "Datasheet" ""
			(at 63.5 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 63.5 93.98 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR030")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 172.72 106.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR037"
			(at 172.72 113.03 0)
		)
		(property "Value" "GND"
			(at 172.72 110.744 0)
		)
		(property "Footprint" ""
			(at 172.72 106.68 0)
		)
		(property "Datasheet" ""
			(at 172.72 106.68 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 172.72 106.68 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR037")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "ERA-1SM+:ERA-1SM+")
		(at 161.29 118.11 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC8"
			(at 156.845 109.22 90)
		)
		(property "Value" "ERA-1SM+"
			(at 156.845 111.76 90)
		)
		(property "Footprint" "ERA1SM"
			(at 228.27 91.44 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
			(at 328.27 91.44 0)
		)
		(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
			(at 161.29 118.11 0)
		)
		(property "Height" "1.52"
			(at 528.27 91.44 0)
		)
		(property "Mouser Part Number" "139-ERA-1SM"
			(at 628.27 91.44 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
			(at 728.27 91.44 0)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at 828.27 91.44 0)
		)
		(property "Manufacturer_Part_Number" "ERA-1SM+"
			(at 928.27 91.44 0)
		)
		(pin "4")
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 208.28 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R19"
			(at 210.82 126.9999 0)
		)
		(property "Value" "300"
			(at 210.82 129.5399 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 206.502 128.27 90)
		)
		(property "Datasheet" "~"
			(at 208.28 128.27 0)
		)
		(property "Description" "Resistor"
			(at 208.28 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 146.05 134.62 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C30"
			(at 146.05 127 90)
		)
		(property "Value" "10n"
			(at 146.05 129.54 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 142.24 135.5852 0)
		)
		(property "Datasheet" "~"
			(at 146.05 134.62 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 146.05 134.62 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C30")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 41.91 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C20"
			(at 41.91 73.66 90)
		)
		(property "Value" "10n"
			(at 41.91 76.2 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 45.72 80.3148 0)
		)
		(property "Datasheet" "~"
			(at 41.91 81.28 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 41.91 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 134.62 140.97 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R16"
			(at 137.16 139.6999 0)
		)
		(property "Value" "R"
			(at 137.16 142.2399 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 136.398 140.97 90)
		)
		(property "Datasheet" "~"
			(at 134.62 140.97 0)
		)
		(property "Description" "Resistor"
			(at 134.62 140.97 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 71.12 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C21"
			(at 71.12 73.66 90)
		)
		(property "Value" "10n"
			(at 71.12 76.2 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 74.93 80.3148 0)
		)
		(property "Datasheet" "~"
			(at 71.12 81.28 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 71.12 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 139.7 106.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR036"
			(at 139.7 113.03 0)
		)
		(property "Value" "GND"
			(at 139.7 110.744 0)
		)
		(property "Footprint" ""
			(at 139.7 106.68 0)
		)
		(property "Datasheet" ""
			(at 139.7 106.68 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 139.7 106.68 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR036")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 195.58 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R17"
			(at 198.12 126.9999 0)
		)
		(property "Value" "300"
			(at 198.12 129.5399 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 193.802 128.27 90)
		)
		(property "Datasheet" "~"
			(at 195.58 128.27 0)
		)
		(property "Description" "Resistor"
			(at 195.58 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 152.4 87.63 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C24"
			(at 156.21 86.3599 0)
		)
		(property "Value" "3p"
			(at 156.21 88.8999 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 151.4348 83.82 0)
		)
		(property "Datasheet" "~"
			(at 152.4 87.63 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 152.4 87.63 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 128.27 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C28"
			(at 128.27 114.3 90)
		)
		(property "Value" "10n"
			(at 128.27 116.84 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 132.08 120.9548 0)
		)
		(property "Datasheet" "~"
			(at 128.27 121.92 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 128.27 121.92 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C28")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 201.93 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R18"
			(at 201.93 115.57 90)
		)
		(property "Value" "18"
			(at 201.93 118.11 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 201.93 123.698 90)
		)
		(property "Datasheet" "~"
			(at 201.93 121.92 0)
		)
		(property "Description" "Resistor"
			(at 201.93 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 168.91 87.63 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C25"
			(at 172.72 86.3599 0)
		)
		(property "Value" "3p"
			(at 172.72 88.8999 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 167.9448 83.82 0)
		)
		(property "Datasheet" "~"
			(at 168.91 87.63 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 168.91 87.63 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C25")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 50.8 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "R12"
			(at 53.34 86.3599 0)
		)
		(property "Value" "R"
			(at 53.34 88.8999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 49.022 87.63 90)
		)
		(property "Datasheet" "~"
			(at 50.8 87.63 0)
		)
		(property "Description" "Resistor"
			(at 50.8 87.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 138.43 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C23"
			(at 138.43 73.66 90)
		)
		(property "Value" "10n"
			(at 138.43 76.2 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 142.24 80.3148 0)
		)
		(property "Datasheet" "~"
			(at 138.43 81.28 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 138.43 81.28 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C23")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 114.3 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C27"
			(at 118.11 126.9999 0)
		)
		(property "Value" "3p"
			(at 118.11 129.5399 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 113.3348 124.46 0)
		)
		(property "Datasheet" "~"
			(at 114.3 128.27 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 114.3 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C27")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 262.89 111.76 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R34"
			(at 262.89 105.41 90)
		)
		(property "Value" "100"
			(at 262.89 107.95 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 262.89 113.538 90)
		)
		(property "Datasheet" "~"
			(at 262.89 111.76 0)
		)
		(property "Description" "Resistor"
			(at 262.89 111.76 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R34")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4259-63:4259-63")
		(at 231.14 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC11"
			(at 250.19 85.09 0)
		)
		(property "Value" "4259-63"
			(at 250.19 87.63 0)
		)
		(property "Footprint" "SOT65P210X110-6N"
			(at 265.43 187.63 0)
		)
		(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe4259ds.pdf"
			(at 265.43 287.63 0)
		)
		(property "Description" "RF switch IC"
			(at 231.14 92.71 0)
		)
		(property "Height" "1.1"
			(at 265.43 487.63 0)
		)
		(property "Mouser Part Number" "81-4259-63"
			(at 265.43 587.63 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/pSemi/4259-63?qs=iw0hurA%2FaD37qvQcKdATTw%3D%3D"
			(at 265.43 687.63 0)
		)
		(property "Manufacturer_Name" "Peregrine Semiconductor"
			(at 265.43 787.63 0)
		)
		(property "Manufacturer_Part_Number" "4259-63"
			(at 265.43 887.63 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 106.68 62.23 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C22"
			(at 110.49 60.9599 0)
		)
		(property "Value" "10n"
			(at 110.49 63.4999 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 105.7148 58.42 0)
		)
		(property "Datasheet" "~"
			(at 106.68 62.23 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 106.68 62.23 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 195.58 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR039"
			(at 195.58 140.97 0)
		)
		(property "Value" "GND"
			(at 195.58 138.684 0)
		)
		(property "Footprint" ""
			(at 195.58 134.62 0)
		)
		(property "Datasheet" ""
			(at 195.58 134.62 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 195.58 134.62 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR039")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 121.92 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR032"
			(at 121.92 95.25 0)
		)
		(property "Value" "GND"
			(at 121.92 92.964 0)
		)
		(property "Footprint" ""
			(at 121.92 88.9 0)
		)
		(property "Datasheet" ""
			(at 121.92 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 121.92 88.9 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR032")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 154.94 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR038"
			(at 154.94 140.97 0)
		)
		(property "Value" "GND"
			(at 154.94 138.684 0)
		)
		(property "Footprint" ""
			(at 154.94 134.62 0)
		)
		(property "Datasheet" ""
			(at 154.94 134.62 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 154.94 134.62 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR038")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 160.02 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR034"
			(at 160.02 100.33 0)
		)
		(property "Value" "GND"
			(at 160.02 98.044 0)
		)
		(property "Footprint" ""
			(at 160.02 93.98 0)
		)
		(property "Datasheet" ""
			(at 160.02 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 160.02 93.98 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR034")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 78.74 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR031"
			(at 78.74 95.25 0)
		)
		(property "Value" "GND"
			(at 78.74 92.964 0)
		)
		(property "Footprint" ""
			(at 78.74 88.9 0)
		)
		(property "Datasheet" ""
			(at 78.74 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 78.74 88.9 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR031")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 99.06 57.15 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R15"
			(at 99.06 50.8 90)
		)
		(property "Value" "137"
			(at 99.06 53.34 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 99.06 58.928 90)
		)
		(property "Datasheet" "~"
			(at 99.06 57.15 0)
		)
		(property "Description" "Resistor"
			(at 99.06 57.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "ERA-1SM+:ERA-1SM+")
		(at 95.25 85.09 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC7"
			(at 99.695 73.66 90)
		)
		(property "Value" "ERA-1SM+"
			(at 99.695 76.2 90)
		)
		(property "Footprint" "ERA1SM"
			(at 28.27 111.76 0)
		)
		(property "Datasheet" "https://www.minicircuits.com/WebStore/dashboard.html?model=ERA-1SM%2B&srsltid=AfmBOopMJ6LGZDp162-GJ4DyJ5EbXofCns5kIKCboT9UIHU_AO_H4lBL"
			(at -71.73 111.76 0)
		)
		(property "Description" "RF Amplifier SMT Gain Block, DC - 8000 MHz, 50 ohms"
			(at 95.25 85.09 0)
		)
		(property "Height" "1.52"
			(at -271.73 111.76 0)
		)
		(property "Mouser Part Number" "139-ERA-1SM"
			(at -371.73 111.76 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/ERA-1SM%2b?qs=xZ%2FP%252Ba9zWqbAX5z6Z5ocXQ%3D%3D"
			(at -471.73 111.76 0)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at -571.73 111.76 0)
		)
		(property "Manufacturer_Part_Number" "ERA-1SM+"
			(at -671.73 111.76 0)
		)
		(pin "4")
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "IC7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 214.63 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR024"
			(at 214.63 101.6 0)
		)
		(property "Value" "GND"
			(at 214.63 99.568 0)
		)
		(property "Footprint" ""
			(at 214.63 95.25 0)
		)
		(property "Datasheet" ""
			(at 214.63 95.25 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 214.63 95.25 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR024")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 57.15 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R14"
			(at 57.15 74.93 90)
		)
		(property "Value" "0"
			(at 57.15 77.47 90)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 57.15 83.058 90)
		)
		(property "Datasheet" "~"
			(at 57.15 81.28 0)
		)
		(property "Description" "Resistor"
			(at 57.15 81.28 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 128.27 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L7"
			(at 129.54 73.6599 0)
		)
		(property "Value" "470n"
			(at 129.54 76.1999 0)
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder"
			(at 128.27 74.93 0)
		)
		(property "Datasheet" "~"
			(at 128.27 74.93 0)
		)
		(property "Description" "Inductor"
			(at 128.27 74.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 134.62 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L10"
			(at 135.89 126.9999 0)
		)
		(property "Value" "470n"
			(at 135.89 129.5399 0)
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder"
			(at 134.62 128.27 0)
		)
		(property "Datasheet" "~"
			(at 134.62 128.27 0)
		)
		(property "Description" "Inductor"
			(at 134.62 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L")
		(at 161.29 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L8"
			(at 161.29 76.2 90)
		)
		(property "Value" "8.2n"
			(at 161.29 78.74 90)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 161.29 81.28 0)
		)
		(property "Datasheet" "~"
			(at 161.29 81.28 0)
		)
		(property "Description" "Inductor"
			(at 161.29 81.28 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "L8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 97.79 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C26"
			(at 101.6 126.9999 0)
		)
		(property "Value" "3p"
			(at 101.6 129.5399 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 96.8248 124.46 0)
		)
		(property "Datasheet" "~"
			(at 97.79 128.27 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 97.79 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C26")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 208.28 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR040"
			(at 208.28 140.97 0)
		)
		(property "Value" "GND"
			(at 208.28 138.684 0)
		)
		(property "Footprint" ""
			(at 208.28 134.62 0)
		)
		(property "Datasheet" ""
			(at 208.28 134.62 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 208.28 134.62 0)
		)
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "#PWR040")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 63.5 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "R13"
			(at 66.04 86.3599 0)
		)
		(property "Value" "R"
			(at 66.04 88.8999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 61.722 87.63 90)
		)
		(property "Datasheet" "~"
			(at 63.5 87.63 0)
		)
		(property "Description" "Resistor"
			(at 63.5 87.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "R13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 185.42 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C29"
			(at 185.42 114.3 90)
		)
		(property "Value" "10n"
			(at 185.42 116.84 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 189.23 120.9548 0)
		)
		(property "Datasheet" "~"
			(at 185.42 121.92 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 185.42 121.92 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "halow-53mhz-converter-1"
				(path
					(reference "C29")
					(unit 1)
				)
			)
		)
	)
)
