(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Oscillator:FT5HV"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Y"
				(at 5.08 11.43 0)
			)
			(property "Value" "FT5HV"
				(at 6.35 8.89 0)
			)
			(property "Footprint" "Oscillator:Oscillator_SMD_Fox_FT5H_5.0x3.2mm"
				(at 0 -19.05 0)
			)
			(property "Datasheet" "https://foxonline.com/wp-content/uploads/pdfs/T5HN_T5HV.pdf"
				(at 0 0 0)
			)
			(property "Description" "HCMOS temperature compensated voltage controlled oscillator"
				(at 0 0 0)
			)
			(property "ki_keywords" "TXCO VCTCXO"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Oscillator*SMD*Fox*FT5H*5.0x3.2mm*"
				(at 0 0 0)
			)
			(symbol "FT5HV_0_1"
				(rectangle
					(start -5.08 5.08)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -4.445 2.54) (xy -3.81 2.54) (xy -3.81 3.81) (xy -3.175 3.81) (xy -3.175 2.54) (xy -2.54 2.54)
						(xy -2.54 3.81) (xy -1.905 3.81) (xy -1.905 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "FT5HV_1_1"
				(pin input line
					(at -7.62 0 0)
					(length 2.54)
					(name "VC")
					(number "1")
				)
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "OUT")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulator_Linear:LT1762"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 8.89 0)
			)
			(property "Value" "LT1762"
				(at 1.27 -6.35 0)
			)
			(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
				(at 0 -8.89 0)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
				(at 0 -13.97 0)
			)
			(property "Description" "150mA, Adjustable, Low Noise, Micropower LDO Regulator, MSOP-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "LDO ADJ"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
				(at 0 0 0)
			)
			(symbol "LT1762_0_1"
				(rectangle
					(start -7.62 7.62)
					(end 7.62 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "LT1762_1_1"
				(pin power_in line
					(at -10.16 5.08 0)
					(length 2.54)
					(name "IN")
					(number "8")
				)
				(pin input line
					(at -10.16 -2.54 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "5")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 5.08 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 2.54 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_out line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin input line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "ADJ")
					(number "2")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "BYP")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+3.3V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "vctcxo adjust"
		(exclude_from_sim no)
		(at 58.42 105.156 0)
	)
	(text "byp. cap for low noise"
		(exclude_from_sim no)
		(at 102.616 39.624 0)
	)
	(junction
		(at 111.76 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 66.04 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 77.47 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 92.71 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 100.33 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 80.01 45.72) (xy 71.12 45.72)
		)
	)
	(wire
		(pts
			(xy 105.41 81.28) (xy 105.41 63.5)
		)
	)
	(wire
		(pts
			(xy 41.91 43.18) (xy 48.26 43.18)
		)
	)
	(wire
		(pts
			(xy 71.12 71.12) (xy 71.12 50.8)
		)
	)
	(wire
		(pts
			(xy 80.01 50.8) (xy 80.01 45.72)
		)
	)
	(wire
		(pts
			(xy 92.71 90.17) (xy 105.41 90.17)
		)
	)
	(wire
		(pts
			(xy 48.26 50.8) (xy 48.26 43.18)
		)
	)
	(wire
		(pts
			(xy 111.76 50.8) (xy 111.76 53.34)
		)
	)
	(wire
		(pts
			(xy 92.71 80.01) (xy 92.71 81.28)
		)
	)
	(wire
		(pts
			(xy 71.12 43.18) (xy 85.09 43.18)
		)
	)
	(wire
		(pts
			(xy 85.09 50.8) (xy 85.09 53.34)
		)
	)
	(wire
		(pts
			(xy 72.39 114.3) (xy 77.47 114.3)
		)
	)
	(wire
		(pts
			(xy 135.89 63.5) (xy 135.89 43.18)
		)
	)
	(wire
		(pts
			(xy 72.39 96.52) (xy 77.47 96.52)
		)
	)
	(wire
		(pts
			(xy 50.8 50.8) (xy 48.26 50.8)
		)
	)
	(wire
		(pts
			(xy 77.47 104.14) (xy 85.09 104.14)
		)
	)
	(wire
		(pts
			(xy 48.26 43.18) (xy 50.8 43.18)
		)
	)
	(wire
		(pts
			(xy 72.39 90.17) (xy 72.39 96.52)
		)
	)
	(wire
		(pts
			(xy 111.76 50.8) (xy 125.73 50.8)
		)
	)
	(wire
		(pts
			(xy 66.04 114.3) (xy 72.39 114.3)
		)
	)
	(wire
		(pts
			(xy 85.09 60.96) (xy 85.09 63.5)
		)
	)
	(wire
		(pts
			(xy 100.33 104.14) (xy 104.14 104.14)
		)
	)
	(wire
		(pts
			(xy 60.96 55.88) (xy 60.96 58.42)
		)
	)
	(wire
		(pts
			(xy 77.47 104.14) (xy 77.47 106.68)
		)
	)
	(wire
		(pts
			(xy 72.39 114.3) (xy 72.39 115.57)
		)
	)
	(wire
		(pts
			(xy 66.04 96.52) (xy 72.39 96.52)
		)
	)
	(wire
		(pts
			(xy 111.76 43.18) (xy 125.73 43.18)
		)
	)
	(wire
		(pts
			(xy 92.71 88.9) (xy 92.71 90.17)
		)
	)
	(wire
		(pts
			(xy 92.71 90.17) (xy 92.71 96.52)
		)
	)
	(wire
		(pts
			(xy 100.33 50.8) (xy 100.33 71.12)
		)
	)
	(wire
		(pts
			(xy 66.04 104.14) (xy 66.04 106.68)
		)
	)
	(wire
		(pts
			(xy 85.09 43.18) (xy 100.33 43.18)
		)
	)
	(wire
		(pts
			(xy 92.71 111.76) (xy 92.71 114.3)
		)
	)
	(wire
		(pts
			(xy 135.89 43.18) (xy 125.73 43.18)
		)
	)
	(wire
		(pts
			(xy 85.09 50.8) (xy 80.01 50.8)
		)
	)
	(wire
		(pts
			(xy 105.41 90.17) (xy 105.41 88.9)
		)
	)
	(wire
		(pts
			(xy 111.76 43.18) (xy 100.33 43.18)
		)
	)
	(wire
		(pts
			(xy 100.33 71.12) (xy 71.12 71.12)
		)
	)
	(wire
		(pts
			(xy 66.04 104.14) (xy 77.47 104.14)
		)
	)
	(wire
		(pts
			(xy 105.41 63.5) (xy 135.89 63.5)
		)
	)
	(wire
		(pts
			(xy 92.71 90.17) (xy 72.39 90.17)
		)
	)
	(wire
		(pts
			(xy 41.91 36.83) (xy 41.91 43.18)
		)
	)
	(hierarchical_label "FREQ_REF"
		(shape input)
		(at 104.14 104.14 0)
	)
	(symbol
		(lib_id "power:GND")
		(at 60.96 58.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR012"
			(at 60.96 64.77 0)
		)
		(property "Value" "GND"
			(at 60.96 62.738 0)
		)
		(property "Footprint" ""
			(at 60.96 58.42 0)
		)
		(property "Datasheet" ""
			(at 60.96 58.42 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 60.96 58.42 0)
		)
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 72.39 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR013"
			(at 72.39 121.92 0)
		)
		(property "Value" "GND"
			(at 72.39 119.888 0)
		)
		(property "Footprint" ""
			(at 72.39 115.57 0)
		)
		(property "Datasheet" ""
			(at 72.39 115.57 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 72.39 115.57 0)
		)
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 105.41 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 107.95 83.8199 0)
		)
		(property "Value" "0"
			(at 107.95 86.3599 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 103.632 85.09 90)
		)
		(property "Datasheet" "~"
			(at 105.41 85.09 0)
		)
		(property "Description" "Resistor"
			(at 105.41 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Oscillator:FT5HV")
		(at 92.71 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Y1"
			(at 101.6 97.7198 0)
		)
		(property "Value" "FT5HV"
			(at 101.6 100.2598 0)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Fox_FT5H_5.0x3.2mm"
			(at 92.71 123.19 0)
		)
		(property "Datasheet" "https://foxonline.com/wp-content/uploads/pdfs/T5HN_T5HV.pdf"
			(at 92.71 104.14 0)
		)
		(property "Description" "HCMOS temperature compensated voltage controlled oscillator"
			(at 92.71 104.14 0)
		)
		(pin "3")
		(pin "4")
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "Y1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 111.76 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR016"
			(at 111.76 59.69 0)
		)
		(property "Value" "GND"
			(at 111.76 57.658 0)
		)
		(property "Footprint" ""
			(at 111.76 53.34 0)
		)
		(property "Datasheet" ""
			(at 111.76 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 111.76 53.34 0)
		)
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 85.09 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 87.63 55.8799 0)
		)
		(property "Value" "10k"
			(at 87.63 58.4199 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 83.312 57.15 90)
		)
		(property "Datasheet" "~"
			(at 85.09 57.15 0)
		)
		(property "Description" "Resistor"
			(at 85.09 57.15 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 85.09 46.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 87.63 45.7199 0)
		)
		(property "Value" "10k"
			(at 87.63 48.2599 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 83.312 46.99 90)
		)
		(property "Datasheet" "~"
			(at 85.09 46.99 0)
		)
		(property "Description" "Resistor"
			(at 85.09 46.99 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 92.71 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 95.25 83.8199 0)
		)
		(property "Value" "R"
			(at 95.25 86.3599 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 90.932 85.09 90)
		)
		(property "Datasheet" "~"
			(at 92.71 85.09 0)
		)
		(property "Description" "Resistor"
			(at 92.71 85.09 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 125.73 46.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C11"
			(at 129.54 45.7199 0)
		)
		(property "Value" "22u"
			(at 129.54 48.2599 0)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 126.6952 50.8 0)
		)
		(property "Datasheet" "~"
			(at 125.73 46.99 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 125.73 46.99 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "C11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 111.76 46.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C9"
			(at 115.57 45.7199 0)
		)
		(property "Value" "10n"
			(at 115.57 48.2599 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 112.7252 50.8 0)
		)
		(property "Datasheet" "~"
			(at 111.76 46.99 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 111.76 46.99 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR014"
			(at 85.09 69.85 0)
		)
		(property "Value" "GND"
			(at 85.09 67.818 0)
		)
		(property "Footprint" ""
			(at 85.09 63.5 0)
		)
		(property "Datasheet" ""
			(at 85.09 63.5 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 85.09 63.5 0)
		)
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 66.04 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 68.58 109.2199 0)
		)
		(property "Value" "R"
			(at 68.58 111.7599 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 64.262 110.49 90)
		)
		(property "Datasheet" "~"
			(at 66.04 110.49 0)
		)
		(property "Description" "Resistor"
			(at 66.04 110.49 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 92.71 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR010"
			(at 92.71 120.65 0)
		)
		(property "Value" "GND"
			(at 92.71 118.618 0)
		)
		(property "Footprint" ""
			(at 92.71 114.3 0)
		)
		(property "Datasheet" ""
			(at 92.71 114.3 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 92.71 114.3 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 77.47 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 80.01 109.2199 0)
		)
		(property "Value" "10k"
			(at 80.01 111.7599 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 75.692 110.49 90)
		)
		(property "Datasheet" "~"
			(at 77.47 110.49 0)
		)
		(property "Description" "Resistor"
			(at 77.47 110.49 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulator_Linear:LT1762")
		(at 60.96 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 60.96 35.56 0)
		)
		(property "Value" "LT1762"
			(at 60.96 38.1 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 60.96 57.15 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1762.pdf"
			(at 60.96 62.23 0)
		)
		(property "Description" "150mA, Adjustable, Low Noise, Micropower LDO Regulator, MSOP-8"
			(at 60.96 48.26 0)
		)
		(pin "6")
		(pin "5")
		(pin "7")
		(pin "1")
		(pin "2")
		(pin "4")
		(pin "8")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 41.91 36.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 41.91 40.64 0)
		)
		(property "Value" "+5V"
			(at 41.91 31.75 0)
		)
		(property "Footprint" ""
			(at 41.91 36.83 0)
		)
		(property "Datasheet" ""
			(at 41.91 36.83 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 41.91 36.83 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 100.33 46.99 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C10"
			(at 104.14 45.7199 0)
		)
		(property "Value" "10n"
			(at 104.14 48.2599 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 99.3648 43.18 0)
		)
		(property "Datasheet" "~"
			(at 100.33 46.99 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 100.33 46.99 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "C10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 66.04 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 68.58 99.0599 0)
		)
		(property "Value" "R"
			(at 68.58 101.5999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 64.262 100.33 90)
		)
		(property "Datasheet" "~"
			(at 66.04 100.33 0)
		)
		(property "Description" "Resistor"
			(at 66.04 100.33 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "lskonv1"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3.3V")
		(at 92.71 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 92.71 83.82 0)
		)
		(property "Value" "+3.3V"
			(at 92.71 74.93 0)
		)
		(property "Footprint" ""
			(at 92.71 80.01 0)
		)
		(property "Datasheet" ""
			(at 92.71 80.01 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 92.71 80.01 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 77.47 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 80.01 99.0599 0)
		)
		(property "Value" "10k"
			(at 80.01 101.5999 0)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 75.692 100.33 90)
		)
		(property "Datasheet" "~"
			(at 77.47 100.33 0)
		)
		(property "Description" "Resistor"
			(at 77.47 100.33 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
)
